SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cd_Ampz146_003
        Comment ( "Sekce vozidlo" )
        Comment ( "Popis fyziky vozu pro OR" )
        Comment ( "Pokyny pro obecne nastaveni OR:" )
        Comment ( "Karta Obecne: Rychlost plneni brzdoveho potrubi 1000 PSI/s (nutne aby OR akceptoval hodnoty engu!)" )
        Comment ( "Karta Simulace: Pokrocily model adheze" )
        Comment ( "Karta Experimentalni: Faktor korekce adheze 100%" )
        Comment ( "Karta Experimentalni: Nahodna zmena faktoru adheze 10%" ) 
        Comment ( "ladeni dle navodu od Josefa Vogeltanze" )
        Comment ( "Obsazenost 2/3" )

	Type ( Carriage )
	Name ("CD vuz Ampz146 003")
	WagonShape ( cd_Ampz146_003.s )
        Freightanim ( prouzek.s 1 1 )
	Size ( 2.89m 4.12m 26.29m )
	CentreOfGravity ( 0m 1.9m 0m )
	Mass ( 51t )
	WheelRadius ( 0.46m )
	InertiaTensor ( Box (2.89m 4.12m 26.29m) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)

Comment ( "Jizdni odpory a treni" )
CentreOfGravity ( 0m 2.03m  0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 2m 500mm )
ORTSUnbalancedSuperelevation ( 150mm )

DerailRailHeight ( 4cm )
DerailRailForce ( 123.5kN )
DerailBufferForce ( 484kN )
ORTSBearingType ( Roller )
ORTSDavis_A ( 853.7 )
ORTSDavis_B ( 17.43 )
ORTSDavis_C ( 0.9041 )

	
	Lights ( 10
		Light	(
			comment( hrac normal predni pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.24 2.12 13.08 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac normal predni levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.24 2.12 13.08 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac normal zadní pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac normal zadní levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac otocene predni pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 4 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.24 2.12 13.08 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac otocene predni levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 4 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.24 2.12 13.08 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac otocene zadní pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac otocene zadní levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( trf normal zadní pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( trf normal zadní levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	) 

Comment ( "Brzdy" )
Comment ( "Brzdovy system Knorr, kotouce, Bv.: 54t" )
Comment ( "Rezim brzdeni P" )
BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

MaxBrakeForce ( 160kN )
MaxHandbrakeForce ( 43kN )
NumberOfHandbrakeLeverSteps ( 10 )

TripleValveRatio ( 2.5 )
MaxReleaseRate ( 0.2bar/s )
MaxApplicationRate ( 0.45bar/s )
MaxAuxilaryChargingRate ( 0.76bar/s )
EmergencyResChargingRate ( 0.76bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 3.8bar )
EmergencyResVolumeMultiplier ( 1.0 )
EmergencyResCapacity ( 160l )
BrakePipeVolume ( 22.1l )

ORTSBrakeShoeFriction ( 0 0.42 1 0.40 2 0.39 3 0.38 4 0.37 5 0.37 7 0.36 8 0.35 9 0.34 12 0.33 14 0.32 16 0.31 20 0.30 24 0.30 30 0.29 34 0.28 40 0.27 48 0.26 56 0.26 68 0.25 84 0.24 120 0.23 160 0.23 )

  	Sound ( "..//..//common.snd//sndVozy//CDvuzOsVetr4nEx-OR.sms" )
)
