SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cd_163078_hk_v2021
Comment (** Verzia pre OpenRails CZ/SK verziu bez ARR + MSTS Vigilance Monitor, 11.7.2021 **)	
	Type ( Engine )
	WagonShape ( "cd_163078_hk_v2021.s" )
	Freightanim ( cd_163078fg_hk_v2021.s 1 1 ) 
	Size ( 2.97m 4.597m 16.856m )
	CentreOfGravity ( 0m 2.25m 0m )
	Mass ( 84.0t )

Comment (** Spriahla nastavene na 1.5cm **)
	Coupling (
		Type ( Chain )
		Spring ( Stiffness (  6.7e6N/m 4.4e8N/m) Break ( 1.1e8N 5e8N ) r0 ( 0cm 1.5cm ) )
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s ) )

	Coupling (
		Type ( Chain )
		Spring ( Stiffness (  6.7e6N/m 4.4e8N/m) Break ( 1.1e8N 5e8N ) r0 ( 0cm 1.5cm ) )
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s ) )

comment (** adheze **)
	ORTSAdhesion (
        ORTSCurtius_Kniffler ( 7.5 55 0.166 0.7 )
        ORTSSlipWarningThreshold ( 80 )
        )
	comment (** pocet naprav - vypocet adheze pro brzdeni **)
	ORTSNumberAxles ( 4 )
        WheelRadius ( 0.608m )

comment (** Merny odpor dle rovnice, uvedene v puvodnim trakcnim grafu **)
comment (** oj = 5.075 + 0.0133*v + 0.000518*v2 **)
AxleMassRange_1 ( 0t 25t )
DavisCoefficientA_1 ( 5.0756 )
DavisCoefficientB_1 ( 0.0133 )
DavisCoefficientC_1 ( 0.000518 )
comment (** odtrhovy odpor **)
ORTSMergeSpeed ( 0.31 )

comment (** odpor v oblouku **)

	ORTSTrackGauge ( 1435mm )
	comment (** rozvor podvozku **)
	ORTSRigidWheelbase ( 2400mm )
	ORTSUnbalancedSuperelevation ( 152.4mm )
	
comment (** celni plocha pro vypocet vlivu vetru na jizdni odpor **)
        ORTSWagonFrontalArea ( 10.5m^2 )
	
	MaxBrakeForce( 88.42kN )
	MaxHandbrakeForce( 6kN )
	NumberOfHandbrakeLeverSteps( 10 )

        comment (** brzda DAKO-GP, rozvadec DAKO LTR **)
        comment (** brzdove valce 8x 8", zdvih 125mm = zdvihovy objem valce 4.054l. Objem valcu: 8*4.054=32.429l **)
        comment (** pomocna jimka 150l **)
        comment (** vypocet nasobitelu pro objem pomocne jimky: objem valcu*TVR*multiplier = 32.429*4.26*1.086=150l **)

	BrakeEquipmentType( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
        TripleValveRatio( 4.26 )
comment (** rezim P = 0.285714bar/s - odbrzdeni 22.4s **)
comment (** rezim G = 0.128bar/s - odbrzdeni 50s **)
	MaxReleaseRateP ( 0.285714bar/s )
	MaxReleaseRateG ( 0.128bar/s )
comment (** rezim P = 1.207547bar/s - zabrzdeni 5.3s **)
comment (** rezim G = 0.290bar/s - zabrzdeni 22s **)
	MaxApplicationRateP ( 1.207547bar/s )
	MaxApplicationRateG ( 0.290bar/s )
	MaxAuxilaryChargingRate ( 0.1bar/s )
	EmergencyResChargingRate ( 0.1bar/s )
comment (** mez necitlivosti rozvadece **)
	BrakeSensitivity ( 0.0052bar/s )
	EmergencyResCapacity( 150l )
	EmergencyResVolumeMultiplier ( 1.086 )
	EmergencyBrakeResMaxPressure( 5bar )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 6.4bar )
comment (** unik vzduchu netesnosti brzdoveho potrubi **)
	TrainPipeLeakRate ( 0.00021bar/s )
comment (** objem brzdoveho potrubi **)
	BrakePipeVolume ( 16.0l )
comment (** zpozdeni naskoku brzdy **)
	BrakeDelayToEngage ( 1.5s )
comment (** Minimalni nutne snizeni tlaku potrubi pro naskok brzdy **)
        BrakePipeMinPressureDropToEngage ( 0.32bar )

comment (** Prime zadani brzdici vahy pro vyvojovou MG verzi, ktera pevne zadani MaxBrakeForce() nepouziva **)
	BrakeMassP ( 44t )
	BrakeMassG ( 24t )
	BrakeMassR ( 44t )
	BrakeMassRMg ( 44t )
comment (** korekce brzdici vahy - pro ucely doladeni hodnoty **)
	DebugKoef ( 0.75 )

comment (** ORTSBrakeShoeFricion (krivka soucinitele treni) - litinove brzdove zdrze - rezim P/G **)
comment (** autor krivky: Pajavlaky **)

	ORTSBrakeShoeFriction (
		       0.0	0.3100
		       1.0	0.2800
		       2.0	0.2670
		       3.0	0.2572
		       4.0	0.2490
		       5.0	0.2419
		       6.0	0.2355
		       7.0	0.2296
		       8.0	0.2242
		       9.0	0.2192
		       10.0	0.2145
		       11.0	0.2100
		       12.0	0.2059
		       13.0	0.2019
		       14.0	0.1981
		       15.0	0.1945
		       16.0	0.1911
		       17.0	0.1878
		       18.0	0.1847
		       19.0	0.1817
		       20.0	0.1788
		       21.0	0.1760
		       22.0	0.1733
		       23.0	0.1708
		       24.0	0.1683
		       25.0	0.1660
		       26.0	0.1637
		       27.0	0.1615
		       28.0	0.1594
		       29.0	0.1574
		       31.0	0.1536
		       32.0	0.1518
		       33.0	0.1501
		       34.0	0.1484
		       35.0	0.1468
		       37.0	0.1439
		       38.0	0.1425
		       40.0	0.1399
		       41.0	0.1387
		       51.0	0.1277
		       57.0	0.1217
		       63.0	0.1163
		       68.0	0.1123
		       74.0	0.1080
		       80.0	0.1044
		       87.0	0.1009
		       94.0	0.0982
		       105.0	0.0949
		       120.0	0.0919
		       140.0	0.0897
		       160.0	0.0897

                      )

Comment (** zdvih zberacov **)
	ORTSPantographs (
                Pantograph (   
                Delay ( 3s )
                     )
                Pantograph (   
                Delay ( 3s ) 
                )
                )

comment	( Lights )
	Lights ( 25
		Light (
			comment ( Svetelny kuzel dialkovy )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBFFFF )
					Position ( 0 2.59 7.89 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 60 )
				)
			)
		)		
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( reflektor lavy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( -0.1 2.59 7.89 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( 0.1 2.59 7.89 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.7 )
				)
			)
		)
                Light (
			comment ( predne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFBDEBE )
					Position ( -0.73 1.68 7.825 )
					Azimuth ( 0.0 0.0 0.0 )
                                        Elevation ( 11 11 11 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( predne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFBDEBE )
					Position ( 0.73 1.68 7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 -7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 -7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		
		comment ( Definicia svetiel pre zadne stanoviste )
                Light (
			comment ( reflektor lavy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( 0.1 2.59 -7.89 )
                                        Elevation ( -10 -10 -10 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( -0.1 2.59 -7.89 )
                                        Elevation ( -10 -10 -10 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.7 )
				)
			)
		)
                Light (
			comment ( predne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( 0.73 1.68 -7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( predne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( -0.73 1.68 -7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 7.825 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 11 11 11 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                comment ( Definicia svetiel pre posunujuci diel )
                Light (
			comment ( Predne lave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFBDEBE )
					Position ( -0.73 1.68 7.825 )
					Elevation ( 11 11 11 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( Predne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFBDEBE )
					Position ( 0.73 1.68 7.825 )
					Elevation ( 11 11 11 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                Light (
			comment ( zadne lave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFBDEBE )
					Position ( -0.73 1.68 -7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFBDEBE )
					Position ( 0.73 1.68 -7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		comment ( Definicia svetiel pre Loose consist )
                Light	(
			comment( Predne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFBDEBE )
					Position ( 0.73 1.68 7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light	(
			comment( Predne lave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFBDEBE )
					Position ( -0.73 1.68 7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light	(
			comment( zadne lave pozicne)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFBDEBE )
					Position ( -0.73 1.68 -7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light	(
			comment( zadne prave pozicne)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFBDEBE )
					Position ( 0.73 1.68 -7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		comment ( Definicia svetiel pre PC )

		Light (
			comment ( Predne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( 0.73 1.68 7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( Predne lave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( -0.73 1.68 7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                Light (
			comment ( zadne lave pozicne )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 -7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadne prave pozicne )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 -7.825 )
                                        Elevation ( 11 11 11 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
	)
Comment (** vonkajsi zvuk **)
	Sound ( "..\\..\\common.snd\\sndX6X\\163IIeng.sms" )
)

Engine ( cd_163078_hk_v2021
	Wagon ( "cd_163078_hk_v2021" )
	Type ( Electric )
	MaxPower ( 3480kW )
	MaxForce ( 285kN )
	MaxContinuousForce ( 177kN )
	ORTSContinuousForceTimeFactor ( 3600 )
	MaxCurrent ( 1140A )
	MaxVelocity ( 120km/h )
	WheelRadius ( 0.608m )
	ORTSNumberDriveAxles ( 4 )
        ORTSDriveWheelWeight ( 84t )
comment (** soucinitel vyuziti adheze **)
        AdhesionEfficiencyKoef ( 0.98 )
        
        Sanding ( 120km/h )
        MaxSandingTime( 800 )

Comment (** hlavny Vypinac ** )
        ORTSCircuitBreaker ( Manual )
        ORTSCircuitBreakerClosingDelay ( 0.5s )
        ORTSPowerOnDelay ( 0.5s )
        ORTSAuxPowerOnDelay ( 10s )
        MultiSystemEngine ( 0 )
        MaxCurrentPower ( 1000 )
        MaxCurrentBrake ( 650A )
        SlipSpeedCritical ( 40km/h )

	DoesBrakeCutPower( 1 )
	BrakeCutsPowerAtBrakeCylinderPressure ( 6.0bar )
	ORTSBrakeCutsPowerAtBrakePipePressure ( 3.6bar )
	ORTSBrakeRestoresPowerAtBrakePipePressure ( 4.7bar )
	DoesPowerLossResetControls ( 1 )

	MaxControllerVolts ( 10 )
	AcceleratingToBrakingChangeTime ( 3 )			Comment (** omeskanie vykonu pri pouziti brzdy **)
	DefaultForceStep ( 7 )
	DynamicBrakeMaxForceAtSelectorStep ( 7 )
	AntiWheelSpinEquipped ( True )
	AntiWheelSpinSpeedDiffThreshold ( 0.32 )

Comment (** vnutorny zvuk **)
	Sound ( "..\\..\\common.snd\\sndX6X\\163IIcabCD.sms" )
Comment (** Pohlad z kabiny **)
	CabView ( "..\\..\\common.cab\\cab163\\163_2s.cvf" )
	HeadOut ( 1.6 3.0 6.6 )

ORTSTractionCharacteristics (   121   13                                       
   throttle (      0   0.27   0.36   0.45   0.55   0.62   0.65   0.73   0.77   0.82   0.91   1.00   )
   table (                                          
      0km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      1km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      2km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      3km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      4km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      5km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      6km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      7km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      8km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      9km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      10km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      11km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      12km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      13km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      14km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      15km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      16km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      17km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      18km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      19km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      20km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      21km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      22km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      23km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.55kN   
      24km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.52kN   223.62kN   239.75kN   271.97kN   295.01kN   
      25km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   179.33kN   210.73kN   223.78kN   239.90kN   271.97kN   293.46kN   
      26km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   179.66kN   210.94kN   223.94kN   240.05kN   271.97kN   291.91kN   
      27km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.86kN   179.99kN   211.15kN   224.11kN   240.19kN   271.97kN   290.36kN   
      28km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.74kN   168.19kN   180.32kN   211.35kN   224.27kN   240.34kN   271.97kN   288.81kN   
      29km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.91kN   168.53kN   180.65kN   211.56kN   224.43kN   240.48kN   271.97kN   287.25kN   
      30km/h   0.00kN   52.88kN   80.65kN   111.82kN   144.08kN   168.86kN   180.97kN   211.76kN   224.59kN   240.62kN   271.97kN   285.70kN   
      31km/h   0.00kN   52.88kN   80.65kN   111.92kN   144.24kN   169.19kN   181.29kN   211.97kN   224.75kN   240.77kN   271.97kN   284.43kN   
      32km/h   0.00kN   52.88kN   80.65kN   112.03kN   144.41kN   169.51kN   181.61kN   212.17kN   224.91kN   240.91kN   271.97kN   282.83kN   
      33km/h   0.00kN   52.88kN   80.65kN   112.13kN   144.57kN   169.83kN   181.92kN   212.37kN   225.07kN   241.05kN   271.97kN   281.24kN   
      34km/h   0.00kN   52.88kN   80.78kN   112.23kN   144.74kN   170.15kN   182.23kN   212.57kN   225.23kN   241.19kN   271.97kN   279.64kN   
      35km/h   0.00kN   52.88kN   80.91kN   112.34kN   144.90kN   170.46kN   182.54kN   212.77kN   225.39kN   241.33kN   271.97kN   278.04kN   
      36km/h   0.00kN   52.88kN   81.04kN   112.44kN   145.06kN   170.78kN   182.84kN   212.97kN   225.54kN   241.47kN   271.97kN   276.45kN   
      37km/h   0.00kN   52.88kN   81.17kN   112.54kN   145.22kN   171.08kN   183.15kN   213.16kN   225.70kN   241.61kN   271.97kN   274.85kN   
      38km/h   0.00kN   53.05kN   81.30kN   112.65kN   145.38kN   171.39kN   183.45kN   213.36kN   225.86kN   241.75kN   271.97kN   273.25kN   
      39km/h   0.00kN   53.22kN   81.43kN   112.75kN   145.54kN   171.69kN   183.74kN   213.55kN   226.01kN   241.89kN   271.97kN   272.65kN   
      40km/h   0.00kN   53.38kN   81.56kN   112.85kN   145.69kN   171.99kN   184.04kN   213.75kN   226.17kN   242.03kN   271.25kN   270.92kN   
      41km/h   0.00kN   53.55kN   81.68kN   112.95kN   145.85kN   172.29kN   184.33kN   213.94kN   226.32kN   242.17kN   269.51kN   269.19kN   
      42km/h   0.00kN   53.71kN   81.81kN   113.05kN   146.01kN   172.59kN   184.62kN   214.13kN   226.47kN   242.31kN   267.77kN   267.47kN   
      43km/h   0.00kN   53.88kN   81.94kN   113.15kN   146.16kN   172.88kN   184.90kN   214.32kN   226.62kN   242.44kN   266.03kN   265.74kN   
      44km/h   0.00kN   54.04kN   82.06kN   113.25kN   146.32kN   173.17kN   185.19kN   214.51kN   226.78kN   242.58kN   264.29kN   264.02kN   
      45km/h   0.00kN   54.20kN   82.19kN   113.35kN   146.47kN   173.45kN   185.47kN   214.70kN   226.93kN   242.72kN   262.55kN   262.29kN   
      46km/h   0.00kN   54.36kN   82.31kN   113.45kN   146.62kN   173.74kN   185.75kN   214.88kN   227.08kN   242.85kN   260.82kN   260.57kN   
      47km/h   0.00kN   54.52kN   82.43kN   113.55kN   146.78kN   174.02kN   186.02kN   215.07kN   227.23kN   242.99kN   259.08kN   258.85kN   
      48km/h   0.00kN   54.67kN   82.56kN   113.65kN   146.93kN   174.30kN   186.30kN   215.25kN   227.38kN   243.12kN   257.35kN   257.13kN   
      49km/h   0.00kN   54.83kN   82.68kN   113.75kN   147.08kN   174.57kN   186.57kN   215.32kN   227.53kN   243.26kN   255.61kN   255.41kN   
      50km/h   0.00kN   54.98kN   82.80kN   113.85kN   147.23kN   174.85kN   186.84kN   215.32kN   227.67kN   243.39kN   253.88kN   253.69kN   
      51km/h   0.00kN   55.14kN   82.92kN   113.94kN   147.38kN   175.12kN   187.10kN   215.32kN   227.82kN   243.52kN   252.15kN   251.97kN   
      52km/h   0.00kN   55.29kN   83.04kN   114.04kN   147.52kN   175.39kN   187.37kN   215.32kN   227.97kN   243.66kN   250.42kN   250.25kN   
      53km/h   0.00kN   55.44kN   83.17kN   114.14kN   147.67kN   175.65kN   187.63kN   215.32kN   228.11kN   243.79kN   248.69kN   248.54kN   
      54km/h   0.00kN   55.59kN   83.28kN   114.24kN   147.82kN   175.92kN   187.89kN   215.32kN   228.26kN   243.92kN   246.96kN   246.82kN   
      55km/h   0.00kN   55.74kN   83.40kN   114.33kN   147.96kN   176.18kN   188.15kN   215.32kN   228.41kN   244.05kN   245.23kN   245.11kN   
      56km/h   0.00kN   55.89kN   83.52kN   114.43kN   148.11kN   176.44kN   188.41kN   215.32kN   228.55kN   244.08kN   243.63kN   243.52kN   
      57km/h   0.00kN   56.04kN   83.64kN   114.52kN   148.25kN   176.70kN   188.66kN   215.32kN   228.69kN   242.40kN   241.89kN   241.79kN   
      58km/h   0.00kN   56.19kN   83.76kN   114.62kN   148.40kN   176.95kN   188.91kN   215.32kN   228.84kN   240.58kN   240.15kN   240.06kN   
      59km/h   0.00kN   56.33kN   83.87kN   114.71kN   148.54kN   177.21kN   189.16kN   215.32kN   228.98kN   238.77kN   238.41kN   238.34kN   
      60km/h   0.00kN   56.48kN   83.99kN   114.81kN   148.68kN   177.46kN   189.41kN   215.32kN   229.12kN   236.96kN   236.67kN   236.61kN   
      61km/h   0.00kN   56.62kN   84.11kN   114.90kN   148.82kN   177.71kN   189.66kN   215.32kN   229.27kN   235.15kN   234.93kN   234.89kN   
      62km/h   0.00kN   56.76kN   84.22kN   115.00kN   148.97kN   177.95kN   189.90kN   215.32kN   229.41kN   233.34kN   233.19kN   233.17kN   
      63km/h   0.00kN   56.91kN   84.34kN   115.09kN   149.11kN   178.20kN   190.14kN   215.32kN   229.55kN   231.53kN   231.46kN   231.44kN   
      64km/h   0.00kN   57.05kN   84.45kN   115.19kN   149.25kN   178.44kN   190.38kN   215.32kN   229.69kN   229.72kN   229.72kN   229.72kN   
      65km/h   0.00kN   57.19kN   84.57kN   115.28kN   149.38kN   178.68kN   187.17kN   214.51kN   225.88kN   227.92kN   229.72kN   229.72kN   
      66km/h   0.00kN   57.33kN   84.68kN   115.37kN   149.52kN   175.65kN   183.99kN   210.96kN   222.10kN   224.14kN   226.55kN   226.55kN   
      67km/h   0.00kN   57.46kN   84.79kN   115.46kN   149.66kN   172.65kN   180.82kN   207.42kN   218.34kN   220.39kN   222.80kN   222.80kN   
      68km/h   0.00kN   57.60kN   84.90kN   115.56kN   149.80kN   169.67kN   177.69kN   203.91kN   214.61kN   216.66kN   219.08kN   219.08kN   
      69km/h   0.00kN   57.74kN   85.01kN   115.65kN   149.93kN   166.72kN   174.60kN   200.43kN   210.91kN   212.96kN   215.37kN   215.37kN   
      70km/h   0.00kN   57.87kN   85.13kN   115.74kN   147.35kN   163.82kN   171.55kN   196.98kN   207.26kN   209.29kN   211.70kN   211.70kN   
      71km/h   0.00kN   58.01kN   85.24kN   115.83kN   144.80kN   160.96kN   168.56kN   193.57kN   203.66kN   205.67kN   208.06kN   208.06kN   
      72km/h   0.00kN   58.14kN   85.35kN   115.92kN   142.29kN   158.15kN   165.62kN   190.22kN   200.12kN   202.10kN   204.47kN   204.47kN   
      73km/h   0.00kN   58.28kN   85.46kN   116.01kN   139.82kN   155.41kN   162.74kN   186.91kN   196.64kN   198.60kN   200.93kN   200.93kN   
      74km/h   0.00kN   58.41kN   85.57kN   114.00kN   137.40kN   152.73kN   159.94kN   183.67kN   193.24kN   195.15kN   197.45kN   197.45kN   
      75km/h   0.00kN   58.54kN   85.67kN   112.04kN   135.03kN   150.12kN   157.21kN   180.51kN   189.92kN   191.79kN   194.03kN   194.03kN   
      76km/h   0.00kN   58.67kN   85.78kN   110.12kN   132.72kN   147.58kN   154.57kN   177.42kN   186.68kN   188.50kN   190.69kN   190.69kN   
      77km/h   0.00kN   58.80kN   85.89kN   108.25kN   130.47kN   145.13kN   152.01kN   174.41kN   183.54kN   185.31kN   187.43kN   187.43kN   
      78km/h   0.00kN   58.93kN   86.00kN   106.44kN   128.29kN   142.76kN   149.54kN   171.49kN   180.51kN   182.21kN   184.26kN   184.26kN   
      79km/h   0.00kN   59.06kN   84.55kN   104.69kN   126.17kN   140.48kN   147.17kN   168.67kN   177.57kN   179.21kN   181.19kN   181.19kN   
      80km/h   0.00kN   59.18kN   83.15kN   103.00kN   124.14kN   138.29kN   144.89kN   165.94kN   174.74kN   176.31kN   178.21kN   178.21kN   
      81km/h   0.00kN   59.31kN   81.79kN   101.37kN   122.17kN   136.18kN   142.70kN   163.31kN   172.02kN   173.52kN   175.34kN   175.34kN   
      82km/h   0.00kN   59.43kN   80.49kN   99.80kN   120.28kN   134.17kN   140.61kN   160.79kN   169.41kN   170.84kN   172.56kN   172.56kN   
      83km/h   0.00kN   58.50kN   79.23kN   98.30kN   118.47kN   132.24kN   138.61kN   158.36kN   166.92kN   168.26kN   169.90kN   169.90kN   
      84km/h   0.00kN   57.60kN   78.01kN   96.86kN   116.74kN   130.41kN   136.71kN   156.04kN   164.53kN   165.79kN   167.34kN   167.34kN   
      85km/h   0.00kN   56.74kN   76.85kN   95.49kN   115.08kN   128.66kN   134.90kN   153.82kN   162.25kN   163.44kN   164.89kN   164.89kN   
      86km/h   0.00kN   55.91kN   75.74kN   94.17kN   113.50kN   126.99kN   133.17kN   151.71kN   160.08kN   161.19kN   162.55kN   162.55kN   
      87km/h   0.00kN   55.12kN   74.68kN   92.92kN   111.99kN   125.41kN   131.54kN   149.69kN   158.01kN   159.05kN   160.31kN   160.31kN   
      88km/h   0.00kN   54.37kN   73.66kN   91.73kN   110.56kN   123.92kN   129.99kN   147.77kN   156.05kN   157.01kN   158.18kN   158.18kN   
      89km/h   0.00kN   53.65kN   72.70kN   90.60kN   109.20kN   122.50kN   128.52kN   145.95kN   154.19kN   155.07kN   156.15kN   156.15kN   
      90km/h   0.00kN   52.97kN   71.78kN   89.53kN   107.90kN   121.15kN   127.13kN   144.21kN   152.42kN   153.23kN   154.22kN   154.22kN   
      91km/h   0.00kN   52.32kN   70.90kN   88.51kN   106.67kN   119.88kN   125.82kN   142.57kN   150.75kN   151.48kN   152.39kN   152.39kN   
      92km/h   0.00kN   51.70kN   70.07kN   87.55kN   105.51kN   118.68kN   124.58kN   141.01kN   149.16kN   149.83kN   150.65kN   150.65kN   
      93km/h   0.00kN   51.11kN   69.28kN   86.63kN   104.41kN   117.54kN   123.40kN   139.54kN   147.66kN   148.26kN   149.00kN   149.00kN   
      94km/h   0.00kN   50.55kN   68.53kN   85.77kN   103.37kN   116.47kN   122.30kN   138.14kN   146.25kN   146.78kN   147.43kN   147.43kN   
      95km/h   0.00kN   50.02kN   67.82kN   84.95kN   102.38kN   115.45kN   121.25kN   136.82kN   144.91kN   145.37kN   145.95kN   145.95kN   
      96km/h   0.00kN   49.52kN   67.15kN   84.18kN   101.45kN   114.50kN   120.27kN   135.57kN   143.64kN   144.05kN   144.55kN   144.55kN   
      97km/h   0.00kN   49.05kN   66.52kN   83.45kN   100.57kN   113.60kN   119.34kN   134.39kN   142.45kN   142.79kN   143.22kN   143.22kN   
      98km/h   0.00kN   48.60kN   65.91kN   82.76kN   99.74kN   112.75kN   118.46kN   133.28kN   141.32kN   141.61kN   141.97kN   141.97kN   
      99km/h   0.00kN   48.18kN   65.35kN   82.10kN   98.95kN   111.94kN   117.64kN   132.23kN   140.26kN   140.49kN   140.79kN   140.79kN   
      100km/h   0.00kN   47.78kN   64.81kN   81.49kN   98.21kN   111.19kN   116.86kN   131.23kN   139.25kN   139.44kN   139.67kN   139.67kN   
      101km/h   0.00kN   47.40kN   64.30kN   80.91kN   97.51kN   110.48kN   116.13kN   130.30kN   138.31kN   138.44kN   138.61kN   138.61kN   
      102km/h   0.00kN   47.04kN   63.82kN   80.36kN   96.85kN   109.80kN   115.43kN   129.41kN   137.41kN   137.50kN   137.61kN   137.61kN   
      103km/h   0.00kN   46.70kN   63.37kN   79.84kN   96.22kN   109.17kN   114.78kN   128.58kN   136.57kN   136.61kN   136.67kN   136.67kN   
      104km/h   0.00kN   46.38kN   62.94kN   79.36kN   95.64kN   108.57kN   114.17kN   127.79kN   135.78kN   135.78kN   135.78kN   135.78kN   
      105km/h   0.00kN   46.09kN   62.54kN   78.86kN   95.04kN   107.89kN   113.45kN   126.99kN   133.59kN   133.59kN   133.59kN   133.59kN   
      106km/h   0.00kN   45.80kN   62.14kN   78.35kN   94.43kN   107.20kN   112.73kN   126.18kN   131.41kN   131.41kN   131.41kN   131.41kN   
      107km/h   0.00kN   45.50kN   61.74kN   77.85kN   93.82kN   106.51kN   112.00kN   125.36kN   129.24kN   129.24kN   129.24kN   129.24kN   
      108km/h   0.00kN   45.20kN   61.33kN   77.33kN   93.20kN   105.81kN   111.26kN   124.53kN   127.09kN   127.09kN   127.09kN   127.09kN   
      109km/h   0.00kN   44.90kN   60.92kN   76.81kN   92.57kN   105.10kN   110.51kN   123.70kN   124.94kN   124.94kN   124.94kN   124.94kN   
      110km/h   0.00kN   44.59kN   60.51kN   76.29kN   91.94kN   104.38kN   109.76kN   122.86kN   122.86kN   122.86kN   122.86kN   122.86kN   
      111km/h   0.00kN   44.28kN   60.09kN   75.76kN   91.31kN   103.66kN   109.00kN   120.72kN   120.72kN   120.72kN   120.72kN   120.72kN   
      112km/h   0.00kN   43.97kN   59.67kN   75.23kN   90.66kN   102.93kN   108.23kN   118.58kN   118.58kN   118.58kN   118.58kN   118.58kN   
      113km/h   0.00kN   43.66kN   59.24kN   74.69kN   90.01kN   102.19kN   107.46kN   116.46kN   116.46kN   116.46kN   116.46kN   116.46kN   
      114km/h   0.00kN   43.34kN   58.81kN   74.15kN   89.36kN   101.45kN   106.67kN   114.35kN   114.35kN   114.35kN   114.35kN   114.35kN   
      115km/h   0.00kN   43.02kN   58.37kN   73.60kN   88.70kN   100.69kN   105.88kN   112.25kN   112.25kN   112.25kN   112.25kN   112.25kN   
      116km/h   0.00kN   42.69kN   57.93kN   73.04kN   88.03kN   99.94kN   105.08kN   110.15kN   110.15kN   110.15kN   110.15kN   110.15kN   
      117km/h   0.00kN   42.37kN   57.49kN   72.48kN   87.35kN   99.17kN   104.28kN   108.07kN   108.07kN   108.07kN   108.07kN   108.07kN   
      118km/h   0.00kN   42.03kN   57.04kN   71.92kN   86.67kN   98.39kN   103.46kN   106.00kN   106.00kN   106.00kN   106.00kN   106.00kN   
      119km/h   0.00kN   41.70kN   56.58kN   71.34kN   85.98kN   97.61kN   102.64kN   103.95kN   103.95kN   103.95kN   103.95kN   103.95kN   
      120km/h   0.00kN   41.36kN   56.13kN   70.77kN   85.29kN   96.82kN   101.81kN   101.90kN   101.90kN   101.90kN   101.90kN   101.90kN     
   )                                          												
)

Comment (** Brzdy a Vzduchotechnika **)
         BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
  	BrakesEngineControllers( "Independent, Train, Dynamic, Blended" )

comment (** kompresor a tlaky v jimkach, vlastnosti potrubi **)

	AirBrakesMainMaxAirPressure( 10bar )
	AirBrakesCompressorRestartPressure( 8.5bar )
	AirBrakesMainResVolume( 900l )
	comment (** kompresor 3DKS100, saci vykon 120m^3/h. Vypoctena rychlost plneni jimky 0.04bar/s**)
	comment (** dvojice kompresoru: rychlost plneni jimky 2*0.04 = 0.08bar/s **)
	comment (** vypoctena doba plneni 900l jimky (oba kompresory) 2.24min. **)
	ORTSMainResChargingRate ( 0.08bar/s )
	ORTSBrakePipeChargingRate ( 4.6bar/s )
	ORTSBrakePipeTimeFactor ( 0.003 )
	ORTSBrakeServiceTimeFactor ( 1.009 )
	ORTSBrakeEmergencyTimeFactor ( 0.1 )

comment (** brzdic DAKO BP - max. tlak 6.4bar **)
comment (** pro plnou funkcnost svih/prebiti/odvetrani je potreba verze ORTS MGIC CZ/SK v1.2.1 **)

	EngineBrakesControllerMaxSystemPressure ( 10bar )
	EngineBrakesControllerFullServicePressureDrop ( 3.6bar )
	BrakeCylinderMaxSystemPressure ( 6.4bar )
	EngineBrakeController_BP1 ( 0.33 0.20 2bar/s )


comment (** brzdic DAKO BSE **)
comment (** pro plnou funkcnost svih/prebiti/odvetrani je potreba verze ORTS MGIC CZ/SK v1.2.1 **)
comment(** krivky strmosti plneni a odvetravani hlavniho potrubi **)

	BrakePipeChargeRate 
	( 						
		0.00bar 0.34bar/s					
		4.65bar 0.34bar/s
        	4.80bar 0.05bar/s
		5.00bar 0.05bar/s
		5.10bar 1.00bar/s
	)

	BrakePipeDischargeRate
	( 						
		0.00bar 0.28bar/s					
		4.65bar 0.28bar/s	
		5.00bar 1.00bar/s		
	)
	
comment (** provozni tlak pro plne odbrzdeni **)
        TrainBrakesControllerMaxSystemPressure ( 5bar )
comment (** max. strmost vysokotlakeho svihu **)
	TrainBrakesControllerMaxQuickReleaseRate ( 4.8bar/s )
comment (** max. tlak nizkotlakeho prebiti **)
	TrainBrakesControllerMaxOverchargePressure ( 5.4bar )
comment (** automaticke zavedeni nizkotlakeho prebiti po vypnuti vysokotlakeho svihu **)
	AutoOverchargePressure ( 1 )
comment (** strmost poklesu tlaku v ramci linearniho odvetrani **)
	OverchargeEliminationRate ( 0.0022bar/s )
	TrainBrakesControllerMaxReleaseRate ( 0.34bar/s )
	TrainBrakesControllerMaxApplicationRate ( 0.28bar/s )
	TrainBrakesControllerEmergencyApplicationRate ( 5.2bar/s )
	TrainBrakesControllerFullServicePressureDrop ( 1.5bar )


Comment (** EDB **)
	DynamicBrakesMaximumForce		( 160kN )
	DynamicBrakesResistorCurrentLimit	( 650 )
	DynamicBrakesDelayTimeBeforeEngaging	( 3 )
	DynamicBrakeHasAutoBailOff		( 1 )
        ORTSDynamicBlendingForceMatch           ( 0 )
        ORTSDynamicBlendingOverride             ( 0 )
        AutoBailOffOnRate( 2.2bar/s )

comment (** krivky prubehu brzdne sily EDB pro radu x63 = prevod do 120km/h max - autor: Igor Hnizdo **)

      ORTSDynamicBrakeForceCurves (
               0.00 (
                    0km/h    0kN
                    140km/h  0kN
               )
               1.00 (
                    0km/h    0kN
                    10km/h    0kN
                    11km/h   61.5kN
                    15km/h   82kN
                    20km/h   110kN
                    25km/h   137kN
                    29.5km/h   160kN
                    69.5km/h   160kN
                    70km/h   158.5kN
                    75km/h   149.5kN
                    80km/h   141kN
                    85km/h   133.5kN
                    90km/h   126.5kN
                    95km/h   119.5kN
                    100km/h  114kN
                    105km/h  109kN
                    110km/h  104kN
                    115km/h  98.5kN
                    120km/h  94kN
                    125km/h  89kN
                    130km/h  85kN
                    135km/h  82kN
                    140km/h  79kN
               )
)

	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 20 )
		MonitoringDeviceAlarmTimeLimit ( 10 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
Comment (** Ovladanie **)
	EngineControllers (

comment (** vykon **)
		Throttle ( 0 1 0.02 0
			NumNotches ( 0 )
		)
comment (** EDB **)
                Brake_Dynamic 	( 0 1 0.05 0
			NumNotches ( 0 )
		)

Comment (** Brzdic Dako BP **)
		Brake_Engine ( 0 1 0.125 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
comment (** Brzdic DAKO BSE **)
		Brake_Train 	( 0 1 0.05 0.8
			NumNotches ( 5
				Notch ( 0 0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.4 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.6 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.8 0 TrainBrakesControllerContinuousServiceStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)
		
		PantographToggle1	( 0 1 0 )
		DirControl 		( -1 0 1 1 )
		Horn 			( 0 1 0 )
		Sanding 		( 0 1 0 )
		Headlights 		( 0 0.5 1 0 )
		Wipers 			( 0 1 0 )
		BailOffButton		( 0 1 0 )
		Vigilance 		( 0 1 0 )
	)

	Name ( "CD 163 078-9 verze 2021" )

	Description (
		"Rada ZSSK 163 je univerzalni elektricka skrinova lokomotiva, pouzivana v osobni a nákladní doprave.\nTyp Bo'-Bo', napeti 3kV ss , 25kV 50Hz str.\n\nDelka pres narazniky: 16,8 m\n\nPrumer hnacich kol: 1250 mm\n\nHmotnost ve sluzbe: 87 t\n\n" +
		"Trvaly vykon trakcnich motoru: 3480 kW ss , 3060kW str.\n\n" +
		"Max. rychlost 120 km/h\n" +
		""
	)
)
