SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( MT_386-040-0
Comment ( "Sekce vozidlo" )
Comment ( "Popis fyziky vozu pro OR" )
Comment ( "Nastaveno pro provoz nakladni dopravy-140 kmh" )
Comment ( "Josef Vogeltanz - 06.01.2021" )

Comment ( "Obecne informace vozu" )
Type ( Engine )
WagonShape ( MT_386-040-0.s )

Size ( 3.052m 4.186m 18.9m )
Mass ( 84t )
WheelRadius ( 0.625m )
ORTSNumberAxles ( 0 )

ORTSFreightAnims (
MSTSFreightAnimEnabled ( 0 )
FreightAnimStatic ( 
SubType ( Default )
Shape ( MT_386-040-0_FREIGHT.s )
Offset ( 0.0, 0.0, 0.0 )
Flip ( 0 )
)
)

Comment ( "Sprahla" )
Coupling (
Type ( Chain )
Spring ( Stiffness ( 3.8e6N/m 2.5e8N/m ) Break ( 834kN 834kN ) r0 ( 0cm 2.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Coupling (
Type ( Chain )
Spring ( Stiffness ( 3.8e6N/m 2.5e8N/m ) Break ( 834kN 834kN ) r0 ( 0cm 2.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Comment ( "Brzdy" )
Comment ( "Brzdovy system Knorr, kotouce, Bv.: 90t" )
Comment ( "Rezim brzdeni P" )
BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

MaxBrakeForce ( 153kN )
MaxHandbrakeForce ( 70kN )
NumberOfHandbrakeLeverSteps ( 10 )

TripleValveRatio ( 2.5 )
MaxReleaseRate ( 0.212bar/s )
MaxApplicationRate ( 0.475bar/s )
MaxAuxilaryChargingRate ( 0.81bar/s )
EmergencyResChargingRate ( 0.81bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 4bar )
EmergencyResVolumeMultiplier ( 2.5 )
EmergencyResCapacity ( 150l )
BrakePipeVolume ( 16.4l )

ORTSBrakeShoeFriction (
0   0.420
8   0.346
16  0.306 
24  0.286 
32  0.272 
40  0.264 
48  0.258 
56  0.252 
64  0.246 
72  0.241 
80  0.236 
88  0.231 
96  0.228 
104 0.225 
112 0.223 
120 0.222 
128 0.222 
136 0.221 
144 0.220 
152 0.220 
160 0.220 
168 0.220 
176 0.220 
184 0.220 
192 0.220 
200 0.220
)

Comment ( "Jizdni odpory a treni" )
CentreOfGravity ( 0m 2.09m  0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 2m 600mm )
ORTSUnbalancedSuperelevation ( 150mm )

ORTSBearingType ( Low )
ORTSDavis_A ( 944.6 )
ORTSDavis_B ( 18.42 )
ORTSDavis_C ( 6.3825 )

ORTSAdhesion (
ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
ORTSSlipWarningThreshold ( 60 )
)

Comment ( "Pantografy" )
ORTSPantographs (
Pantograph (
Delay ( 3s ) 
) 
Pantograph ( 
Delay ( 3s )
)
)

Comment ( "Ostatni informace" )
Sound ( "146-2Eng.sms" )
Include ( "LIGHTS/LIGHTS-MTR386040-CZ.inc" )
)

Engine ( MT_386-040-0
Comment ( "Sekce pohon" )
Comment ( "Obecne informace pohonu" )
Wagon ( MT_386-040-0 )
Name ( "MTR_386-040-0" )

Comment ( "Pohon" )
Type ( Electric )
MaxVelocity ( 140km/h )
WheelRadius ( 0.625m )
Sanding ( 100km/h )
ORTSNumberDriveAxles ( 4 )
ORTSDriveWheelWeight ( 84t )
MaxForce ( 300kN )
MaxContinuousForce ( 258kN )
MaxPower ( 5600kW )
MaxCurrent ( 1050A )
BrakeCutsPowerAtBrakeCylinderPressure ( 1.4bar )

ORTSCircuitBreaker ( Manual )
ORTSCircuitBreakerClosingDelay ( 2s )
ORTSPowerOnDelay ( 5s )

ORTSContinuousForceTimeFactor ( 3600 )
ORTSTractionCharacteristics ( 29 12
throttle ( 0 0.22 0.31 0.4 0.49 0.58 0.67 0.76 0.85 0.94 1.00 )
table (
0km/h   0kN 66kN 93kN 120kN 147kN 174kN 201kN 228kN 255kN 282kN 300kN
5km/h   0kN 65kN 92kN 118kN 145kN 172kN 198kN 225kN 252kN 278kN 296kN
10km/h  0kN 64kN 91kN 117kN 143kN 169kN 196kN 222kN 248kN 274kN 292kN
15km/h  0kN 63kN 89kN 115kN 141kN 167kN 193kN 219kN 245kN 271kN 288kN
20km/h  0kN 62kN 88kN 114kN 139kN 165kN 190kN 216kN 241kN 267kN 284kN
25km/h  0kN 62kN 87kN 112kN 138kN 163kN 188kN 214kN 239kN 264kN 281kN
30km/h  0kN 61kN 86kN 111kN 136kN 161kN 186kN 211kN 236kN 261kN 278kN
35km/h  0kN 61kN 85kN 110kN 135kN 160kN 184kN 209kN 234kN 259kN 275kN
40km/h  0kN 60kN 84kN 109kN 133kN 158kN 182kN 207kN 231kN 256kN 272kN
45km/h  0kN 59kN 83kN 107kN 131kN 155kN 180kN 204kN 228kN 252kN 268kN
50km/h  0kN 58kN 82kN 106kN 130kN 154kN 178kN 201kN 225kN 249kN 265kN
55km/h  0kN 58kN 81kN 105kN 128kN 152kN 176kN 199kN 223kN 246kN 262kN
60km/h  0kN 57kN 80kN 104kN 127kN 150kN 174kN 197kN 220kN 243kN 259kN
65km/h  0kN 56kN 79kN 102kN 125kN 148kN 171kN 194kN 217kN 240kN 255kN
70km/h  0kN 55kN 78kN 101kN 123kN 146kN 169kN 192kN 214kN 237kN 252kN
75km/h  0kN 55kN 77kN 100kN 122kN 144kN 167kN 189kN 212kN 234kN 249kN
80km/h  0kN 53kN 74kN 96kN  118kN 139kN 161kN 182kN 204kN 226kN 240kN
85km/h  0kN 49kN 69kN 89kN  109kN 129kN 149kN 169kN 190kN 210kN 223kN
90km/h  0kN 46kN 64kN 83kN  101kN 120kN 139kN 157kN 176kN 195kN 207kN
95km/h  0kN 42kN 60kN 77kN  95kN  112kN 129kN 147kN 164kN 181kN 193kN
100km/h 0kN 40kN 56kN 72kN  88kN  104kN 121kN 137kN 153kN 169kN 180kN
105km/h 0kN 37kN 52kN 68kN  83kN  98kN  113kN 128kN 144kN 159kN 169kN
110km/h 0kN 35kN 49kN 63kN  77kN  92kN  106kN 120kN 134kN 149kN 158kN
115km/h 0kN 33kN 46kN 59kN  73kN  86kN  99kN  112kN 126kN 139kN 148kN
120km/h 0kN 31kN 43kN 56kN  69kN  81kN  94kN  106kN 119kN 132kN 140kN
125km/h 0kN 29kN 41kN 53kN  65kN  77kN  88kN  100kN 112kN 124kN 132kN
130km/h 0kN 28kN 39kN 50kN  61kN  73kN  84kN  95kN  106kN 118kN 125kN
135km/h 0kN 26kN 37kN 47kN  58kN  68kN  79kN  90kN  100kN 111kN 118kN
140km/h 0kN 25kN 35kN 45kN  55kN  65kN  75kN  85kN  95kN  105kN 112kN
)
)

Comment ( "Brzdy" )
Comment ( "Brzdovy system Knorr, brzdice Brzdic BSE 5 poloh, Brzdic Knorr 3p, kompresor SC-20-5-51" )
Comment ( "Brzdeni I.zpusob, rezim brzdeni P" )
BrakesTrainBrakeType ( "Air_single_pipe" )
BrakesEngineControllers ( "Independent, Train, Dynamic, Blended" )

ORTSDynamicBrakeForceCurves (
0 ( 0.0 0 44.4 0 )
0.2 ( 0.0 0 2.8 30000  5.6 30000  8.3 30000  11.1 30000  13.9 30000  16.7 30000  19.4 30000  22.2 30000  25.0 30000  27.8 30000  30.6 30000  33.3 30000  36.1 30000  38.9 28600 )
0.4 ( 0.0 0 2.8 60000  5.6 60000  8.3 60000  11.1 60000  13.9 60000  16.7 60000  19.4 60000  22.2 60000  25.0 60000  27.8 60000  30.6 60000  33.3 60000  36.1 60000  38.9 57200 )
0.6 ( 0.0 0 2.8 90000  5.6 90000  8.3 90000  11.1 90000  13.9 90000  16.7 90000  19.4 90000  22.2 90000  25.0 90000  27.8 90000  30.6 90000  33.3 90000  36.1 90000  38.9 85800 )
0.8 ( 0.0 0 2.8 120000 5.6 120000 8.3 120000 11.1 120000 13.9 120000 16.7 120000 19.4 120000 22.2 120000 25.0 120000 27.8 120000 30.6 120000 33.3 120000 36.1 120000 38.9 114400 )
1.0 ( 0.0 0 2.8 150000 5.6 150000 8.3 150000 11.1 150000 13.9 150000 16.7 150000 19.4 150000 22.2 150000 25.0 150000 27.8 150000 30.6 150000 33.3 150000 36.1 150000 38.9 143000 )
)

DynamicBrakesMaximumForce ( 150kN )
DynamicBrakesResistorCurrentLimit ( 600A )
DynamicBrakesDelayTimeBeforeEngaging ( 5s )
DynamicBrakeHasAutoBailOff ( 1 )
DynamicBrakesMaximumSpeedForFadeOut ( 140km/h )
DynamicBrakesMaximumEffectiveSpeed ( 135km/h )
DynamicBrakesEffectAtMaximumFadeOut ( 0 )
DynamicBrakesFadingSpeed ( 10km/h )
DynamicBrakesMinUsableSpeed ( 5km/h )
ORTSDynamicBlendingForceMatch ( 1 )
ORTSDynamicBlendingOverride ( 0 )
DoesBrakeCutPower ( 1 )

ORTSMainResChargingRate ( 0.05bar/s )
ORTSBrakePipeChargingRate ( 20.7bar/s ) 
AirBrakesMainMaxAirPressure ( 10bar )
AirBrakesMainResVolume ( 800l )
AirBrakesCompressorRestartPressure ( 8.5bar )
TrainPipeLeakRate ( 0.0042bar/s )

ORTSEngineBrakeReleaseRate ( 1.0bar/s )
ORTSEngineBrakeApplicationRate ( 1.3bar/s )
EngineBrakesControllerMinPressureReduction ( 0.3bar )
EngineBrakesControllerFullServicePressureDrop ( 1.0bar )
EngineBrakesControllerMaxApplicationRate ( 1.33bar/s )
EngineBrakesControllerMaxReleaseRate ( 1.0bar/s )
EngineBrakesControllerMaxSystemPressure ( 5bar )

TrainBrakesControllerMinPressureReduction ( 0.3bar )
TrainBrakesControllerFullServicePressureDrop ( 1.5bar )
TrainBrakesControllerMaxReleaseRate ( 0.5bar/s )
TrainBrakesControllerMaxApplicationRate ( 0.5bar/s )
TrainBrakesControllerMaxQuickReleaseRate ( 2.0bar/s )
TrainBrakesControllerEmergencyApplicationRate ( 1.86bar/s )
TrainBrakesControllerMaxSystemPressure ( 5bar )

ORTSBrakePipeTimeFactor ( 0.003 )
ORTSBrakeServiceTimeFactor ( 1.009 )
ORTSBrakeEmergencyTimeFactor ( 0.1 ) 

Comment ( "Ovladani jizdy" )

Comment ( "Vlakovy zabezpecovac - pouze KBS" )
VigilanceMonitor (
MonitoringDeviceMonitorTimeLimit ( 16 )
MonitoringDeviceAlarmTimeLimit ( 6 )
MonitoringDevicePenaltyTimeLimit ( 0 )
MonitoringDeviceCriticalLevel ( 0 )
MonitoringDeviceResetLevel ( 0 )
MonitoringDeviceAppliesFullBrake ( 0 )
MonitoringDeviceAppliesEmergencyBrake ( 1 )
MonitoringDeviceAppliesCutsPower ( 1 )
MonitoringDeviceAppliesShutsDownEngine ( 0 )
MonitoringDeviceResetOnResetButton ( 1 )
MonitoringDeviceResetOnZeroSpeed ( 1 )
)

Comment ( "Rizeni" )

EngineControllers (

Throttle ( 0 1 0.02 0 
NumNotches ( 1 
Notch ( 0 1 Dummy ) 
)
)

Brake_Dynamic ( 0 1 0.05 0
NumNotches ( 0 )
)

Brake_Engine ( 0 1 0.1 0
NumNotches ( 1
Notch ( 0 1 Dummy )
)
)

Brake_Train ( 0 1 0.1 0.2
NumNotches ( 6
Notch ( 0.0 0 TrainBrakesControllerFullQuickReleaseStart )
Notch ( 0.1 0 TrainBrakesControllerReleaseStart )
Notch ( 0.2 0 TrainBrakesControllerNeutralhandleOffStart )
Notch ( 0.3 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
Notch ( 0.9 0 TrainBrakesControllerSuppressionStart )
Notch ( 1.0 0 TrainBrakesControllerEmergencyStart )
)
)

Brake_Hand ( 0 1 0.025 0
NumNotches ( 0 )
)

DirControl ( -1 0 1 1 )
Sanding ( 0 1 0 )
Horn ( 0 1 0 )
Wipers ( 0 1 0 )
EmergencyStopToggle ( 0 1 1 )
Vigilance ( 0 1 0 )
PantographToggle1 ( 0 1 0 )
Headlights ( 0 0.25 1 0 )
)

Comment ( "Ostatni informace" )
Sound ( "146-2Cab.sms" )
CabView ( "es64f4_classVM_cz.cvf" )
HeadOut ( 1.7 2.9 7.4 )

Comment ( "Poznamky" )
Description (
"Pokyny pro obecne nastaveni OR:\n"+
"-> Karta Obecne: Rychlost plneni brzdoveho potrubi 1000 PSI/s (nutne aby OR akceptoval hodnoty engu!)\n"+
"-> Karta Simulace: Pokrocily model adheze\n"+
"-> Karta Experimentalni: Faktor korekce adheze 100%\n"+
"-> Karta Experimentalni: Nahodna zmena faktoru adheze 10%\n\n"+ 
"Rada 386.0 je vicesystemova univerzalni lokomotiva\n"+
"Typ TRAXX F140 MS2e od Bombardier Transportation"
"pro pouziti v nakladni i osobni doprave\n\n"+
"Roky vyroby: 2014 az 2017\n\n"+
"Napajeni: AC 15 kV a 25 kV, DC 3 kV a 1,5 kV\n\n"+
"Trvaly vykon: 5600 kW\n\n"+
"Max. provozni rychlost:  140 km/h naklad, 160 km/h osobni\n\n"+
"Max. tazna sila na haku: 300 kN\n\n"+
"Trvala tazna sila na haku: 258 kN\n\n"+
"Delka pres nar.: 18900 mm\n\n"+
"Hmotnost lokomotivy: 85 t"  
)
EngineOperatingProcedures (
"Viz. manual Open Rails.\n\n"+
"TIP: V prubehu jizdy pomoc na klavese F1."
)
)