SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( csd_240086
	Type ( Engine )
	WagonShape ( csd_240086.s )
        Freightanim ( csd_240086fa.s 1 1 )

	Comment ( Eng created by ZSR - http://csd.webzdarma.cz )
	Comment ( Datum: 19/12/2008 )
	Comment ( Version: 1.07 )
	Comment ( Svetla: Robo )

	

comment	( Overall physics )

	Mass ( 84.5t )
	Size  ( 3.03m 4.55m 16.165m )
	CentreOfGravity ( 0m 2.25m 0m )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box ( 3.03m 4.55m 16.165m ) )	

Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)

comment	( Adhesion and Friction )

	Adheasion ( 0.07 0.75 1.3 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*85t )
	DerailBufferForce ( 800kN )
	NumWheels (	4 )
	Friction (
		3000N/m/s		0		11.5mph		25N/m/s		2.2
		5.1N/rad/s		1		-1rad/s		0		1
	)



comment	( Wagon Brakes )

 	Comment ( P=52kN, G=32kN )
 	
	MaxBrakeForce( 52kN )
	MaxHandbrakeForce( 18kN )
	NumberOfHandbrakeLeverSteps( 100 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 1.3 )
	MaxApplicationRate( 4 )
	MaxAuxilaryChargingRate( 2.5 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 11 )
	EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 )
	
comment	( Freight, Inside, IntakePoint )

		
   	
	Inside (
		PassengerCabinFile ( csd_240086.s )
		PassengerCabinHeadPos ( -1.7 3.2 5.7 )
		RotationLimit ( 40 90 0 )
		StartDirection ( 0 -90 0 )
	)

comment	( Lights )
comment ( svetelne kuzely ) 
	
	Lights ( 32
		Light (
			comment ( Svetelny kuzel dálkovy )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFFF )
					Position ( 0 1 8 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 120 )
				)
			)
		)
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( reflektor lavy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.09 3.8 7.48 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 7 7 7 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.09 3.8 7.48 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 7 7 7 )
				)
			)
		)
                Light (
			comment ( reflektor tretie svetlo )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFE085 )
					Position ( 0 4.0 7.52 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.1 )
				)
			)
		)
		Light (
			comment ( predne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( -0.67 1.690 7.54 )
					Azimuth ( -15 -15 -15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( predne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( 0.67 1.690 7.5 )
					Azimuth ( 15 15 15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.77 1.690 -7.5 )
					Azimuth ( -165 -165 -165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.77 1.690 -7.5 )
					Azimuth ( 165 165 165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		
		comment ( Definicia svetiel pre zadne stanoviste )

		Light (
			comment ( reflektor lavy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.09 3.8 -7.48 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 7 7 7 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.09 3.8 -7.48 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 7 7 7 )
				)
			)
		)
                Light (
			comment ( reflektor tretie svetlo )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFE085 )
					Position ( 0 4.0 -7.52 )
					Azimuth ( 180 180 180 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.1 )
				)
			)
		)
		Light (
			comment ( predne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D  )
					Position ( 0.67 1.690 -7.5 )
					Azimuth ( 165 165 165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( predne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D  )
					Position ( -0.67 1.690 -7.5 )
					Azimuth ( -165 -165 -165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( zadne lave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.77 1.690 7.5 )
					Azimuth ( 15 15 15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( zadne prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.77 1.690 7.5 )
					Azimuth ( -15 -15 -15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
                comment ( Definicia svetiel pre podvozky )
                Light (
			comment ( Prave predne Vo)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 1.40 0.772 4.854 )
					Azimuth ( 0 0 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		) 
                Light (
			comment ( Lave predne Vo)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -1.40 0.772 4.854 )
					Azimuth ( 0 -180 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)   
                Light (
			comment ( Prave zadne Vo)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 1.40 0.772 -4.854 )
					Azimuth ( 0 0 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		) 
                Light (
			comment ( Lave zadne Vo)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -1.40 0.772 -4.854 )
					Azimuth ( 0 -180 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)    
                Light (
			comment ( Prave predne Vn)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 1.40 0.772 2.915 )
					Azimuth ( 0 0 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		) 
                Light (
			comment ( Lave predne Vn)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -1.40 0.772 2.915 )
					Azimuth ( 0 -180 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)   
                Light (
			comment ( Prave zadne Vn)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 1.40 0.772 -2.915 )
					Azimuth ( 0 0 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		) 
                Light (
			comment ( Lave zadne Vn)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -1.40 0.772 -2.915 )
					Azimuth ( 0 -180 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)   
                comment ( Definicia svetiel pre posunujuci diel )

		Light (
			comment ( Predne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( 0.67 1.690 7.5 )
					Azimuth ( 15 15 15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( zadne leve pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( -0.67 1.690 -7.5 )
					Azimuth ( -165 -165 -165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		
		
		comment ( Definicia svetiel pre Loose consist )

		Light	(
			comment( Prave predne pozicne - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( 0.67 1.690 7.5 )
					Azimuth ( 15 15 15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light	(
			comment( Lave zadne pozicne - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( -0.67 1.690 -7.5 )
					Azimuth ( -165 -165 -165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		

		comment ( Definicia svetiel pre HDV ovladane PC )

		Light (
			comment ( PC predne prave )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D  )
					Position ( 0.67 1.690 7.5 )
					Azimuth ( 15 15 15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( PC predne leve )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D  )
					Position ( -0.67 1.690 7.5 )
					Azimuth ( -15 -15 -15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( reflektor tretie svetlo )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFE085 )
					Position ( 0 4.0 7.52 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.1 )
				)
			)
		)
		Light (
			comment ( PC zadne lave koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.77 1.690 -7.5 )
					Azimuth ( -165 -165 -165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( PC zadne prave koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.77 1.690 -7.5 )
					Azimuth ( 165 165 165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
	)
comment	( EngSound )

	Sound ( "..\\..\\common.snd\\sndelok\\240eng.sms" )


)

  Engine ( csd_240086 
  Wagon ( csd_240086 )  
	Name ( "CSD_240.086-9" )

	
comment	( Basic physical engine data )

	Type ( Electric )
	MaxPower ( 3584kW )
	MaxForce ( 3889kN )	
	MaxContinuousForce ( 3889kN )
	MaxCurrent ( 24500A ) 
	MaxVelocity ( 120kmh )
	DieselEngineSpeedOfMaxTractiveEffort( 0mph )  
	WheelRadius ( 0.625m )
	comment( sanding system is switched off when faster than given velocity )
	Sanding ( 1e9mph )
	NumWheels ( 4 )

	
comment	( CabSound and Views )

	Sound ( "..\\..\\common.snd\\sndelok\\240cab.sms" )
	
	CabView ( "../../common.cab/cab240zssk/240zscs.cvf" )
	HeadOut (1.7 3.2 5.7 )
	


comment	( Brakes )


	AirBrakesAirCompressorPowerRating ( 1.18 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 145 )	
	AirBrakesMainResVolume ( 42.378 )
	AirBrakesAirCompressorWattage ( 16000 )
	AirBrakesCompressorRestartPressure ( 116 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 3 )
	TrainBrakesControllerMaxApplicationRate ( 1 )
	TrainBrakesControllerMaxReleaseRate ( 0.5 )
	TrainBrakesControllerMaxQuickReleaseRate ( 1.5 )
	TrainBrakesControllerEmergencyApplicationRate ( 3 )
	TrainBrakesControllerMinSystemPressure ( 3 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22 )
	TrainPipeLeakRate ( 0.033 )
	TrainBrakesControllerFullServicePressureDrop ( 22 )
	
	DynamicBrakesResistorCurrentLimit    ( 3581 )
	DynamicBrakesDelayTimeBeforeEngaging   ( 3 )
	DynamicBrakesNumberOfControllerNotches   ( 36 )
	DynamicBrakesMaxAirBrakePressure    ( 20 )
	DynamicBrakeHasAutoBailOff      ( 1 )
	DynamicBrakesMaximumForce      ( 724kN )
	DynamicBrakesLowerSpeedCurveExponent   ( 1 )
	DynamicBrakesMinUsableSpeed      ( 6.21 )
	DynamicBrakesFadingSpeed      ( 80.78 )
	DynamicBrakesMaximumEffectiveSpeed    ( 80.78 )
	DynamicBrakesMaximumSpeedForFadeOut    ( 80.78 )
	DynamicBrakesEffectAtMaximumFadeOut    ( 0 )
	DynamicBrakesCutInSpeed       ( 6.21 )
	DynamicBrakesCutOutSpeed       ( 6.21 )
	DynamicBrakesHigherSpeedCurveExponent   ( 1 )	


	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train, Dynamic" )

	DoesBrakeCutPower ( 1 )

comment ( Monitors )


EmergencyStopMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0 )
  MonitoringDeviceAlarmTimeLimit ( 0 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 0 )
  MonitoringDeviceResetLevel ( 0 )
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  
 )
 VigilanceMonitor (
  MonitoringDeviceMonitorTimeLimit ( 27 )
  MonitoringDeviceAlarmTimeLimit ( 17 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 0 )
  MonitoringDeviceResetLevel ( 0 )
  
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceResetOnZeroSpeed ( 1 )
  MonitoringDeviceResetOnResetButton ( 1 )
  MonitoringDeviceResetOnDirectionNeutral ( 1 )
 )
 OverspeedMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0 )
  MonitoringDeviceAlarmTimeLimit ( 5 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 78.7 )
  MonitoringDeviceResetLevel ( 0 )
  Comment ( MonitoringDeviceTriggerOnHighCurrent ( 1250 ) )
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 0 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceAlarmTimeBeforeOverSpeed ( 0 )
  MonitoringDeviceDoesSuppressionReset ( 0 )
  MonitoringDeviceTriggerOnOverspeed ( 77.6 )
  MonitoringDeviceTriggerOnTrackOverspeed ( 0 )
  MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnResetButton ( 0 )
 )
		
	 
Comment	( Controllers )

        EngineControllers (
		Throttle ( 0 1 0.001 0
			NumNotches ( 69
			    Notch ( 0.0   0 Dummy )
			    
			    Notch ( 0.01  0 Dummy )
			    Notch ( 0.011 0 Dummy )
			    
			    Notch ( 0.02  0 Dummy )
			    Notch ( 0.021 0 Dummy )
			    
			    Notch ( 0.025 0 Dummy )
			    Notch ( 0.026 0 Dummy )
			    
			    Notch ( 0.03   0 Dummy )
			    Notch ( 0.031 0 Dummy )
			    
			    Notch ( 0.04  0 Dummy )
			    Notch ( 0.041 0 Dummy )
			    
			    Notch ( 0.05   0 Dummy )
			    Notch ( 0.051 0 Dummy )
			    
			    Notch ( 0.08  0 Dummy )
			    Notch ( 0.081 0 Dummy )
			    
			    Notch ( 0.1   0 Dummy )
			    Notch ( 0.101 0 Dummy )
			    
			    Notch ( 0.12  0 Dummy )
			    Notch ( 0.121 0 Dummy )
			    
			    Notch ( 0.14  0 Dummy )
			    Notch ( 0.141 0 Dummy )
			    
			    Notch ( 0.16   0 Dummy )
			    Notch ( 0.161 0 Dummy )
			    
			    Notch ( 0.19  0 Dummy )
			    Notch ( 0.191 0 Dummy )
			    
			    Notch ( 0.21  0 Dummy )
			    Notch ( 0.211 0 Dummy )
			    
			    Notch ( 0.24  0 Dummy )
			    Notch ( 0.241 0 Dummy )
			    
			    Notch ( 0.26  0 Dummy )
			    Notch ( 0.261 0 Dummy )
			    
			    Notch ( 0.29   0 Dummy )
			    Notch ( 0.291 0 Dummy )
			    
			    Notch ( 0.32  0 Dummy )
			    Notch ( 0.321 0 Dummy )
			    
			    Notch ( 0.35  0 Dummy )
			    Notch ( 0.351 0 Dummy )
			    
			    Notch ( 0.37  0 Dummy )
			    Notch ( 0.371 0 Dummy )
			    
			    Notch ( 0.40  0 Dummy )
			    Notch ( 0.401 0 Dummy )
			    
			    Notch ( 0.43   0 Dummy )
			    Notch ( 0.431 0 Dummy )
			    
			    Notch ( 0.46  0 Dummy )
			    Notch ( 0.461 0 Dummy )
			    
			    Notch ( 0.48  0 Dummy )
			    Notch ( 0.481 0 Dummy )
			    
			    Notch ( 0.51  0 Dummy )
			    Notch ( 0.511 0 Dummy )
			    
			    Notch ( 0.54  0 Dummy )
			    Notch ( 0.541 0 Dummy )
			    
			    Notch ( 0.58   0 Dummy )
			    Notch ( 0.581 0 Dummy )
			    
			    Notch ( 0.61  0 Dummy )
			    Notch ( 0.611 0 Dummy )
			    
			    Notch ( 0.64  0 Dummy )
			    Notch ( 0.641 0 Dummy )
			    
			    Notch ( 0.67  0 Dummy )
			    Notch ( 0.671 0 Dummy )
			    
			    Notch ( 0.70  0 Dummy )
			    Notch ( 0.701 0 Dummy )
			    
			    Notch ( 0.73  0 Dummy )
			    Notch ( 0.731 0 Dummy )
			    
			    Notch ( 0.75  0 Dummy )
			    Notch ( 0.751 0 Dummy )
			    
			    Notch ( 0.81  0 Dummy )
			    Notch ( 0.86  0 Dummy )
			    Notch ( 0.92  0 Dummy )
			    Notch ( 1     0 Dummy )
		)
	)           

		
	comment (***Primocinna brzda typ DAKO-BP***)
		Brake_Engine ( 0 0.8 0.05 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )                   
                )
            )
        comment (***Prubezna brzda typ DAKO-BS2***)
		Brake_Train ( 0 1 0.04 0.87
			NumNotches ( 7
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
				Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)

            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
		
            Brake_Dynamic  ( 0 1 0.001 0
			NumNotches ( 48
			    Notch ( 0.0   0 Dummy )
			    Notch ( 0.001   0 Dummy )
			    
			    Notch ( 0.01  0 Dummy )
			    Notch ( 0.011 0 Dummy )
			    
			    Notch ( 0.02  0 Dummy )
			    Notch ( 0.021 0 Dummy )
			    
			    Notch ( 0.025 0 Dummy )
			    Notch ( 0.026 0 Dummy )
			    
			    Notch ( 0.03   0 Dummy )
			    Notch ( 0.031 0 Dummy )
			    
			    Notch ( 0.04  0 Dummy )
			    Notch ( 0.041 0 Dummy )
			    
			    Notch ( 0.05   0 Dummy )
			    Notch ( 0.051 0 Dummy )
			    
			    Notch ( 0.08  0 Dummy )
			    Notch ( 0.081 0 Dummy )
			    
			    Notch ( 0.1   0 Dummy )
			    Notch ( 0.101 0 Dummy )
			    
			    Notch ( 0.12  0 Dummy )
			    Notch ( 0.121 0 Dummy )
			    
			    Notch ( 0.14  0 Dummy )
			    Notch ( 0.141 0 Dummy )
			    
			    Notch ( 0.16   0 Dummy )
			    Notch ( 0.161 0 Dummy )
			    
			    Notch ( 0.19  0 Dummy )
			    Notch ( 0.191 0 Dummy )
			    
			    Notch ( 0.21  0 Dummy )
			    Notch ( 0.211 0 Dummy )
			    
			    Notch ( 0.24  0 Dummy )
			    Notch ( 0.241 0 Dummy )
			    
			    Notch ( 0.26  0 Dummy )
			    Notch ( 0.261 0 Dummy )
			    
			    Notch ( 0.29   0 Dummy )
			    Notch ( 0.291 0 Dummy )
			    
			    Notch ( 0.32  0 Dummy )
			    Notch ( 0.321 0 Dummy )
			    
			    Notch ( 0.35  0 Dummy )
			    Notch ( 0.351 0 Dummy )
			    
			    Notch ( 0.37  0 Dummy )
			    Notch ( 0.371 0 Dummy )
			    
			    Notch ( 0.40  0 Dummy )
			    Notch ( 0.401 0 Dummy )
			    
			    Notch ( 0.43   0 Dummy )
			    Notch ( 0.431 0 Dummy )
			    
			    Notch ( 0.46  0 Dummy )
			    Notch ( 0.461 0 Dummy )
			    
			    Notch ( 0.48  0 Dummy )
			    Notch ( 0.481 0 Dummy )
			    
	       		)
  		)
	    Combined_Control( 0 2 1 1 throttle dynamic  )	
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            BailOffButton( 0 1 0 )
        )
	
Comment	( Operations )

	 Description (
	  "Rada 240 ZSCS je univerzální elektrická skrínová lokomotiva, pouzívaná v nákladní doprave.\n\n"+
	  "Typ Bo'-Bo', napeti 25 kV 50Hz.\n\n"+
	  "Délka pres nárazniky: 16,44 m\n\n"+
	  "Prumer hnacích kol: 1250 mm\n\n"+
	  "Hmotnost ve sluzbe: 84.5 t\n\n"+
	  "Trvaly vykon trakcních motoru: 3080 kW\n\n"+
	  "Max. rychlost 110 km/h\n\n"+
	  "Ovladani a proudy v MSTS:\n\n"+
	  "Maximalni proud (nadproudova ochrana): 1250A\n\n"+
	  "Trvaly proud: 1100A\n\n"+
	  "Hodinovy proud: 1140A\n\n"+
	  "15 minutovy proud: 1300A\n\n"+
	  "5 minutovy proud: 1500A\n\n"+
	  "Proud na mezi adheze (skluz): 1548A\n\n"+
	  "Proud na mezi adheze s piskovanim (skluz): 1961A\n\n"+
	  "Kontroler: 32 stupnu (1%-75%) + 4 shuntovaci (81%-100%)\n\n"+
	  "EDB: 23 stupnu (1%-48%)\n\n"+
	  "Maximalni vykon EDB: 2000kW\n\n"+
	  "Maximalni proud kotvy EDB pri rychlosti  57km/h: 760A\n\n"+	  
	  "Maximalni proud kotvy EDB pri rychlosti  80km/h: 544A\n\n"+
	  "Maximalni proud kotvy EDB pri rychlosti 100km/h: 438A\n\n"+
	  "Maximalni proud kotvy EDB pri rychlosti 120km/h: 333A\n\n"+
	  "Maximalni proud buzeni EDB: 1250A\n\n"+
	  "Maximalni proud buzeni EDB na meraku, ktery nesmite prekrocit!: 760A\n\n"
	 )

	 EngineOperatingProcedures (
	  "Jak se rozjet\n"+
	  "1. Uz máte zvednutý pantograf. (Pokud z nejakého duvodu zvednutý není, stisknete klávesu P pro jeho zvednutí.)\n"+
	  "2. Stisknete W na prestavení reverzního kontoleru do polohy 'vpred'.\n"+
	  "3. Stisknete a drzte ; pro odbrzdení vlakové brzdy.\n"+
	  "(4. Stisknete a drzte [ pro odbrzdení lokomotivní brzdy.)\n"+
	  "5. Stisknete D pro zvýsení pozadovaného výkonu.\n"+
	  "6. Pomalu zvysujte výkon stiskem D, dokud vlak nedosáhne pozadované rychlosti.\n\n"+
	  "Jak zpomalit\n"+
	  "1. Stisknete A pro snízení pozadovaného výkonu (postupne az na 0).\n"+
	  "2. Jestlize je to nutné tak pouzijte brzdy pro postupné rychlejsí snizování rychlosti.\n\n"+
	  "Jak pouzít vlakovou brzdu\n"+
	  "1. Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosáhnete pozadovaného brzdného tlaku.\n"+
	  "2. Po dosazení pozadovaného brzd. tlaku stiskem ; presunte rukojet brzdy do polhy ZÁVER.\n\n"+
	  "Jak odbrzdit vlakovou brzdu\n"+
	  "1. Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENÍ.\n"+
	  "2. Pockejte, az klesne tlak v brzdových valcích na 0.\n"+
	  "3. Stisknete ' pro presunutí rukojeti brzdy do polohy ZÁVER.\n"+
	  "Jak pouzít lokomotvní brzdu\n"+
	  "1. Stisknete a drzte ] pro zabrzdení lokomotivní brzdy (0-100%).\n\n"+
	  "Jak odbrzdit lokomotivní brzdu\n"+
	  "1. Stisknete a drzte [ pro odbrzdení lokomotivní brzdy (0-100%).\n\n"+
	  "Jak pouzít zachrannou brzdu\n"+
	  "1. Stisknete a drzte A pro snízení výkonu az na 0.\n"+
	  "2. Stisknete BACKSPACE pro aktivaci záchrané brzdy.\n\n"+
	  "Jak zrusit záchrannou brzdu\n"+
	  "1. Pockejte na úplné zastavení vlaku.\n"+
	  "2. Stisknete Z pro odblokování ovládání lokomotivy.\n"+
	  "3. Stisknete ; a [ pro odbrzdení brzdných systému.\n"+
	  "4. Pomalu zvysujte výkon stiskem D .\n\n"+
	  "Jak zmenit smer\n"+
	  "1. Zastavte vlak.\n"+
	  "2. Presunte paku reverzniho kontroleru do polohy vzad nebo vpred dvojitým stiskem S.\n"+
	  "3. Odbrzdete brzdy stiskem ; (prípadne [ ).\n"+
	  "4. Pomalu zvysujte vykon stiskem D .\n\n"+
	  "Jak pripojit vagony/lokomotivy\n"+
	  "1. K vagonu musíte prijet pomalu, optimální rychlost je okolo 1 km/h.\n"+
	  "Tip: Pro zobrazení pohledu na spráhlo stisknete klávesu 6.\n"+
	  "2. Stisknete F9 pro otevrení okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
	  "3. Jestlize je ikona vozu cervená, je zatazena rucní brzda. Dvojtukem mysí na voze uvolníte/zatáhne rucní brzdu.\n"+
	  "4. Zavrete okno sestavení vlaku stiskem F9.\n"+
	  "5. Pockejte az odbrzdíte pripojené vozy.\n\n"+
	  "Odpojení vozu nebo lokomotivy\n"+
	  "POZOR! Melo by se provádet jen tehdy, pokud VLAK STOJÍ!\n"+
	  "1. Otevrete okno sestavy vlaku F9.\n"+
	  "2. Poklepejte 2x na ikonu vozu, ktery se má odpojit, pokud chcete, aby mel vuz zatazenou rucní brzdu.\n"+
	  "3. Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
	  "4. Pomalu se rozjedte smerem od odpojene casti vlaku.\n"+
	  "(Pozn.: V nekterých prípadech pri rychlejsím odjezdu dojde k opetovnému spojení spráhel. Pokud se toto stane tak soupravu opet rozpojte a velmi pomalu odjízdejte az do vzdálenosti jednoho prazce. Pak jiz muzete zacít zrychlovat.)\n"+
	  "5. Zavrete okno sestavení vlaku stiskem F9.\n\n"
	 ) 
)