SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( Rpool_186-534-4ms
 Type ( Freight )
Name ( "Rpool_186-534-4 Silk Road ms" )
WagonShape ( Rpool_186-534-4.s )
ORTSFreightAnims (
	MSTSFreightAnimEnabled ( 0 )
		FreightAnimStatic ( 
			SubType ( Default )
			Shape ( Rpool_186-534-4_FREIGHT.s )
			Offset ( 0.0, 0.0, 0.0 )
			Flip ( 0 )
			)
		)
Size ( 3.052m 4.186m 18.885m )
CentreOfGravity ( 0m 2.09m 0m )
 Mass ( 84t )
 WheelRadius ( 0.625m )
 ORTSNumberAxles ( 4 )

Comment ( "Sprahla" )
Coupling (
Type ( Chain )
Spring ( Stiffness ( 3.8e6N/m 2.5e8N/m ) Break ( 834kN 834kN ) r0 ( 0cm 1.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Coupling (
Type ( Chain )
Spring ( Stiffness ( 3.8e6N/m 2.5e8N/m ) Break ( 834kN 834kN ) r0 ( 0cm 1.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

ORTSBearingType ( Low )
ORTSDavis_A ( 944.6 )
ORTSDavis_B ( 18.42 )
ORTSDavis_C ( 6.3825 )

ORTSAdhesion (
ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
ORTSSlipWarningThreshold ( 60 )
)

Comment ( "Jizdni odpory a treni" )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 2m 600mm )
ORTSUnbalancedSuperelevation ( 150mm )

Comment ( "Brzdy" )
Comment ( "Brzdovy system Knorr, kotouce, Bv.: 90t" )
Comment ( "Rezim brzdeni P" )
BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

MaxBrakeForce ( 153kN )
MaxHandbrakeForce ( 70kN )
NumberOfHandbrakeLeverSteps ( 10 )

TripleValveRatio ( 2.5 )
MaxReleaseRate ( 0.212bar/s )
MaxApplicationRate ( 0.475bar/s )
MaxAuxilaryChargingRate ( 0.81bar/s )
EmergencyResChargingRate ( 0.81bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 4bar )
EmergencyResVolumeMultiplier ( 2.5 )
EmergencyResCapacity ( 150l )
BrakePipeVolume ( 16.4l )

 Sound ( "..\\..\\common.snd\\sndelok\\lokpor.sms" )
 )
