SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( zssk_750183
Comment ( "Sekce vozidlo" )
Comment ( "Popis fyziky vozu pro OR" )
Comment ( "Bez parniho agregatu, dobalastovano" )
Comment ( "Josef Vogeltanz - 26.07.2018" )
Comment ( "Uprava - 02.03.2021" )

Comment ( "Obecne informace vozu" )
Type ( Engine )
WagonShape ( zssk_750183.s )

Size ( 3.096m 4.605m 16.54m )
Mass ( 74t )
WheelRadius ( 0.5m )
ORTSNumberAxles ( 0 )

ORTSFreightAnims (
MSTSFreightAnimEnabled ( 1 )
FreightAnimStatic (
SubType ( Default )
Shape ( zssk_750183_fg.s )
Offset ( 0.0, 0.0, 0.0 )
Flip ( 0 )
)
)

Comment ( "Sprahla" )
Coupling (
Type ( Chain )
Spring ( Stiffness (  6.7e6N/m 4.4e8N/m ) Break ( 850kN 850kN ) r0 ( 0cm 2.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Coupling (
Type ( Chain )
Spring ( Stiffness (  6.7e6N/m 4.4e8N/m ) Break ( 850kN 850kN ) r0 ( 0cm 2.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Comment ( "Brzdy" )
Comment ( "Brzdovy system DAKO, zdrze, Bv.: 50t" )
Comment ( "Rezim brzdeni P")
BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

MaxBrakeForce ( 121kN )
MaxHandbrakeForce ( 45kN )
NumberOfHandbrakeLeverSteps ( 10 )

TripleValveRatio ( 2.5 )
MaxReleaseRate ( 0.212bar/s )
MaxApplicationRate ( 0.475bar/s )
MaxAuxilaryChargingRate ( 0.528bar/s )
EmergencyResChargingRate ( 0.528bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 4bar )
EmergencyResVolumeMultiplier ( 2.5 )
EmergencyResCapacity ( 230l )
BrakePipeVolume ( 14.5l )

ORTSBrakeShoeFriction (
0   0.310
8   0.238
16  0.193
24  0.168
32  0.152
40  0.140
48  0.131
56  0.123
64  0.116
72  0.109
80  0.105
88  0.101
96  0.098
104 0.096
112 0.094
120 0.093
128 0.092
136 0.092
144 0.092
152 0.092
160 0.092
)

Comment ( "Jizdni odpory a treni" )
CentreOfGravity ( 0m 2.3m  0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 2m 400mm )
ORTSUnbalancedSuperelevation ( 150mm )

ORTSBearingType ( Roller )
ORTSDavis_A ( 987.6 )
ORTSDavis_B ( 24.34 )
ORTSDavis_C ( 6.325 )
ORTSWagonFrontalArea ( 12.1m^2 )

ORTSAdhesion (
ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
ORTSSlipWarningThreshold ( 60 )
)

Comment ( "Nastaveni svetel - CD")
Lights ( 51

Comment ( "Svetelny kuzel dalkovy" )
Light (
Type ( 1 )
Conditions ( Headlight ( 3 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFFFFC4 ) Position ( 0 3.8 7.8 ) Angle ( 15 ) Transition ( 1 ) Radius ( 100 ) )
)
)

Comment ( "Svetelny kuzel tlumeny" )
Light (
Type ( 1 )
Conditions ( Headlight ( 2 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFFFFC4 ) Position ( 0 3.8 7.8 ) Angle ( 35 ) Transition ( 1 ) Radius ( 35 ) )
)
)

Comment ( "Svetelny kuzel navestni" )
Light (
Type ( 1 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFFFC4 ) Position ( 0 0.5 8.3 ) Angle ( 90 ) Transition ( 1 ) Radius ( 3 ) )
)
)

Comment ( "Definice svetel pro predni stanoviste" )
Comment ( "Reflektor dalkovy 1" )
Light (
Type ( 0 )
Conditions ( Headlight ( 3 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFFEA99 ) Position ( 0 3.8 7.83 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.45 ) )
)
)

Comment ( "Reflektor tlumeny 1A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFEA99 ) Position ( 0 3.8 7.83 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.45 ) )
)
)

Comment ( "Reflektor tlumeny 1B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFFFF9E0 ) Position ( 0 3.77 7.8302 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.2 ) )
)
)

Comment ( "Predni leve pozicni A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( 0.64 1.4 7.66 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Predni leve pozicni B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( 0.64 1.37 7.6602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Predni prave pozicni A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( -0.64 1.4 7.66 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Predni prave pozicni B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( -0.64 1.37 7.6602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Predni horni zapnute 1A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFEA99 ) Position ( 0 3.8 7.83 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.45 ) )
)
)

Comment ( "Predni horni zapnute 1B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFFFF9E0 ) Position ( 0 3.77 7.8302 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.2 ) )
)
)

Comment ( "Predni leve zapnute A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( 0.64 1.4 7.66 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Predni leve zapnute B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( 0.64 1.37 7.6602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Predni prave zapnute A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( -0.64 1.4 7.66 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Predni prave zapnute B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( -0.64 1.37 7.6602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Zadni leve pozicni A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( 0.64 1.4 -7.66 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni leve pozicni B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( 0.64 1.37 -7.6602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Zadni prave pozicni A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( -0.64 1.4 -7.66 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni prave pozicni B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( -0.64 1.37 -7.6602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Zadni leve koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( 0.89 1.4 -7.66 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni leve koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( 0.89 1.37 -7.6602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Zadni prave koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( -0.89 1.4 -7.66 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni prave koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( -0.89 1.37 -7.6602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Definice svetel pro zadni stanoviste" )
Comment ( "Reflektor dalkovy 1" )
Light (
Type ( 0 )
Conditions ( Headlight ( 3 ) Unit ( 5 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFFEA99 ) Position ( 0 3.8 -7.83 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.45 ) )
)
)

Comment ( "Reflektor tlumeny 1A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 5 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFEA99 ) Position ( 0 3.8 -7.83 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.45 ) )
)
)

Comment ( "Reflektor tlumeny 1B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 5 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFFFF9E0 ) Position ( 0 3.77 -7.8302 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.2 ) )
)
)

Comment ( "Predni horni zapnute 1A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFEA99 ) Position ( 0 3.8 -7.83 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.45 ) )
)
)

Comment ( "Predni horni zapnute 1B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFFFF9E0 ) Position ( 0 3.77 -7.8302 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.2 ) )
)
)

Comment ( "Predni leve zapnute A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( 0.64 1.4 -7.66 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Predni leve zapnute B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( 0.64 1.37 -7.6602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Predni prave zapnute A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( -0.64 1.4 -7.66 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Predni prave zapnute B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( -0.64 1.37 -7.6602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Zadni leve koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( 0.89 1.4 7.66 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni leve koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( 0.89 1.37 7.6602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Zadni prave koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( -0.89 1.4 7.66 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni prave koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( -0.89 1.37 7.6602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Prave predni pozicni A - Loose consist" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Control ( 0 ) Service ( 1 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( -0.64 1.4 7.66 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Prave predni pozicni B - Loose consist" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Control ( 0 ) Service ( 1 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( -0.64 1.37 7.6602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Leve zadni pozicni A - Loose consist" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Control ( 0 ) Service ( 1 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( 0.64 1.4 -7.66 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Leve zadni pozicni B - Loose consist" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Control ( 0 ) Service ( 1 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( 0.64 1.37 -7.6602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Definice svetel pro loko ovladanou PC" )
Comment ( "PC predni leve A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( 0.64 1.4 7.66 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "PC predni leve B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( 0.64 1.37 7.6602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "PC predni prave A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( -0.64 1.4 7.66 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "PC predni prave B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( -0.64 1.37 7.6602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "PC predni horni 1A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFEA99 ) Position ( 0 3.8 7.83 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.45 ) )
)
)

Comment ( "PC predni horni 1B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFFFF9E0 ) Position ( 0 3.77 7.8302 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.2 ) )
)
)

Comment ( "PC zadni leve koncove A" )
Light (
Type ( 0 )
Conditions ( Unit ( 3 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( 0.89 1.4 -7.66 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "PC zadni leve koncove B" )
Light (
Type ( 0 )
Conditions ( Unit ( 3 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( 0.89 1.37 -7.6602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "PC zadni prave koncove A" )
Light (
Type ( 0 )
Conditions ( Unit ( 3 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( -0.89 1.4 -7.66 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "PC zadni prave koncove B" )
Light (
Type ( 0 )
Conditions ( Unit ( 3 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( -0.89 1.37 -7.6602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)
)

ORTS3DCab (
ORTS3DCabFile ( "..//..//common.cab//3DCab750//cab750.s" )
ORTS3DCabHeadPos ( 0.76 3.1 6.1 )
RotationLimit ( 40 60 0 )
StartDirection ( 12 0 0 )
)

ORTS3DCab (
ORTS3DCabFile ( "..//..//common.cab//3DCab750//cab750.s" )
ORTS3DCabHeadPos ( -0.76 3.1 -6.1 )
RotationLimit ( 40 60 0 )
StartDirection ( 12 180 0 )
)

Comment ( "Ostatni informace" )
Sound ( "..//..//common.snd//snd754//750eng.sms" )
IntakePoint ( 0 2 FuelDiesel )
)

Engine ( zssk_750183
Comment ( "Sekce pohon" )
Comment ( "Motor CKD K12V230DR, trakcni generator CKD TD 802E, trakcni motory CKD TE 005E" )
Wagon ( zssk_750183 )
Name ( "ZSSK 750 183-6 2019" )

Comment ( "Projevy pohonu" )
Effects (
DieselSpecialEffects (
Exhaust1 ( -0.23 4.63 2.23 0 1 0 0.2 )
Exhaust2 ( 0.23 4.63 2.23 0 1 0 0.2 )
)
)

Comment ( "Obecne informace pohonu" )
Type ( Diesel )
MaxVelocity ( 100km/h )
WheelRadius ( 0.5m )
Sanding ( 35km/h )
ORTSNumberDriveAxles ( 4 )
ORTSDriveWheelWeight ( 76.8t )
ORTSSpeedOfMaxContinuousForce ( 30km/h )
MaxForce ( 185kN )
MaxContinuousForce ( 128kN )
MaxPower ( 1020kW )
MaxDieselLevel ( 2500l )
DieselEngineType ( electric )
MaxCurrent ( 2400A )

Comment ( "Agregat" )
ORTSDieselEngines ( 1
Diesel (
IdleRPM ( 480 )
MaxRPM ( 1100 )
StartingRPM ( 321 )
StartingConfirmRPM ( 528 )
ChangeUpRPMpS ( 100 )
ChangeDownRPMpS ( 75 )
RateOfChangeUpRPMpSS ( 10 )
RateOfChangeDownRPMpSS ( 10 )
MaximalPower ( 1325kW )
IdleExhaust ( 4 )
MaxExhaust ( 11 )
ExhaustDynamics ( 1.2 )
ExhaustDynamicsDown ( 0.5 )
ExhaustColor ( 00999792 )
ExhaustTransientColor ( FF5B5851 )
DieselPowerTab (
0 0
480 79500
500 132500
530 218625
600 397500
700 632688
810 871188
910 1036813
1000 1185875
1100 1325000
)
DieselConsumptionTab (
0 0
480 31.5
500 57.7
530 78.7
600 98
700 122.5
810 157.5
910 224.1
1000 280.1
1100 350.1
)
ThrottleRPMTab (
0 480
3 500
8 530
19 600
35 700
53 810
69 910
84 1000
100 1100
)
DieselTorqueTab (
0 0
480 7338
1100 8783
)
MinOilPressure ( 200kPa )
MaxOilPressure ( 600kPa )
MaxTemperature ( 85 )
Cooling ( 3 )
TempTimeConstant ( 720 )
OptTemperature ( 70 )
IdleTemperature ( 60 )
)
)

ORTSContinuousForceTimeFactor ( 3600 )
ORTSMaxTractiveForceCurves (
0 ( 0.0 0 27.8 0 )
0.03 ( 0.0 40000  1.4 23500  2.8 15000  4.2 7000   5.6 2000   6.9 2000   8.3 2000   9.7 2000   11.1 2000  12.5 2000  13.9 2000  15.3 2000  16.7 2000  18.1 2000  19.4 2000  20.8 2000  22.2 2000  23.6 2000  25.0 2000  26.4 2000  27.8 2000 )
0.08 ( 0.0 77000  1.4 50000  2.8 35000  4.2 24000  5.6 16000  6.9 10000  8.3 5000   9.7 5000   11.1 5000  12.5 5000  13.9 5000  15.3 5000  16.7 5000  18.1 5000  19.4 5000  20.8 5000  22.2 5000  23.6 5000  25.0 5000  26.4 5000  27.8 5000 )
0.20 ( 0.0 168000 1.4 114000 2.8 74000  4.2 50000  5.6 38000  6.9 27000  8.3 19000  9.7 14000  11.1 11000 12.5 8000  13.9 6000  15.3 4000  16.7 4000  18.1 4000  19.4 4000  20.8 4000  22.2 4000  23.6 4000  25.0 4000  26.4 4000  27.8 4000 )
0.35 ( 0.0 185000 1.4 149000 2.8 108000 4.2 80000  5.6 62000  6.9 50000  8.3 40000  9.7 33000  11.1 27500 12.5 23000 13.9 20000 15.3 17000 16.7 14500 18.1 13000 19.4 11000 20.8 9500  22.2 9000  23.6 8000  25.0 7500  26.4 7000  27.8 7000 )
0.53 ( 0.0 163000 1.4 163000 2.8 140000 4.2 109000 5.6 87000  6.9 70000  8.3 58000  9.7 50000  11.1 43000 12.5 38000 13.9 33500 15.3 30000 16.7 27500 18.1 25000 19.4 23000 20.8 21500 22.2 19500 23.6 18000 25.0 17000 26.4 16000 27.8 15000 )
0.70 ( 0.0 153000 1.4 153000 2.8 153000 4.2 153000 5.6 116000 6.9 98000  8.3 84000  9.7 72000  11.1 64000 12.5 56000 13.9 50000 15.3 45000 16.7 41000 18.1 37000 19.4 34500 20.8 32000 22.2 30000 23.6 28000 25.0 26500 26.4 25000 27.8 23500 )
0.84 ( 0.0 130000 1.4 130000 2.8 130000 4.2 130000 5.6 130000 6.9 115000 8.3 99500  9.7 88500  11.1 78500 12.5 70000 13.9 63500 15.3 57500 16.7 53000 18.1 48000 19.4 45000 20.8 41500 22.2 38500 23.6 36500 25.0 34000 26.4 32500 27.8 31000 )
1.00 ( 0.0 122000 1.4 122000 2.8 122000 4.2 122000 5.6 122000 6.9 122000 8.3 117000 9.7 103000 11.1 93000 12.5 85000 13.9 78000 15.3 71000 16.7 65000 18.1 60000 19.4 56000 20.8 51500 22.2 48500 23.6 46000 25.0 43000 26.4 41500 27.8 40000 )
)

Comment ( "Brzdy" )
Comment ( "Brzdovy system DAKO, brzdice DAKO BS2, DAKO BP, kompresor K3 lok-1" )
Comment ( "Brzdeni I.zpusob, rezim brzdeni P")
BrakesTrainBrakeType ( "Air_single_pipe" )
BrakesEngineControllers ( "Independent, Train" )

ORTSMainResChargingRate ( 0.07bar/s )
ORTSBrakePipeChargingRate ( 20.7bar/s )
ORTSTrainBrakesControllerMaxOverchargePressure ( 5.4bar )
ORTSTrainBrakesControllerOverchargeEliminationRate ( 0.0023bar/s )	

AirBrakesMainMaxAirPressure ( 10bar )
AirBrakesMainResVolume ( 1m^3 )
AirBrakesCompressorRestartPressure ( 8.5bar )
TrainPipeLeakRate ( 0.0042bar/s )

ORTSEngineBrakeReleaseRate ( 1.0bar/s )
ORTSEngineBrakeApplicationRate ( 1.33bar/s )
EngineBrakesControllerMinPressureReduction ( 0.3bar )
EngineBrakesControllerFullServicePressureDrop ( 1.0bar )
EngineBrakesControllerMaxApplicationRate ( 1.33bar/s )
EngineBrakesControllerMaxReleaseRate ( 1.0bar/s )
EngineBrakesControllerMaxSystemPressure ( 5bar )

TrainBrakesControllerMinPressureReduction ( 0.3bar )
TrainBrakesControllerFullServicePressureDrop ( 1.5bar )
TrainBrakesControllerMaxApplicationRate ( 0.67bar/s )
TrainBrakesControllerMaxReleaseRate ( 0.67bar/s )
TrainBrakesControllerMaxQuickReleaseRate ( 2.0bar/s )
TrainBrakesControllerEmergencyApplicationRate ( 1.86bar/s )
TrainBrakesControllerMaxSystemPressure ( 5bar )

ORTSBrakePipeTimeFactor ( 0.003 )
ORTSBrakeServiceTimeFactor ( 1.009 )
ORTSBrakeEmergencyTimeFactor ( 0.1 )

Comment ( "Ovladani jizdy" )

Comment ( "Vlakovy zabezpecovac - pouze KBS" )
VigilanceMonitor (
MonitoringDeviceMonitorTimeLimit ( 16 )
MonitoringDeviceAlarmTimeLimit ( 6 )
MonitoringDevicePenaltyTimeLimit ( 0 )
MonitoringDeviceCriticalLevel ( 0 )
MonitoringDeviceResetLevel ( 0 )
MonitoringDeviceAppliesFullBrake ( 0 )
MonitoringDeviceAppliesEmergencyBrake ( 1 )
MonitoringDeviceAppliesCutsPower ( 1 )
MonitoringDeviceAppliesShutsDownEngine ( 0 )
MonitoringDeviceResetOnResetButton ( 1 )
MonitoringDeviceResetOnZeroSpeed ( 1 )
)

Comment ( "Rizeni" )

EngineControllers (
Throttle ( 0 1 0.125 0
NumNotches ( 9
Notch ( 0 0 Dummy )
Notch ( 0.03 0 Dummy )
Notch ( 0.08 0 Dummy )
Notch ( 0.19 0 Dummy )
Notch ( 0.35 0 Dummy )
Notch ( 0.53 0 Dummy )
Notch ( 0.69 0 Dummy )
Notch ( 0.84 0 Dummy )
Notch ( 1.00 0 Dummy )
)
)

Comment ( "Primocinna brzda typu DAKO BP" )
Brake_Engine ( 0 1 0.1 0.8
NumNotches  ( 1 
Notch ( 0 1 Dummy ) )
)

Comment ( "Prubezna brzda typ DAKO-BS2" )
Brake_Train ( 0 1 0.04 0.21
NumNotches ( 8
Notch ( 0 0 TrainBrakesControllerFullQuickReleaseStart )
Notch ( 0.02 0 TrainBrakesControllerOverchargeStart )
Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
Notch ( 0.95 0 TrainBrakesControllerNeutralhandleOffStart )
Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
)
)

Brake_Hand ( 0 1 0.025 0
NumNotches ( 0 )
)

DirControl ( -1 0 1 1 )
Sanding ( 0 1 0 )
Horn ( 0 1 0 )
Wipers ( 0 1 0 )
EmergencyStopToggle ( 0 1 1 )
Vigilance ( 0 1 0 )
Headlights ( 0 0.25 1 0 )
)

Comment ( "Ostatni informace" )
Sound ( "..//..//common.snd//snd754//750cab.sms" )
CabView ( "..//..//common.cab//3DCab750//cab750.cvf" )
HeadOut ( 1.7 3.2 6.45 )

Comment ( "Poznamky" )
Description (
"Pokyny pro obecne nastaveni OR:\n"+
"-> Karta Obecne: Rychlost plneni brzdoveho potrubi 1000 PSI/s (nutne aby OR akceptoval hodnoty engu!)\n"+
"-> Karta Simulace: Pokrocily model adheze\n"+
"-> Karta Experimentalni: Faktor korekce adheze 100%\n"+
"-> Karta Experimentalni: Nahodna zmena faktoru adheze 10%\n\n"+ 
"Rada 750 CD je dieselelektricka skrinova lokomotiva, pouzivana dnes uz vetsinou jen v nakladni doprave.\n\n"+
"Lokomotivy vznikly jako rekonstrukce rady 753 nahrazenim parniho generatoru topnym alternatorem.\n\n"+
"Prenos vykonu: elektricky\n\n"+
"Zdroj vykonu: naftovy motor CKD K 12 V 230 DR\n\n"+
"Max. vykon motoru: 1325 kW\n\n"+
"Max. trakcni vykon: 1200 kW\n\n"+
"Max. vyska: 4,335 m\n\n"+
"Max. sirka: 3,074 m\n\n"+
"Delka pres narazniky: 16,540 m\n\n"+
"Hmotnost: 76,8 t\n\n"+
"Max. rychlost: 100 km/h"
)

EngineOperatingProcedures (
"Viz. manual Open Rails.\n\n"+
"TIP: V prubehu jizdy pomoc na klavese F1."
)
)