SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( 141-045 
Comment ( "Sekce vozidlo" )
Comment ( "Popis fyziky vozu pro OR" )
Comment ( "Nastavení pro OR Josef Vogeltanz, vykon a TCh Acatus 1/2021" )

Comment ( "Obecne informace vozu" )
Type ( Engine )
WagonShape ( 141-045.s )
Size ( 3.15m 4.71m 16.18m )
Mass ( 84t )
WheelRadius ( 0.625m )
InertiaTensor ( Box ( 3.15m 4.71m 15.88m ) )

ORTSFreightAnims (
MSTSFreightAnimEnabled ( 0 )
FreightAnimStatic (
SubType( Default )
Shape( strojv.s )
Offset( 0.0, 0.0, 0.0 )
)
)

Comment ( "Sprahla" )
Coupling (
Type ( Chain )
Spring ( Stiffness (  6.7e6N/m 4.4e8N/m) Break ( 850kN 850kN ) r0 ( 0cm 1.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Coupling (
Type ( Chain )
Spring ( Stiffness (  6.7e6N/m 4.4e8N/m) Break ( 850kN 850kN ) r0 ( 0cm 1.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )	

Comment ( "Brzdy" )
Comment ( "Brzdovy system DAKO, zdrze, Bv.P: 51t" )
Comment ( "Rezim brzdeni P")
BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

MaxBrakeForce( 155kN )
MaxHandbrakeForce( 51kN )
NumberOfHandbrakeLeverSteps( 100 )

TripleValveRatio ( 2.5 )
MaxReleaseRate ( 0.212bar/s )
MaxApplicationRate ( 0.475bar/s )
MaxAuxilaryChargingRate ( 0.506bar/s )
EmergencyResChargingRate ( 0.506bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 4bar )
EmergencyResVolumeMultiplier ( 1.0 )
EmergencyResCapacity ( 240l )
BrakePipeVolume ( 14.2l )

ORTSBrakeShoeFriction ( 0 0.31 1 0.30 2 0.28 3 0.27 4 0.26 5 0.25 7 0.24 8 0.23 9 0.22 12 0.21 14 0.20 17 0.19 20 0.18 24 0.17 29 0.16 34 0.15 40 0.14 47 0.13 55 0.12 66 0.11 84 0.10 115 0.09 160 0.09 )

Comment ( "Jizdni odpory a treni" )
CentreOfGravity ( 0.0m 2.35m 0.0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 3m 330mm )
ORTSUnbalancedSuperelevation ( 150mm )

ORTSAdhesion (
ORTSCurtius_Kniffler ( 6.1 44 0.161 0.7 )
ORTSSlipWarningThreshold ( 70 )
)

ORTSBearingType ( Roller )
ORTSDavis_A ( 1051.3 )
ORTSDavis_B ( 27.64 )
ORTSDavis_C ( 6.3825 )
NumWheels ( 4 )

Comment ( "Pantografy" )
ORTSPantographs (
Pantograph (
Delay ( 3s )
)
Pantograph (
Delay ( 3s )
)
)

Comment ( "Svetla" )
Lights ( 32

Light (
comment ( Svetelny kuzel dalkovy )
Type ( 1 )
Conditions ( Headlight ( 3 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 1 )
FadeOut ( 1 )
Cycle ( 0 )
States ( 1
State (
Duration ( 0 ) LightColour ( FFFFC085 ) Position ( 0.0 3 3 ) Angle ( 10 ) Transition ( 1 ) Radius ( 300 ) )
)
)

Light (
comment ( Svetelny kuzel tlumeny )
Type ( 1 )
Conditions ( Headlight ( 2 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FF444444 ) Position ( 0.0 3 3 ) Angle ( 30 ) Transition ( 1 ) Radius ( 150 ) )
)
)

comment ( Definice svetel pro prední stanoviste )
Light (
comment ( reflektor tlumeny )
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 1.0 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0.0 ) LightColour ( 80EED15D ) Position ( 0.0 3.58 7.42 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0.6 ) )
)
)

Light (
comment ( reflektor dalkovy )
Type ( 0 )
Conditions ( Headlight ( 3 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 1.0 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0.0 ) LightColour ( EEEED15D ) Position ( 0.0 3.58 7.42 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0.6 ) )
)
)

Light (
comment ( Prední levé pozicní )
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0.0 ) LightColour ( 60EED15D ) Position ( -0.89 1.53 7.46 ) Azimuth ( 0.0 0.0 0.0 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( Prední pravé pozicní )
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0.0 ) LightColour ( 60EED15D ) Position ( 0.89 1.53 7.46 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( prední levé zapnuté )
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0.0 ) LightColour ( C0EED15D ) Position ( -0.89 1.53 7.46 ) Azimuth ( 0.0 0.0 0.0 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( prední pravé zapnuté )
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1 State ( Duration ( 0.0 ) LightColour ( C0EED15D ) Position ( 0.89 1.53 7.46 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( zadní levé pozicní )
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0.0 ) LightColour ( 60EED15D ) Position ( -0.89 1.53 -7.46 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( zadní pravé pozicní )
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1 State ( Duration ( 0.0 ) LightColour ( 60EED15D ) Position ( 0.89 1.53 -7.46 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( zadní levé koncové )
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 3 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0.0 ) LightColour ( 80ff0000 ) Position ( -0.89 1.53 -7.46 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( zadní pravé koncové )
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 3 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0.0 ) LightColour ( 80ff0000 ) Position ( 0.89 1.53 -7.46 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

comment ( Definice svetel pro zadní stanoviste )
Light (
comment ( reflektor dalkovy )
Type ( 0 ) 
Conditions ( Headlight ( 3 ) Unit ( 5 ) Control ( 2 ) )
FadeIn ( 2 )
FadeOut ( 2 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( fffad09f ) Position ( 0.0 3.58 -7.42 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
)
)

Light (
comment ( reflektor tlumeny )
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 1.0 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0.0 ) LightColour ( 80EED15D ) Position ( 0.0 3.58 7.42 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0.6 ) )
)
)

Light (
comment ( Prední levé pozicní )
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( 60EED15D ) Position ( -0.89 1.53 -7.46 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( Prední pravé pozicní )
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( 60EED15D ) Position ( 0.89 1.53 -7.46 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( prední levé zapnuté )
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( C0EED15D ) Position ( -0.89 1.53 -7.46 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( prední pravé zapnuté )
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( C0EED15D ) Position ( 0.89 1.53 -7.46 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( zadní levé pozicní )
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( 60EED15D ) Position ( -0.89 1.53 7.46 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( zadní pravé pozicní )
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( 60EED15D ) Position ( 0.89 1.53 7.46 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( zadní levé koncové )
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 4 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFF0000 ) Position ( -0.89 1.53 7.46 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( zadní pravé koncové )
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 4 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFF0000 ) Position ( 0.89 1.53 7.46 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

comment ( Definice svetel pro Loose consist )
Light	(
comment( Levé prední pozicní - Loose consist )
Type ( 0 )
Conditions ( Headlight ( 0 ) Control ( 0 ) Service ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle	( 0 )
States ( 1
State	( Duration ( 0.0 ) LightColour ( 60EED15D ) Position ( -0.89 1.53 7.46 ) Azimuth ( 0.0 0.0 0.0 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light	(
comment( Pravé prední pozicní - Loose consist )
Type ( 0 )
Conditions ( Headlight ( 0 ) Control ( 0 ) Service ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle	( 0 )
States ( 1
State	( Duration ( 0.0 ) LightColour ( 60EED15D ) Position ( 0.89 1.53 7.46 ) Azimuth ( 0.0 0.0 0.0 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light	(
comment( Levé zadní pozicní - Loose consist)
Type ( 0 )
Conditions ( Headlight ( 0 ) Control ( 0 ) Service ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle	( 0 )
States ( 1
State	( Duration ( 0.0 ) LightColour ( 60EED15D ) Position ( -0.89 1.53 -7.46 ) Azimuth ( -180 -180 -180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light	(
comment( Pravé zadní pozicní - Loose consist)
Type ( 0 )
Conditions ( Headlight ( 0 ) Control ( 0 ) Service ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle	( 0 )
States ( 1
State	( Duration ( 0.0 ) LightColour ( 60EED15D ) Position ( 0.89 1.53 -7.46 ) Azimuth ( -180 -180 -180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

comment ( Definice svetel pro loko ovládanou PC )
Light (
comment ( PC prední pravé )
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) )
FadeIn ( 1 )
FadeOut ( 1 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( 60EED15D ) Position ( 0.89 1.53 7.46 ) Azimuth ( 0 -5 5 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( PC prední levé )
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) )
FadeIn ( 1 )
FadeOut ( 1 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( 60EED15D ) Position ( -0.89 1.53 7.46 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( PC reflektor prední 1 )
Conditions ( Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( fffad09f ) Position ( 0.0 3.58 7.42 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0.6 ) )
)
)

Light (
comment ( PC zadní levé koncové )
Type ( 0 )
Conditions ( Unit ( 3 ) Control ( 1 ) Service ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFF0000 ) Position ( -0.89 1.53 -7.46 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

Light (
comment ( PC zadní pravé koncové )
Type ( 0 )
Conditions ( Unit ( 3 ) Control ( 1 ) Service ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
Cycle ( 0 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFF0000 ) Position ( 0.89 1.53 -7.46 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Radius ( 0.4 ) )
)
)

comment( *** zablesky na smykadle *** )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Service ( 2 ) )
FadeIn ( 0 )
FadeOut ( 0 )
Cycle ( 0 )
States ( 16
State ( Duration ( 0.03 ) LightColour ( ff0000ff ) Position ( 0 5.50 -4.22 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 3 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.04 ) LightColour ( ff87cefa ) Position ( -0.05 5.50 -4.22 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 7.6 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.1 ) LightColour ( ff87cefa ) Position ( 0.025 5.50 -4.22 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 8.3 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.04 ) LightColour ( ff87cefa ) Position ( 0 5.50 -4.22 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 0.05 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.05 ) LightColour ( ff0000ff ) Position ( -0.01 5.50 -4.22 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 9 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.07 ) LightColour ( ff0000ff ) Position ( -0.05 5.50 -4.22 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 12 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.05 ) LightColour ( ff87cefa ) Position ( 0.01 5.50 -4.22 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 0.1 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.03 ) LightColour ( ff0000ff ) Position ( -0.01 5.50 -4.22 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 13 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
)
)
)

Comment ( "Ostatní informace" )
Sound ( "..//..//common.snd//sndElok//141eng.sms" )
)

Engine ( 141-045
Comment ( "Sekce pohon" )
Comment ( "Obecne informace pohonu" )

Wagon ( 141-045 )

Comment ( "Pohon" )
Type ( Electric ) 
MaxVelocity ( 120km/h )
WheelRadius ( 0.625m )
Sanding ( 10km/h )
NumWheels ( 4 )
ORTSDriveWheelWeight ( 84t )
MaxForce ( 525kN )
MaxContinuousForce ( 520kN )
AntiSlip ( 1 )
MaxPower ( 2344kW )
MaxCurrent ( 1440A )

ORTSCircuitBreaker ( Manual )
ORTSCircuitBreakerClosingDelay ( 2s )
ORTSPowerOnDelay ( 5s )

comment ( doplneni trakcni charakteristiky a prislusne úpravy trakce - Acatus 1/2021 )
    comment ( 0    X     1     2     3     4     5     6     7      8     9   10   11    12    13    14    15    16    17    18    19    20    21    22    23   24-S    SI   SII  SIII   SIV     A     B     C   25    26    27    28    29    30    31    32    33    PI   PII  PIII   PIV    PV   PVI ) 
ORTSContinuousForceTimeFactor ( 1800 )
ORTSTractionCharacteristics ( 26 49
Throttle ( 0.00  0.04  0.05  0.07  0.09  0.11  0.13  0.14  0.15  0.16  0.17 0.18  0.19  0.20  0.21  0.22  0.23  0.24  0.25  0.26  0.27  0.28  0.29  0.30  0.31  0.32  0.33  0.35  0.37  0.39  0.41  0.44  0.47  0.50  0.52  0.54  0.56  0.58  0.60  0.63  0.67  0.71  0.75  0.80  0.85  0.90  0.95  1.00 ) 
 table ( 
  0.0km/h 0.0kN 0.0kN  33kN  54kN  75kN  95kN 119kN 134kN 158kN 181kN 199kN 215kN 244kN 277kN 420kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN
  5.0km/h 0.0kN 0.0kN  29kN  46kN  62kN  78kN  96kN 108kN 124kN 144kN 155kN 172kN 190kN 210kN 232kN 275kN 290kN 315kN 380kN 450kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN
 10.0km/h 0.0kN 0.0kN  26kN  39kN  52kN  64kN  78kN  90kN 102kN 113kN 123kN 137kN 153kN 173kN 197kN 218kN 238kN 262kN 290kN 308kN 350kN 430kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN
 15.0km/h 0.0kN 0.0kN  23kN  34kN  43kN  53kN  63kN  71kN  79kN  87kN  95kN 103kN 115kN 128kN 147kN 164kN 179kN 198kN 225kN 257kN 280kN 350kN 430kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN
 20.0km/h 0.0kN 0.0kN  20kN  29kN  37kN  44kN  51kN  57kN  64kN  69kN  73kN  78kN  87kN  95kN 107kN 116kN 125kN 137kN 158kN 184kN 204kN 219kN 258kN 292kN 330kN 400kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN
 25.0km/h 0.0kN 0.0kN  18kN  25kN  31kN  35kN  39kN  43kN  47kN  50kN  54kN  57kN  66kN  72kN  78kN  83kN  90kN  95kN 104kN 117kN 127kN 147kN 170kN 195kN 215kN 240kN 260kN 280kN 290kN 308kN 290kN 240kN 220kN 210kN 260kN 350kN 480kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN
 30.0km/h 0.0kN 0.0kN  16kN  22kN  26kN  29kN  32kN  35kN  40kN  42kN  45kN  48kN  51kN  55kN  58kN  62kN  67kN  71kN  76kN  83kN  89kN  95kN 103kN 111kN 120kN 133kN 153kN 175kN 200kN 234kN 220kN 210kN 200kN 197kN 231kN 271kN 286kN 305kN 350kN 400kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN
 35.0km/h 0.0kN 0.0kN  13kN  18kN  22kN  24kN  26kN  27kN  29kN  31kN  33kN  36kN  37kN  39kN  42kN  44kN  47kN  49kN  52kN  55kN  59kN  62kN  64kN  67kN  71kN  84kN  95kN 110kN 135kN 171kN 165kN 160kN 160kN 166kN 196kN 230kN 247kN 280kN 320kN 390kN 480kN 500kN 500kN 500kN 500kN 500kN 500kN 500kN
 40.0km/h 0.0kN 0.0kN  12kN  17kN  18kN  21kN  22kN  23kN  25kN  27kN  28kN  29kN  31kN  32kN  33kN  34kN  36kN  37kN  39kN  41kN  43kN  46kN  49kN  51kN  54kN  62kN  72kN  91kN 100kN 130kN 132kN 135kN 137kN 139kN 162kN 195kN 208kN 235kN 280kN 308kN 340kN 400kN 500kN 500kN 500kN 500kN 500kN 500kN
 45.0km/h 0.0kN 0.0kN  10kN  15kN  17kN  18kN  19kN  19kN  20kN  21kN  22kN  23kN  24kN  25kN  26kN  27kN  28kN  30kN  31kN  33kN  35kN  37kN  39kN  41kN  43kN  45kN  56kN  63kN  75kN 100kN 105kN 107kN 110kN 114kN 133kN 160kN 170kN 195kN 232kN 269kN 300kN 345kN 400kN 500kN 500kN 500kN 500kN 500kN
 50.0km/h 0.0kN 0.0kN   9kN  11kN  13kN  14kN  15kN  15kN  16kN  17kN  18kN  19kN  20kN  21kN  22kN  22kN  23kN  24kN  25kN  26kN  27kN  28kN  39kN  29kN  30kN  32kN  46kN  58kN  56kN  77kN  47kN  48kN  50kN  88kN  90kN 125kN 134kN 152kN 186kN 215kN 248kN 280kN 290kN 300kN 311kN 323kN 335kN 350kN
 55.0km/h 0.0kN 0.0kN   8kN  11kN  12kN  13kN  13kN  13kN  14kN  15kN  16kN  16kN  17kN  18kN  18kN  19kN  19kN  20kN  20kN  21kN  21kN  22kN  23kN  24kN  25kN  26kN  37kN  48kN  45kN  60kN  72kN  73kN  74kN  80kN  90kN 100kN 107kN 117kN 137kN 159kN 187kN 212kN 231kN 250kN 260kN 269kN 277kN 285kN  
 60.0km/h 0.0kN 0.0kN   6kN   9kN  10kN  10kN  11kN  11kN  11kN  12kN  12kN  12kN  13kN  14kN  15kN  15kN  16kN  16kN  17kN  17kN  18kN  18kN  19kN  19kN  20kN  21kN  31kN  41kN  39kN  52kN  55kN  58kN  64kN  70kN  77kN  85kN  91kN  97kN 114kN 131kN 138kN 160kN 178kN 200kN 214kN 223kN 231kN 242kN 
 65.0km/h 0.0kN 0.0kN   6kN   7kN   8kN   8kN   9kN   9kN   9kN  10kN  10kN  10kN  11kN  11kN  11kN  12kN  12kN  12kN  13kN  14kN  15kN  15kN  16kN  16kN  17kN  18kN  22kN  27kN  33kN  44kN  53kN  54kN  55kN  60kN  66kN  73kN  76kN  83kN  89kN  98kN 106kN 115kN 131kN 152kN 174kN 187kN 198kN 208kN   
 70.0km/h 0.0kN 0.0kN   5kN   6kN   6kN   8kN   8kN   7kN   8kN   9kN   8kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  14kN  14kN  14kN  14kN  22kN  28kN  30kN  39kN  44kN  42kN  40kN  53kN  57kN  61kN  64kN  71kN  74kN  80kN  86kN  91kN 101kN 117kN 135kN 150kN 165kN 180kN   
 75.0km/h 0.0kN 0.0kN   4kN   5kN   5kN   7kN   8kN   7kN   7kN   8kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  10kN  11kN  11kN  11kN  12kN  12kN  12kN  18kN  26kN  26kN  34kN  37kN  40kN  43kN  46kN  50kN  53kN  55kN  62kN  64kN  69kN  72kN  75kN  84kN  96kN 109kN 123kN 138kN 156kN  
 80.0km/h 0.0kN 0.0kN   4kN   6kN   7kN   7kN   7kN   7kN   7kN   8kN   7kN   7kN   7kN   8kN   8kN   8kN   9kN   9kN   9kN   9kN   9kN  10kN  10kN  10kN  10kN  11kN  12kN  16kN  21kN  30kN  33kN  36kN  39kN  42kN  44kN  47kN  50kN  56kN  57kN  59kN  61kN  64kN  74kN  84kN  94kN 104kN 114kN 130kN  
 85.0km/h 0.0kN 0.0kN   3kN   5kN   6kN   7kN   7kN   6kN   7kN   7kN   7kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN   9kN   9kN   9kN   9kN   9kN   9kN   9kN   9kN  10kN  12kN  13kN  18kN  24kN  30kN  37kN  39kN  41kN  43kN  49kN  52kN  55kN  57kN  56kN  66kN  76kN  86kN  96kN 106kN 116kN   
 90.0km/h 0.0kN 0.0kN   3kN   4kN   5kN   5kN   6kN   6kN   6kN   7kN   7kN   7kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN   9kN   9kN   9kN   9kN   9kN   9kN   9kN   9kN  11kN  11kN  16kN  21kN  26kN  33kN  34kN  36kN  37kN  44kN  49kN  51kN  53kN  54kN  63kN  73kN  83kN  93kN 103kN 113kN   
 95.0km/h 0.0kN 0.0kN   3kN   4kN   4kN   5kN   6kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   7kN   7kN   8kN   8kN   8kN   8kN   8kN   9kN   8kN   8kN   8kN   8kN   8kN   9kN  10kN  10kN  15kN  20kN  25kN  30kN  32kN  34kN  36kN  42kN  45kN  48kN  50kN  52kN  58kN  66kN  75kN  85kN  94kN 104kN  
100.0km/h 0.0kN 0.0kN   3kN   3kN   4kN   4kN   5kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   7kN   7kN   8kN   8kN   8kN   8kN   8kN   8kN   8kN   8kN   8kN   8kN   8kN   9kN  10kN  15kN  19kN  22kN  27kN  29kN  30kN  35kN  40kN  43kN  45kN  48kN  50kN  55kN  63kN  72kN  82kN  91kN  99kN   
105.0km/h 0.0kN 0.0kN   2kN   3kN   4kN   4kN   5kN   5kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   7kN   7kN   7kN   8kN   7kN   8kN   8kN   8kN   8kN   8kN   8kN   8kN   9kN   9kN  14kN  18kN  21kN  26kN  27kN  28kN  31kN  38kN  40kN  43kN  45kN  47kN  53kN  61kN  70kN  80kN  90kN  97kN   
110.0km/h 0.0kN 0.0kN   2kN   3kN   3kN   4kN   4kN   5kN   5kN   5kN   6kN   6kN   6kN   7kN   7kN   7kN   7kN   7kN   7kN   7kN   7kN   8kN   8kN   8kN   8kN   8kN   8kN   8kN   9kN   9kN  12kN  17kN  20kN  24kN  25kN  26kN  29kN  35kN  38kN  40kN  42kN  44kN  51kN  59kN  67kN  76kN  88kN  95kN   
115.0km/h 0.0kN 0.0kN   2kN   3kN   3kN   3kN   4kN   4kN   5kN   5kN   5kN   6kN   6kN   6kN   7kN   7kN   7kN   7kN   7kN   7kN   7kN   7kN   8kN   8kN   8kN   8kN   8kN   8kN   9kN   9kN  12kN  16kN  19kN  22kN  23kN  24kN  27kN  30kN  34kN  36kN  39kN  41kN  49kN  57kN  65kN  74kN  85kN  91kN   
120.0km/h 0.0kN 0.0kN   2kN   2kN   3kN   3kN   3kN   4kN   4kN   5kN   5kN   5kN   6kN   6kN   6kN   7kN   7kN   7kN   7kN   7kN   7kN   7kN   7kN   8kN   8kN   8kN   8kN   8kN   8kN   9kN  11kN  14kN  17kN  20kN  21kN  22kN  26kN  28kN  30kN  31kN  37kN  39kN  45kN  55kN  63kN  72kN  82kN  90kN   
125.0km/h 0.0kN 0.0kN   1kN   2kN   2kN   3kN   3kN   3kN   4kN   4kN   5kN   5kN   6kN   6kN   6kN   6kN   6kN   7kN   7kN   7kN   7kN   7kN   7kN   7kN   8kN   8kN   8kN   8kN   8kN   8kN  10kN  12kN  15kN  17kN  18kN  19kN  24kN  25kN  26kN  28kN  33kN  35kN  43kN  54kN  62kN  71kN  81kN  91kN      
 ) 
 )

Comment ( "Brzdy" )
Comment ( "Brzdic DAKO-BP a DAKO-BS2, kompresor K1" )
Comment ( "Brzdeni I.zpusob, rezim brzdeni P")

ORTSMainResChargingRate ( 0.08bar/s )
ORTSBrakePipeChargingRate ( 20.7bar/s )
AirBrakesMainMinResAirPressure ( 5bar )
AirBrakesMainMaxAirPressure ( 8bar )
AirBrakesMainResVolume ( 0.9m^3 )
AirBrakesAirCompressorWattage ( 35000 )
AirBrakesCompressorRestartPressure ( 6.5bar )
AirBrakesIsCompressorElectricOrMechanical ( 0 )
TrainPipeLeakRate ( 0.0042bar/s )

ORTSEngineBrakeReleaseRate ( 1.0bar/s )
ORTSEngineBrakeApplicationRate ( 1.3bar/s )
EngineBrakesControllerMinPressureReduction ( 0.3bar )
EngineBrakesControllerFullServicePressureDrop ( 1.0bar )
EngineBrakesControllerMaxApplicationRate ( 1.33bar/s )
EngineBrakesControllerMaxReleaseRate ( 1.0bar/s )
EngineBrakesControllerMaxSystemPressure ( 5bar )

TrainBrakesControllerMinPressureReduction ( 0.3bar )
TrainBrakesControllerFullServicePressureDrop ( 1.5bar )
TrainBrakesControllerMaxReleaseRate ( 0.67bar/s )
TrainBrakesControllerMaxApplicationRate ( 0.67bar/s )
TrainBrakesControllerMaxQuickReleaseRate ( 2.0bar/s )
TrainBrakesControllerEmergencyApplicationRate ( 1.86bar/s )
TrainBrakesControllerMaxSystemPressure ( 5bar )

ORTSBrakePipeTimeFactor ( 0.003 )
ORTSBrakeServiceTimeFactor ( 1.009 )
ORTSBrakeEmergencyTimeFactor ( 0.1 )

BrakesEngineBrakeType ( "Air_single_pipe" )
BrakesTrainBrakeType ( "Air_single_pipe" )
BrakesEngineControllers( "Independent, Train" )

Comment ( "Ovladani jizdy" )

Comment ( "Vlakovy zabezpecovac" )
VigilanceMonitor (
MonitoringDeviceMonitorTimeLimit ( 16 )
MonitoringDeviceAlarmTimeLimit ( 6 )
MonitoringDevicePenaltyTimeLimit ( 0 )
MonitoringDeviceCriticalLevel ( 0 )
MonitoringDeviceResetLevel ( 1.3 )
MonitoringDeviceAppliesFullBrake ( 0 )
MonitoringDeviceAppliesEmergencyBrake ( 1 )
MonitoringDeviceAppliesCutsPower ( 1 )
MonitoringDeviceAppliesShutsDownEngine ( 0 )
MonitoringDeviceTriggerOnOverspeed ( 1.6 )
MonitoringDeviceTriggerOnTrackOverspeed ( 0 )
MonitoringDeviceTriggerOnTrackOverspeedMargin ( 0.2 )
MonitoringDeviceResetOnZeroSpeed ( 1 )
MonitoringDeviceResetOnResetButton ( 1 )
)

Comment ( "Rizeni" )
EngineControllers (

Comment ( "Kontroler" )
Throttle ( 0 1 0.005 0 
NumNotches ( 48 
Notch ( 0.00 0 Dummy ) comment( 0 ) 
Notch ( 0.04 0 Dummy ) comment( X ) 
Notch ( 0.05 0 Dummy ) comment( 1 ) 
Notch ( 0.07 0 Dummy ) comment( 2 ) 
Notch ( 0.09 0 Dummy ) comment( 3 ) 
Notch ( 0.11 0 Dummy ) comment( 4 ) 
Notch ( 0.13 0 Dummy ) comment( 5 ) 
Notch ( 0.14 0 Dummy ) comment( 6 xxxA 137kN 0kMh ) 
Notch ( 0.15 0 Dummy ) comment( 7 ) 
Notch ( 0.16 0 Dummy ) comment( 8 ) 
Notch ( 0.17 0 Dummy ) comment( 9 ) 
Notch ( 0.18 0 Dummy ) comment( 10 ) 
Notch ( 0.19 0 Dummy ) comment( 11 ) 
Notch ( 0.20 0 Dummy ) comment( 12 ) 
Notch ( 0.21 0 Dummy ) comment( 13 ) 
Notch ( 0.22 0 Dummy ) comment( 14 ) 
Notch ( 0.23 0 Dummy ) comment( 15 ) 
Notch ( 0.24 0 Dummy ) comment( 16 ) 
Notch ( 0.25 0 Dummy ) comment( 17 ) 
Notch ( 0.26 0 Dummy ) comment( 18 ) 
Notch ( 0.27 0 Dummy ) comment( 19 ) 
Notch ( 0.28 0 Dummy ) comment( 20 ) 
Notch ( 0.29 0 Dummy ) comment( 21 ) 
Notch ( 0.30 0 Dummy ) comment( 22 ) 
Notch ( 0.31 0 Dummy ) comment( 23 ) 
Notch ( 0.32 0 Dummy ) comment( 24 Serie ) 
Notch ( 0.33 0 Dummy ) comment( SI ) 
Notch ( 0.35 0 Dummy ) comment( SII ) 
Notch ( 0.37 0 Dummy ) comment( SIII ) 
Notch ( 0.39 0 Dummy ) comment( SIV ) 
Notch ( 0.41 0 Dummy ) comment( A ) 
Notch ( 0.44 0 Dummy ) comment( B ) 
Notch ( 0.47 0 Dummy ) comment( C ) 
Notch ( 0.50 0 Dummy ) comment( 25 ) 
Notch ( 0.52 0 Dummy ) comment( 26 ) 
Notch ( 0.54 0 Dummy ) comment( 27 ) 
Notch ( 0.56 0 Dummy ) comment( 28 ) 
Notch ( 0.58 0 Dummy ) comment( 29 ) 
Notch ( 0.60 0 Dummy ) comment( 30 ) 
Notch ( 0.63 0 Dummy ) comment( 31 ) 
Notch ( 0.67 0 Dummy ) comment( 32 ) 
Notch ( 0.71 0 Dummy ) comment( 33 ) 
Notch ( 0.75 0 Dummy ) comment( PI )
Notch ( 0.80 0 Dummy ) comment( P5I ) 
Notch ( 0.85 0 Dummy ) comment( PIII )
Notch ( 0.90 0 Dummy ) comment( PIV ) 
Notch ( 0.95 0 Dummy ) comment( PV ) 
Notch ( 1.00 0 Dummy ) comment( PVI ) 
) 
)

Comment ( "Primocinna brzda typ DAKO-BP" )
Brake_Engine ( 0 0.8 0.125 0.8
NumNotches( 1 
Notch( 0 1 Dummy ) )
)

Comment ( "Prubezna brzda typ DAKO-BS2" )
Brake_Train ( 0 1 0.04 0.21
NumNotches ( 6
Notch ( 0 0 TrainBrakesControllerFullQuickReleaseStart )
Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
Notch ( 0.95 0 TrainBrakesControllerSuppressionStart )
Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
)
)

Comment ( "Rucni brzda" )
Brake_Hand ( 0 1 0.025 0
NumNotches ( 0 )
)

DirControl ( -1 0 1 1 )
BellToggle ( 0 1 0 )
Sanding ( 0 1 0 )
Horn ( 0 1 0 )
Wipers ( 0 1 0 )
PantographToggle1 ( 0 1 0 )
PantographToggle2		( 0 1 0 ) 
PantographsToggle_4 		( 0 1 0 ) 
EmergencyStopToggle ( 0 1 1 )
Vigilance ( 0 1 0 )
Headlights ( 0 0.25 1 0 )
BailOffButton ( 0 1 0 )
)

Comment ( "Ostatní informace" )
Name ( " CSD 141 045-5" )
CabView ( "141.cvf" )
HeadOut ( 1.6 2.9 6.2 )
Sound ( "..//..//common.snd//sndElok//141cab.sms" )

Comment ( "Poznamky" )
Description (
"Rada E499.1 CSD je univerzalni elektricka lokomotiva\n\n"+
"pro vozbu rychliku a osobnich vlaku\n\n"+
"Max. provozni rychlost: 120km/h\n\n"+
"Hmotnost plne vyzbroj. lokomotivy: 84tun\n\n"+
"Vykon 38% odpovida hospodarnemu seriovemu stupni\n\n"+
"Vykon 64% odpovida hospodarnemu serioparalelnimu stupni\n\n"+
"Vykon hodinovy : 2344kW\n\n"+
"Vykon trvaly : 2032kW\n\n"+
"Tazna sila na haku : 230kN\n\n"+
"Proud p?i Ft = 200kN : 450A\n\n"+
"Proud p?i Ft = 175kN : 400A\n\n"+
"Proud p?i Ft = 160kN : 365A\n\n"+
"Pretizeni:\n"+
"Proud trvaly : 360A\n\n"+
"60min: 415A\n\n"+
"45min: 455A\n"+
"30min: 510A\n"+
"15min: 605A\n"+
"Brzda DAKO-L\n\n"+
"Brzdic prubezne vlakove brzdy Skoda N/O, pozdeji vymenen za DAKO-BS2\n\n"+
"Brzdic lokomotivni brzdy DAKO-BP."
)

EngineOperatingProcedures (
"Viz. manual Open Rails"+
"TIP: V prubehu jizdy pomoc na klavese F1.\n\n"+
"Rozjezd: Pantograf nahoru (P), nahodit jistic (O).\n\n"+
"Stupne kontroleru(informativne):\n"+
"1.-23.	Rozjezdove stupne seriove\n"+
"24.	Hospodarny seriovy stupen (odporniky vyrazeny)\n"+
"I.-IV.	Shuntovaci rozjedove stupne, vsechny motory v serii\n"+
"A.B.C.	Prechodove stupne serie - > serioparalel\n"+
"25.-32.Odporove serioparalelni stupne (vzdy dva motory v serii)\n"+
"33.	Hospodarny serioparalelni stupen (odporniky vyrazeny)\n"+
"I.-V.	Shuntovaci stupne pro serioparalelni zapojeni motoru"
)
)
