SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( 141-045
	Type ( Engine )
	WagonShape ( 141-045.s )

	Comment ( Eng modified by ZSR - http://csd.webzdarma.cz )
	Comment ( Version 1.11 )
	Comment ( Datum: 23.3.2010 )	
	Comment ( Vyladena kompletni vykonova charakteristika - adheasion, friction, maxpower, maxcurrent, maxforce )
	Comment ( Umisten brzdic Skoda N/O - dle originalni dokumentace )
	Comment ( Svetla pro BIN )
	Comment ( Update nadproudove ochrany pro BIN 1.7x ) 

	Size ( 3.15m 4.59m 15.88m )
	Mass ( 84.0t )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box ( 3.15m 4.59m 15.88m ) )

	Coupling ( 
		Type ( Chain ) 
			Spring ( 
			Stiffness ( 7.5E6N/m 1E7N/m ) 
			Damping ( 1E6N/m/s 2E6N/m/s ) 
			Break ( 1.1E7N 5E7N ) 
			r0 ( 30cm 60cm ) 
		) 
		CouplingHasRigidConnection ( 0 ) 
		Velocity ( 0.01m/s ) 
	) 
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 10cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)

	Adheasion ( 0.114 0.64 1.35 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*84t )
	DerailBufferForce ( 350kN )
	NumWheels (	4 )
	Friction (
		1051.4N/m/s		-0.1		1.3mph		14.200N/m/s		2.100
		5.1N/rad/s		1		-1rad/s		0		1
	)

comment	( Brzdy vozu )

	MaxBrakeForce( 51kN )
	MaxHandbrakeForce( 14kN )
	NumberOfHandbrakeLeverSteps( 100 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 1.3 )
	MaxApplicationRate( 4 )
	MaxAuxilaryChargingRate( 2.5 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
        EmergencyResVolumeMultiplier ( 11 )
        EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 ) 
	
comment	( EngSound, Freight, Inside )


	
      	Inside (
		PassengerCabinFile ( 141-045.s )
		PassengerCabinHeadPos ( -1.6 2.9 6.2 )
		RotationLimit ( 0 190 0 )
		StartDirection ( 0 0 0 )
	)	
	

comment ( Lights ) 


	Lights ( 32
	
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0 1 7 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 80 )
				)
			)
		)
		Light (
			comment ( Svetelný kuzel tlumený )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FF666666 )
					Position ( 0 2 -2 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 60 )
				)
			)
		)
		
		comment ( Definice svetel pro prední stanoviste )

		Light (
			comment ( reflektor dálkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					LightColour ( EEEED15D ) 
					Position ( 0.0 3.60 7.42 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 1 ) 
					Radius ( 0.9 ) 
				)
			)
		)
		Light (
			comment ( reflektor tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D ) 
					Position ( 0.0 3.60 7.42 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 1 ) 
					Radius ( 0.4 ) 
				)
			)
		)

		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( 0.9 1.53 7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		
		Light (
			comment ( Prední leve pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( -0.9 1.53 7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)		
		
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( -0.9 1.53 -7.47 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.3 )
				)
			)
		)
		
		Light (
			comment ( zadní prave pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( 0.9 1.53 -7.47 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.3 )
				)
			)
		)		
		
		
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( -0.9 1.53 7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( 0.9 1.53 7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)


		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 ) 
					Position ( -0.9 1.53 -7.47 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 ) 
					Position ( 0.9 1.53 -7.47 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )

		Light (
			comment ( reflektor dálkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D ) 
					Position ( 0.0 3.60 -7.42 ) 
					Azimuth ( -180 -180 -175 ) 
					Transition ( 0 ) 
					Radius ( 0.9 ) 
				)
			)
		)
		Light (
			comment ( reflektor tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D ) 
					Position ( 0.0 3.60 -7.42 ) 
					Azimuth ( -180 -180 -180 ) 
					Transition ( 0 ) 
					Radius ( 0.4 ) 
				)
			)
		)
		
		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( 0.9 1.53 7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		
		Light (
			comment ( Prední leve pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( -0.9 1.53 7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)		
		
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( -0.9 1.53 -7.47 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.3 )
				)
			)
		)
		
		Light (
			comment ( zadní prave pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( 0.9 1.53 -7.47 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.3 )
				)
			)
		)		
		
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( -0.9 1.53 -7.47 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( 0.9 1.53 -7.47 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 ) 
					Position ( -0.9 1.53 7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 ) 
					Position ( 0.9 1.53 7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Levé p?ední pozi?ní - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFE085 ) 
					Position ( -0.9 1.53 -7.47 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		Light	(
			comment( Pravé p?ední pozi?ní - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFE085 ) 
					Position ( 0.9 1.53 -7.47 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		Light	(
			comment( Levé zadní pozi?ní - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFE085 ) 
					Position ( -0.9 1.53 7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		Light	(
			comment( Pravé zadní pozi?ní - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFE085 ) 
					Position ( 0.9 1.53 7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
					)
			)
		)

		comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( Svetelný kuzel tlumený )
			Type ( 1 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FF666666 )
					Position ( 0 2 -2 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 60 )
				)
			)
		)
		Light (
			comment ( PC reflektor prední )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D ) 
					Position ( 0.0 3.60 7.42 ) 
					Azimuth ( 0 0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.4 ) 
				)
			)
		)
		Light (
			comment ( PC prední leve )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( -0.9 1.53 7.47 ) 
					Azimuth ( 0.0 0.0 0.0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		Light (
			comment ( PC prední prave )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 ) 
					Position ( 0.9 1.53 7.47 ) 
					Azimuth ( 0.0 0.0 0.0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)

		Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 ) 
					Position ( -0.9 1.53 -7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 ) 
					Position ( 0.9 1.53 -7.47 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.3 ) 
     					)
   				)
   			)	
  		)

	Sound ( "../../common.snd/sndelok/141eng.sms" )	
)  
	
Engine ( 141-045

	Wagon	( 141-045 )
	

	Type ( Electric )
	MaxVelocity								( 77.5mph )
	MaxPower								( 2814kW )
	MaxForce								( 1248kN )	
	MaxContinuousForce						( 1248kN )
	MaxCurrent								( 4581A )
	DieselEngineSpeedOfMaxTractiveEffort	( 0mph )
	WheelRadius								( 0.625m )
	NumWheels								( 4 )
	Sanding									( 60km/h )
	MaxSandingTime                         	( 600 )
	DoesBrakeCutPower                      	( 1 )
	DoesHornTriggerBell                    	( 0 )
	
comment	( CabSound and Views )

	Sound ( "../../common.snd/sndelok/141cab.sms" )


	CabView ( "../../common.cab/cab141/141.cvf" )

	
	HeadOut ( 1.6 2.9 6.2 ) 	
	

comment	( Brzdy loko )

	BrakesEngineBrakeType	( Air_single_pipe )
	BrakesTrainBrakeType	( Air_single_pipe )
	BrakesEngineControllers	( "Hand, Train, Independent" )

	AirBrakesAirCompressorPowerRating ( 1.18 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 102 )	
	AirBrakesMainResVolume ( 32.84 )
	AirBrakesAirCompressorWattage ( 15000 )
	AirBrakesCompressorRestartPressure ( 80 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 3 )
	TrainBrakesControllerMaxApplicationRate ( 1 )
	TrainBrakesControllerMaxReleaseRate ( 0.5 )
	TrainBrakesControllerMaxQuickReleaseRate ( 1.5 )
	TrainBrakesControllerEmergencyApplicationRate ( 3 )
	TrainBrakesControllerMinSystemPressure ( 3 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22 )
	TrainPipeLeakRate ( 0.033 )
	TrainBrakesControllerFullServicePressureDrop ( 22 )
	
	DoesBrakeCutPower ( 1 )

comment	( Monitors )

	EmergencyStopMonitor (
	  MonitoringDeviceMonitorTimeLimit ( 0 )
	  MonitoringDeviceAlarmTimeLimit ( 0 )
	  MonitoringDevicePenaltyTimeLimit ( 0 )
	  MonitoringDeviceCriticalLevel ( 0 )
	  MonitoringDeviceResetLevel ( 0 )
	  MonitoringDeviceAppliesFullBrake ( 0 )
	  MonitoringDeviceAppliesEmergencyBrake ( 0 )
	  MonitoringDeviceAppliesCutsPower ( 1 )
	  MonitoringDeviceAppliesShutsDownEngine ( 0 )
	  MonitoringDeviceResetOnZeroSpeed ( 1 ) 

	 )
	 VigilanceMonitor (
	  MonitoringDeviceMonitorTimeLimit ( 27 )
	  MonitoringDeviceAlarmTimeLimit ( 17 )
	  MonitoringDevicePenaltyTimeLimit ( 0 )
	  MonitoringDeviceCriticalLevel ( 0 )
	  MonitoringDeviceResetLevel ( 0 )

	  MonitoringDeviceAppliesFullBrake ( 0 )
	  MonitoringDeviceAppliesEmergencyBrake ( 1 )
	  MonitoringDeviceAppliesCutsPower ( 1 )
	  MonitoringDeviceAppliesShutsDownEngine ( 0 )
	  MonitoringDeviceResetOnZeroSpeed ( 1 )
	  MonitoringDeviceResetOnResetButton ( 1 )
	  MonitoringDeviceResetOnDirectionNeutral ( 1 )
	 )
	 OverspeedMonitor (
	  MonitoringDeviceMonitorTimeLimit ( 0 )
	  MonitoringDeviceAlarmTimeLimit ( 5 )
	  MonitoringDevicePenaltyTimeLimit ( 0 )
	  MonitoringDeviceCriticalLevel ( 77.5 )
	  MonitoringDeviceResetLevel ( 0 )
	  Comment ( MonitoringDeviceTriggerOnHighCurrent ( 700 ) )
	  MonitoringDeviceAppliesFullBrake ( 0 )
	  MonitoringDeviceAppliesEmergencyBrake ( 1 )
	  MonitoringDeviceAppliesCutsPower ( 0 )
	  MonitoringDeviceAppliesShutsDownEngine ( 0 )
	  MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
	  MonitoringDeviceDoesSuppressionReset ( 0 )
	  MonitoringDeviceTriggerOnOverspeed ( 77.6 )
	  MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
	  MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
	  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
	  MonitoringDeviceResetOnResetButton ( 0 )
	 )
	 

Comment ( End of Monitors )
		
comment	( Controllers )

	EngineControllers (

		AWS				( 0 1 0 )
		BailOffButton			( 0 1 0 )
		BellToggle			( 0 1 0 )
		DirControl			( -1 0 1 1 )
		EmergencyStopToggle		( 0 1 0 )
		Headlights			( 0 0.25 1 0 )
		Horn				( 0 1 0 )
		PantographToggle1 		( 0 1 0 ) 
		PantographToggle2		( 0 1 0 ) 
		PantographsToggle_4 		( 0 1 0 ) 
		Sanding				( 0 1 0 )
		Vigilance			( 0 1 0 )
		Wipers				( 0 1 0 )

	Throttle ( 0 1 0.005 0
	NumNotches ( 48
	Notch ( 0.0   0 Dummy )
	Notch ( 0.004 0 Dummy )

	Notch ( 0.02  0 Dummy )
	Notch ( 0.03  0 Dummy )
	Notch ( 0.05  0 Dummy )
	Notch ( 0.06  0 Dummy )
	Notch ( 0.08  0 Dummy )

	Notch ( 0.10  0 Dummy )
	Notch ( 0.12  0 Dummy )
	Notch ( 0.13  0 Dummy )
	Notch ( 0.14  0 Dummy )
	Notch ( 0.15  0 Dummy )

	Notch ( 0.16  0 Dummy )
	Notch ( 0.18  0 Dummy )
	Notch ( 0.20  0 Dummy )
	Notch ( 0.22  0 Dummy )
	Notch ( 0.24  0 Dummy )

	Notch ( 0.26  0 Dummy )
	Notch ( 0.28  0 Dummy )
	Notch ( 0.30  0 Dummy )
	Notch ( 0.32  0 Dummy )
	Notch ( 0.34  0 Dummy )

	Notch ( 0.35  0 Dummy )
	Notch ( 0.36  0 Dummy )
	Notch ( 0.37  0 Dummy )

	Notch ( 0.38  0 Dummy )

	Notch ( 0.41  0 Dummy )
	Notch ( 0.44  0 Dummy )
	Notch ( 0.47  0 Dummy )
	Notch ( 0.50  0 Dummy )

	Notch ( 0.505 0 Dummy )
	Notch ( 0.510 0 Dummy )
	Notch ( 0.515  0 Dummy )

	Notch ( 0.52  0 Dummy )
	Notch ( 0.53  0 Dummy )
	Notch ( 0.55  0 Dummy )
	Notch ( 0.57  0 Dummy )
	Notch ( 0.59  0 Dummy )
	Notch ( 0.61  0 Dummy )
	Notch ( 0.62  0 Dummy )
	Notch ( 0.63  0 Dummy )

	Notch ( 0.64  0 Dummy )

	Notch ( 0.71  0 Dummy )
	Notch ( 0.78  0 Dummy )
	Notch ( 0.85  0 Dummy )
	Notch ( 0.93  0 Dummy )
	Notch ( 0.999 0 Dummy )
	Notch ( 1     0 Dummy )
	) )

	Brake_Hand		( 0 1 1.0 0
		NumNotches	( 0 )
		)

	Brake_Engine	( 0 1 0.07 0
		NumNotches	( 1
		Notch		( 0	1 Dummy )
	) )

comment ( Prubezna brzda typ Skoda N/O )
           Brake_Train ( 0 1 0.03 0.95 
                NumNotches ( 5
                    
		    Notch ( 0.2  0 TrainBrakesControllerFullQuickReleaseStart )
                    Notch ( 0.3  0 TrainBrakesControllerReleaseStart ) 
                    Notch ( 0.45 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch ( 0.95 0 TrainBrakesControllerSuppressionStart )
                    Notch ( 1 0 TrainBrakesControllerEmergencyStart )  
                  
                    
                    
                )
            )

	)
	Name	( " CSD 141 045-5" )
Comment	( Operations )

	Description (
	"Rada 141 CD je univerzalni elektricka kapotova lokomotiva\n\n"+
	"Max. provozni rychlost:  120km/h TBZ=132km/h\n\n"+
	"Hmotnost plne vyzbroj. lokomotivy: 84tun\n\n"+
	"Vykon 38% odpovida hospodarnemu seriovemu stupni\n\n"+ 
	"Vykon 64% odpovida hospodarnemu serioparalelnimu stupni\n\n"+
	"Vykon hodinovy : 2344kW\n\n"+
	"Vykon trvaly   : 2032kW\n\n"+
	"Tazna sila na haku  : 205kN\n\n"+
	"Proud pri Ft = 200kN : 550A\n\n"+
	"Proud pri Ft = 175kN : 500A\n\n"+
	"Proud pri Ft = 160kN : 450A\n\n"+
	"Pretizeni:\n"+
	"Proud trvaly : 360A\n\n"+
    		"60min: 415A\n\n"+
    		"45min: 455A\n"+
    		"30min: 510A\n"+
    		"15min: 605A\n"+
	"Brzda DAKO-L\n\n"+
	"Brzdic prubezne vlakove brzdy Skoda N/O\n\n"+
	"Brzdic lokomotivni brzdy DAKO-BP\n\n"
    	)

   	EngineOperatingProcedures (
		"Stupne kontroleru:\n"+
		"1.-23.	Rozjezdove stupne seriove\n"+
		"24.	Hospodarny seriovy stupen (odporniky vyrazeny)\n"+
		"I.-IV.	Shuntovaci rozjedove stupne, vsechny motory v serii\n"+
		"A.B.C.	Prechodove stupne serie - > serioparalel\n"+
		"25.-32.Odporove serioparalelni stupne (vzdy dva motory v serii)\n"+
		"33.	Hospodarny serioparalelni stupen (odporniky vyrazeny)\n"+
		"I.-V.	Shuntovaci stupne pro serioparalelni zapojeni motoru\n\n"
	)
	
)
