SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( IDS_742260

	Comment (** regulator GC34P **)
	Comment (** ladeni ORCZ/SK **)
	comment (** prosinec 2023 - Igor Hnizdo - prepracovano na ORCZ/SK v1.8, nutna minimalne verze 1.8.348. Ve starsich verzich programu nemusi ladeni spravne fungovat. **)


	Type ( Engine )
	WagonShape ( IDS_742260.s )
	ORTSFreightAnims (
        	 MSTSFreightAnimEnabled ( 0 )
				FreightAnimStatic (
				SubType( Default )
				Shape( "IDS_742260fg.s" )
				Offset( -0.0, 0.0, 0.0 )
				Visibility ( "Cab2D" )
				)
				FreightAnimStatic (
				SubType( Default )
				Shape( "742_kapota.s" )
				Offset( -0.0, 0.0, 0.0 )
				Visibility ( "Outside" )
				)
				FreightAnimStatic (
				SubType( Default )
				Shape( "742_kapota.s" )
				Offset( -0.0, 0.0, 0.0 )
				Visibility ( "Cab2D" )
				)
				FreightAnimStatic (
				SubType( Default )
				Shape( "742_horne_zaluzie.s" )
				Offset( -0.0, 0.0, 0.0 )
				Visibility ( "Outside" )
				)
				FreightAnimStatic (
				SubType( Default )
				Shape( "742_fan.s" )
				Offset( -0.0, 0.0, 0.0 )
				Visibility ( "Outside" )
				)
		)
	
Mass ( 64t )

Include 	("../../common.eng/74x/udaje_742.inc")
Include 	("../../common.inc/spriahlo/1-5cm.inc")
Include 	("../../common.eng/74x/adheze_odpor_742.inc")
Include 	("../../common.eng/74x/brzda_74x.inc")
comment (** unik vzduchu netesnosti brzdoveho potrubi **)
TrainPipeLeakRate ( 0.000283bar/s )
Include 	("../../common.eng/74x/MBF_742.inc")
comment (** krivka soucinitele treni brzdovych zdrzi **)
Include 	("../../common.inc/brzdna_krivka/zdrze-litina-PG.inc")
Include 	("../../common.eng/74x/svetla_742-delene.inc")

comment (** smerovani na vnejsi ozvuceni **)
Sound ( "../../common.snd/snd742.512-IH/742.512eng-ORCZ.sms" )

     )

Engine ( IDS_742260

        Wagon ( IDS_742260 )

comment (** smerovani na pohled z kabiny **)
CabView ( "../../common.cab/cab742d/cab742d.cvf" )

comment (** smerovani na ozvuceni pohledu z kabiny **)
Sound ( "../../common.snd/snd742.512-IH/742.512cab-ORCZ.sms" )

Include 	("../../common.eng/74x/HeadOut74x.inc")
Include 	("../../common.eng/74x/parametry_742GC33P-adh100.inc")
Include 	("../../common.eng/74x/motor_K6S230-GC33P-100.inc")
Include 	("../../common.eng/74x/efekty_kour_74x.inc")
Include 	("../../common.eng/74x/tch742.inc")
Include 	("../../common.eng/74x/Trakcni_proud_742.inc")
Include 	("../../common.eng/74x/vzduchotechnika_74x.inc")
Include 	("../../common.inc/brzdice/BP-4bar.inc")
Include 	("../../common.inc/brzdice/BS2.inc")
Include 	("../../common.inc/MIREL_VZ/LS90_140kmh.inc")
Include 	("../../common.eng/74x/ovladani_742.inc")


comment (** nazev v menu ORTS **)
Name ( "IDS 742 260-3 ORCZ" )

Description (
	 "Rada 742 CD je univerzalni dieselelektricka kapotova lokomotiva"+
	 "pro pouziti od posunovaciho provozu pres tazeni osobnich"+
	 "az do tazeni stredne tezkych nakladnich vlaku v dvojclennem rizeni.\n\n"+
	 "Usporadani dvojkoli: B0'B0'\n\n"+
	 "Prenos vykonu: elektricky\n\n"+
	 "Zdroj vykonu: naftovy motor CKD K 6 S 230 DR\n\n"+
	 "Vykon spalovaciho motoru: 883kW\n\n"+
	 "Max. provozni rychlost:  90km/h\n\n"+
	 "Trvala tazna sila na haku: 121kN pri 1200A\n\n"+
	 "Max. vyska: 4722mm\n\n"+
	 "Delka pres nar.: 13600mm\n\n"+
	 "Max. sirka: 3060mm\n\n"+
	 "Hmotnost plne vyzbroj. lokomotivy: 64t"  
    	)

)