SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( awt_753732
	comment( upravil Ondra Janis na zaklade poznatku o ladeni eng 
  souboru od Ppoolllla, Jacka, O.Frinty & ZSR  - verze 1.5 - svetla CZ )
	comment( upravy brzd pro zvuky, svetla pro MSTSbin dle Jacka )
	Type ( Engine )
	WagonShape ( awt_753732.s )
	Size ( 3.10m 4.47m 16.24m )  
	CentreOfGravity ( 0m 1.9m 0m )
	Mass ( 73t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3m 4.4m 16.2m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)

	Adheasion ( 0.15 0.64 1.80 0 )
  comment ( melo by odpovidat stredni adhezni sile pro 753.7 ~210kN )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*73t )
	DerailBufferForce ( 350kN )
comment( pocet naprav )
	NumWheels (	4 )
comment( sily urcujici jizdni odpory )
	Friction (
		2058N/m/s		0		0.625mph		7.8N/m/s		2
		5.1N/rad/s		1		-1rad/s		0		1
	)

  BrakeEquipmentType( "handbrake, graduated_release_triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 47kN )
	comment(odpovida 70 brzdnym % v rezimu P - ZD 620m)

	MaxHandbrakeForce( 11kN )
	NumberOfHandbrakeLeverSteps( 100 )

	EmergencyBrakeResMaxPressure( 73 )
	TripleValveRatio( 2.48 )
	MaxReleaseRate( 1.5 )
	comment (brzda v rezimu P - odbrzdeni cca. 16s)
	MaxApplicationRate( 2 )
  comment (brzda v rezimu P - plneni cca. 5s)
	MaxAuxilaryChargingRate( 5 )
	EmergencyResCapacity( 14 )
	EmergencyResChargingRate( 5 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 0.02 )

	IntakePoint ( 0 1.0 FuelDiesel )

	PassengerCapacity ( 80.0 )
	Comment (kapacita cestujicich - jen kvuli tvorbe Jr v misich)
  comment	( Lights )

  comment (nastaveni svetel - CZ)
	Lights ( 31
		Light (
			comment ( Svetelny kuzel dalkovy )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
			  	Position ( 0.0 1.6 7.75 )
					Angle ( 20 )
					Transition ( 1 )
					Radius ( 120 )
				)
			)
		)
		Light (
			comment ( Svetelny kuzel tlumeny )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FF87CEFA )
					Position ( 0.0 1.6 7.75 )
					Angle ( 25 )
					Transition ( 1 )
					Radius ( 50 )
				)
			)
		)
		
		comment ( Definice svetel pro predni stanoviste )

		Light (
			comment ( reflektor dalkovy L )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )       
					Position ( -0.641 1.389 7.67 )
          Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor dalkovy P )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )       
					Position ( 0.641 1.389 7.67 ) 
          Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FF87CEFA )     
					Position ( -0.891 1.389 7.67 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
        Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FF87CEFA )      
					Position ( 0.891 1.389 7.67 ) 
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Predni leve zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FF87CEFA )     
					Position ( -0.891 1.389 7.67 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Predni prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
        Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FF87CEFA )      
					Position ( 0.891 1.389 7.67 ) 
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( predni horni )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )   
					Position ( 0.0 3.78 7.835 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni leve pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
        Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FF87CEFA )        
					Position ( -0.891 1.389 -7.67 )  
 					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni prave pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
        Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FF87CEFA )        
					Position ( 0.891 1.389 -7.67 ) 
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni leve koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( ffFF0000 )       
					Position ( -0.891 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( ffFF0000 )       
					Position ( 0.891 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		
		comment ( Definice svetel pro zadni stanoviste )

		Light (
			comment ( reflektor dalkovy L )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )       
					Position ( 0.641 1.389 -7.67 )
          Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor dalkovy P )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )       
					Position ( -0.641 1.389 -7.67 ) 
          Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Predni leve zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FF87CEFA )     
					Position ( 0.891 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Predni prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
        Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FF87CEFA )      
					Position ( -0.891 1.389 -7.67 ) 
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( predni horni )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )   
					Position ( 0.0 3.78 -7.835 )
          Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni leve koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( ffFF0000 )       
					Position ( 0.891 1.389 7.67 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( ffFF0000 )       
					Position ( -0.891 1.389 7.67 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Leve predni pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FF87CEFA )        
					Position ( -0.891 1.389 7.67 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Prave predni pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FF87CEFA )        
					Position ( 0.891 1.389 7.67 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Leve zadni pozicni - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FF87CEFA )        
					Position ( -0.891 1.389 -7.67 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Prave zadni pozicni - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FF87CEFA )        
					Position ( 0.891 1.389 -7.67 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
			)
		)

		comment ( Definice svetel pro loko ovladanou PC )

		Light (
			comment ( PC predni prave )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FF87CEFA )        
					Position ( 0.891 1.389 7.67 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC predni leve )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FF87CEFA )        
					Position ( -0.891 1.389 7.67 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC horni )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )   
					Position ( 0.0 3.78 7.835 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC reflektor predni L )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )       
					Position ( 0.641 1.389 7.67 )
          Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC reflektor predni P )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )       
					Position ( -0.641 1.389 7.67 )
          Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC zadni leve koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffFF0000 )       
					Position ( -0.891 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC zadni prave koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffFF0000 )       
					Position ( 0.891 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
	)
	Sound ( "..\\..\\common.snd\\sndDlok\\750.7eng.sms" )
)

Engine ( awt_753732
	Effects (
		DieselSpecialEffects (
			Exhaust1
			(
					0.454 4.6 1.59
					0 1 0
					0.1
			)
			Exhaust2
			(
					-0.454 4.6 1.59
					0 1 0
					0.1
			)
		)
	)
	Wagon ( awt_753732 )
	Type ( Diesel )
	MaxPower ( 1135kW ) 
      comment (vykon na obvodu kol - vypocteno z trakcni char.) 
	MaxForce ( 205kN )
	    comment (SW omezeni tazne sily pro 753.7)
	RunUpTimeToMaxForce ( 10.0 )
	MaxContinuousForce ( 205kN )
	MaxVelocity ( 100km/h )
	MaxCurrent ( 3870A )
	 comment(nejde o skutecny max. proud, ale kompromis pro realnejsi ukazovani ampermetru - 2200A pri F = 127kN )
	WheelRadius ( 0.5m )
	Sanding ( 30km/h )
	NumWheels ( 4 )
	MaxTemperature ( 120 )
	MaxOilPressure ( 90 )
	DieselEngineSpeedOfMaxTractiveEffort( 31km/h )
	
  AirBrakesAirCompressorPowerRating( 1.72 )
	AirBrakesMainMinResAirPressure( 68 )
	AirBrakesMainMaxAirPressure( 142 )
	AirBrakesMainResVolume( 35 )
	AirBrakesAirCompressorWattage( 23500 )
	AirBrakesCompressorRestartPressure( 116 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 2 )
	AirBrakesHasLowPressureTest( 1 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

  EngineBrakesControllerMaxQuickReleaseRate ( 4 )  
  EngineBrakesControllerMaxReleaseRate ( 2 )  
  EngineBrakesControllerMinPressureReduction ( 1 )  
  EngineBrakesControllerMaxApplicationRate ( 4 )  
  EngineBrakesControllerEmergencyApplicationRate ( 4 )  
  EngineBrakesControllerMinSystemPressure ( 0 )  
  EngineBrakesControllerMaxSystemPressure ( 73 )  
  EngineBrakesControllerFullServicePressureDrop ( 56 )  
  EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 )  
  EngineBrakesControllerHasProportionalBrake ( 0 )  
  EngineBrakesProportionalBrakeLag ( 0 ) 

	TrainBrakesControllerMinPressureReduction( 3 )
	TrainBrakeControllerMinContinuousService ( 2 )	
	TrainBrakesControllerMaxApplicationRate( 2 )
	TrainBrakesControllerMaxReleaseRate( 2 )
	TrainBrakesControllerMaxQuickReleaseRate ( 4 )
	TrainBrakesControllerEmergencyApplicationRate( 6 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22.5 )
	TrainBrakesControllerMaxSystemPressure( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 60 )
	TrainBrakesControllerFullServicePressureDrop( 22.5 )
	TrainPipeLeakRate( 0.1 )
	
	DynamicBrakesMaximumForce ( 110kN )
	DynamicBrakesResistorCurrentLimit ( 570 )
	DynamicBrakesMaxAirBrakePressure ( 50 )
  DynamicBrakesMinUsableSpeed ( 0.5 )
  DynamicBrakesCutInSpeed ( 3 )
	DynamicBrakesFadingSpeed ( 13.75 )
	DynamicBrakesMaximumEffectiveSpeed ( 40 )
	DynamicBrakesMaximumSpeedForFadeOut ( 94 )
	DynamicBrakesEffectAtMaximumFadeOut ( 0.2 )
	DynamicBrakesDelayTimeBeforeEngaging ( 1 )
	DynamicBrakesHigherSpeedCurveExponent ( 2 )
	DynamicBrakesLowerSpeedCurveExponent ( 1.1 )
	DynamicBrakesNumberOfControllerNotches ( 10 )
		
	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
  BrakesEngineControllers( "Independent, Train, Dynamic" )

 	CabView ( "../../common.cab/cab756/753.7.cvf" )
	HeadOut ( 1.7 3.2 6.45 )

 	MaxDieselLevel ( 5500l )
	DieselUsedPerHourAtMaxPower ( 358l )
	DieselUsedPerHourAtIdle ( 11l )

	DieselSmokeEffectInitialMagnitude( 0.4 )
	DieselSmokeEffectMaxMagnitude( 0.8 )
	
  DieselSmokeEffectInitialSmokeRate( 0.4 )
	DieselSmokeEffectMaxSmokeRate( 1.0 )

	DieselEngineIdleRPM( 600 )
	DieselEngineMaxRPM( 1800 )
  DieselEngineMaxRPMChangeRate( 100 )

	DoesHornTriggerBell( 0 )

	MaxSandingTime( 3000 )

	EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 27 )
		MonitoringDeviceAlarmTimeLimit ( 17 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 73 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 1 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 72 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 0 )
	)
		
	EngineVariables( 4000 )
			
        EngineControllers (
            Throttle ( 0 1 0.08 0
                NumNotches ( 1
		          		Notch ( 0    1 Dummy )
	             		)
            )            
           comment (Brake_Engine ( 0 1 0.1 0.5
                NumNotches ( 3
                    Notch ( 0.1 1 EngineBrakesControllerReleaseStart )
                    Notch ( 0.5 0 EngineBrakesControllerHoldStart )
                    Notch ( 0.9 1 EngineBrakesControllerApplyStart  )
                )
            )    )
            Brake_Engine ( 0 0.76 0.05 0.55
		           NumNotches ( 3
				          Notch ( 0.0 0 EngineBrakesControllerReleaseStart )
				          Notch ( 0.55 0 EngineBrakesControllerNeutralhandleOffStart )
				          Notch ( 0.9 0 EngineBrakesControllerFullServiceStart )
                )   
            ) 
            Brake_Dynamic ( 0 1 0.01 0
			         NumNotches ( 10
				          Notch ( 0 0 Dummy )
				          Notch ( 0.01 0 Dummy )
			           	Notch ( 0.125 0 Dummy )
				          Notch ( 0.25 0 Dummy )
				          Notch ( 0.325 0 Dummy )
				          Notch ( 0.5 0 Dummy )
				          Notch ( 0.625 0 Dummy )
				          Notch ( 0.75 0 Dummy )
				          Notch ( 0.875 0 Dummy )
				          Notch ( 1 0 Dummy )
			            )
		        )            
            comment(***Prubezna brzda typ DAKO-BSE (ovladac OBE-1)***)            
            Brake_Train ( 0 1 0.14 0.71
                NumNotches ( 5
                    Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
                    Notch ( 0.43 0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.57 0 TrainBrakesControllerRunningStart )
                    Notch ( 0.71 0 TrainBrakesControllerContinuousServiceStart )
                    Notch ( 1.00 0 TrainBrakesControllerEmergencyStart )
                )
            )
            Brake_Hand ( 0 1 0.0125 0 
            NumNotches( 1
                    Notch(0    1 Dummy)
                )
            )
            Combined_Control ( 0 1 0.5 0.5 throttle dynamic )
            DirControl ( -1 0 1 1 )
            AWS ( 0 1 0 )
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 1 )
            EmergencyStopToggle( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
	        	Vigilance ( 0 1 0 )
	        	BailOffButton( 0 1 0 )
        )
        
     	Name ("AWT 753 732-7")
    	Description (
     	"Rada 753.7 CD Cargo vznikla rekonstrukci rady 753\n\n"+
    	"Prenos vykonu: elektricky\n\n"+
    	"Zdroj vykonu: naftovy motor Caterpillar 3512B\n\n"+
    	"Max. vykon motoru: 1455 kW\n\n"+
    	"Max. trakcni vykon: 1200 kW\n\n"+
    	"Max. vyska: 4,430 m\n\n"+
    	"Max. sirka: 3,070 m\n\n"+
    	"Delka pres narazniky: 16,660 m\n\n"+
    	"Hmotnost: 72 t\n\n"+
    	"Max. rychlost: 100 km/h"
    	)
    	EngineOperatingProcedures (
		"Jak se rozjet:\n"+
		"1.	Stisknete W na prestaveni reverzniho kontoleru do polohy 'vpred'.\n"+
		"2.	Stisknete a drzte ; pro odbrzdeni vlakove brzdy.\n"+
		"(3.	Stisknete a drzte [ pro odbrzdeni lokomotivni brzdy.)\n"+
		"4.	Stisknete D pro zvyseni pozadovaneho vykonu.\n"+
		"5.	Pomalu zvysujte vykon stiskem D, dokud vlak nedosahne pozadovane rychlosti.\n"+
		"6.	Jakmile se vlak rozjede tak jednim stiskem ' presunte vlakovou brzdu do polohy ZaVER.\n\n"+
		"Jak zpomalit\n"+
		"1.	Stisknete A pro snizeni pozadovaneho vykonu (postupne az na 0).\n"+
		"2.	Jestlize je to nutne tak pouzijte brzdy pro postupne rychlejsi snizovani rychlosti.\n\n"+
		"Jak pouzit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosahnete pozadovaneho brzdneho tlaku.\n"+
		"2.	Po dosazeni pozadovaneho brzdneho tlaku stiskem ; presunte rukojet brzdy do polhy ZaVER.\n\n"+
		"Jak odbrzdit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENi.\n"+
		"2.	Pockejte, az klesne tlak v brzdovych valcich na 0.\n"+
		"3.	Po odbrzdeni a uvedeni vlaku do pohybu stisknete ' pro presunuti rukojeti brzdy do polohy ZaVER.\n\n"+
 		"Jak pouzit lokomotvni brzdu\n"+
		"1.	Stisknete a drzte ] pro zabrzdeni lokomotivni brzdy (0-100%).\n\n"+
		"Jak odbrzdit lokomotivni brzdu\n"+
		"1.	Stisknete a drzte [ pro odbrzdeni lokomotivni brzdy (0%).\n\n"+
		"Jak pouzit zachrannou brzdu\n"+
		"1.	Stisknete a drzte A pro snizeni vykonu az na 0.\n"+
		"2.	Stisknete BACKSPACE pro aktivaci zachrane brzdy.\n\n"+
		"Jak zrusit zachrannou brzdu\n"+
		"1.	Pockejte na uplne zastaveni vlaku.\n"+
		"2.	Stisknete Z pro odblokovani ovladani lokomotivy.\n"+
		"3.	Stisknete ; a [ pro odbrzdeni brzdnych systemu.\n"+
		"4.	Pomalu zvysujte vykon stiskem D .\n\n"+
		"Jak zmenit smer\n"+
		"1.	Zastavte vlak.\n"+
		"2.	Presunte paku reverzniho kontroleru do polohy vzad nebo vpred dvojitym stiskem S.\n"+
		"3.	Odbrzdete brzdy stiskem ; (pripadne [ ).\n"+
		"4.	Pomalu zvysujte vykon stiskem D .\n\n"+
  		"Vystup a nastup cestujicich\n"+
		"1.	Zastavte ve stanici.\n"+
		"2.	Stisknete ENTER pro zahajeni vystupu a nastupu cestujicich.\n"+
		"3.	Pockejte na signal k odjezdu.\n"+
		"TIP: Pro zobrazeni casu prijezdu a odjezdu u teto a nasledujici stanice pouzijte klavesu F10.\n\n"+
		"Jak pripojit vagony/lokomotivy:\n"+
		"1.	Najedte pomalu na soupravu (optimalni rychlost 1 km/h).\n"+
		"Tip: Pro zobrazeni pohledu na sprahlo stisknete klavesu 6.\n"+
		"2.	Stisknete F9 pro otevreni okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
		"3.	Jestlize je ikona vozu cervena, je zatazena rucni brzda. Dvojtukem mysi na voze uvolnite/zatahne rucni brzdu.\n"+
		"4.	Zavrete okno sestaveni vlaku stiskem F9.\n"+
		"5.	Pockejte az odbrzdite pripojene vozy.\n\n"+
		"Odpojeni vozu nebo lokomotivy\n"+
		"POZOR! Melo by se provadet jen tehdy, pokud VLAK STOJi!\n"
		"1.	Otevrete okno sestavy vlaku F9.\n"+
		"2.	Poklepejte 2x na ikonu vozu, ktery se ma odpojit, pokud chcete, aby mel vuz zatazenou rucni brzdu.\n"+
		"3.	Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
		"4.	Zavrete okno sestaveni vlaku stiskem F9."
		"Jak doplnit naftu\n"+
		"1.	Zastavte u naftoveho stojanu stredem nadrze.\n"+
		"2.	Stisknete klavesu T a drzte ji po dobu doplnovani nafty stisknutou.\n"+
		"TIP: Pro zobrazeni prubehu plneni nadrze stisknete F9 a klepnete mysi na ikonu lokomotivy.\n\n"+
	)
	Sound ( "..\\..\\common.snd\\sndDlok\\750.7cab.sms" )
)
