SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cd_754007_old
Comment ( Upraveno pro MSTS-BIN , sprahla na 80cm )
Comment ( Pro simulaci zapnuteho topeni musite zamenit :
	    MaxPower z 1200kW na 880kW
	    MaxForce ze 190kN na 150kN
	    MaxContinuousForce ze 140kN na 120kN
	    MaxCurrent ze 4400A na 4080A
	    DieselEngineIdleRPM z 500 na 700  
	Tyto zmeny doporucuji provadet jen zkusenym ! ! !
	Puvodni soubor ENG si vzdy zalohujte ! ! ! )
	Type ( Engine )
	WagonShape ( cd_754007_old.s )
	Freightanim ( cd_754007_oldfg.s 1 1 )
	Thumbnail ( Loco.ace )
	Size ( 3.10m 4.60m 15.74m )
	CentreOfGravity ( 0m 1.5m 0m )
	Mass ( 74.4t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3.10m 4.60m 15.74m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5E6N/m 1E7N/m )
			Damping ( 1E6N/m/s 2E6N/m/s )
			Break ( 1.1E8N 5E8N )
			r0 ( 80cm 150cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Adheasion ( 0.2 0.4 4 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*74.4t )
	DerailBufferForce ( 372kN )
	NumWheels ( 4 )
	Friction (
		990.2N/m/s	-0.10	 1.4mph    12.705N/m/s	1.896
		5.1N/rad/s	 1	-1rad/s	0N/rad/s	1
	)
	PassengerCapacity ( 1 )
	BrakeEquipmentType ( "triple_valve,auxilary_reservoir,emergency_brake_reservoir" )
	BrakeSystemType ( Air_single_pipe )
	Comment ( MaxBrakeForce : P - 50 / G - 35 )
	MaxBrakeForce( 50kN )
	MaxHandbrakeForce( 18kN )
	NumberOfHandbrakeLeverSteps( 100 )
	TripleValveRatio ( 2.5 )
	Comment ( MaxReleaseRate : P - 1.4 / G - 1.0 )
	MaxReleaseRate ( 1.4 )
	Comment ( MaxApplicationRate : P - 1.2 / G - 0.8 )
	MaxApplicationRate ( 1.2 )
	EmergencyResCapacity ( 3 )
	MaxAuxilaryChargingRate ( 3 )
	EmergencyResChargingRate ( 25 )
	EmergencyBrakeResMaxPressure ( 72 )
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 40 )

	IntakePoint ( 3.33  0.4 FuelDiesel )
	IntakePoint ( 3.33 -0.4 FuelDiesel )

 	Inside (
	Comment ( Pohled na levou stranu pro predni kabinu )
		PassengerCabinFile ( cd_754007_old.s )
  		PassengerCabinHeadPos ( -1.7m 3m 6.8m )
  		RotationLimit ( 30 90 0 )
  		StartDirection ( 0 -90 0 )
 	)
	Lights ( 25
		Light (
		Comment ( Svetelny kuzel posun tma )
			Type ( 1 )
			Conditions (
			Unit ( 2 )
			Headlight ( 1 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0 2 0 )
				Transition ( 1 )
				Radius ( 30 )
				Angle ( 25 )
		)	)	)
		Light (
		Comment ( Svetelny kuzel tlumeny )
			Type ( 1 )
			Conditions (
			Unit ( 2 )
			Headlight ( 2 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0 2.5 0 )
				Transition ( 1 )
				Radius ( 100 )
				Angle ( 20 )
		)	)	)
		Light (
		Comment ( Svetelny kuzel zkraceny )
			Type ( 1 )
			Conditions (
			Unit ( 2 )
			Headlight ( 3 )
			TimeOfDay ( 1 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFFF )
				Position ( 0 2.5 0 )
				Transition ( 1 )
				Radius ( 150 )
				Angle ( 15 )
		)	)	)
		Light (
		Comment ( Svetelny kuzel plny )
			Type ( 1 )
			Conditions (
			Unit ( 2 )
			Headlight ( 3 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFFF )
				Position ( 0 2.5 0 )
				Transition ( 1 )
				Radius ( 200 )
				Angle ( 10 )
		)	)	)
		Light (
		Comment ( Predni reflektor tlumeny PK )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 2 )
			Headlight ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0 3.8 7.84 )
				Azimuth ( 0 0 0 )
				Transition ( 1 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Predni reflektor plny PK )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 2 )
			Headlight ( 3 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFFF )
				Position ( 0 3.8 7.84 )
				Azimuth ( 0 0 0 )
				Transition ( 1 )
				Radius ( 0.4 )
		)	)	)
		Light (
		Comment ( Predni reflektor TR )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 1 )
			Service ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0 3.8 7.84 )
				Azimuth ( 0 0 0 )
				Transition ( 1 )
				Radius ( 0.35 )
		)	)	)
		Light (
		Comment ( Zadni reflektor tlumeny ZK )
			Type ( 0 )
			Conditions (
			Unit ( 5 )
			Control ( 2 )
			Headlight ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0 3.8 -7.84 )
				Azimuth ( 180 180 180 )
				Transition ( 1 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni reflektor plny ZK )
			Type ( 0 )
			Conditions (
			Unit ( 5 )
			Control ( 2 )
			Headlight ( 3 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFFF )
				Position ( 0 3.8 -7.84 )
				Azimuth ( 180 180 180 )
				Transition ( 1 )
				Radius ( 0.4 )
		)	)	)
		Light (
		Comment ( Predni leve bile PK + TR )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Service ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( 0.64 1.39 7.67 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Predni leve bile posun ZK )
			Type ( 0 )
			Conditions (
			Unit ( 4 )
			Control ( 2 )
			Headlight ( 1 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( 0.64 1.39 7.67 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Predni leve cervene ZK )
			Type ( 0 )
			Conditions (
			Unit ( 4 )
			Control ( 2 )
			Headlight ( 4 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( 0.89 1.39 7.67 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Predni prave bile PK + TR )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Service ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( -0.64 1.39 7.67 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Predni prave bile posun ZK )
			Type ( 0 )
			Conditions (
			Unit ( 4 )
			Control ( 2 )
			Headlight ( 1 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( -0.64 1.39 7.67 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Predni prave cervene ZK )
			Type ( 0 )
			Conditions (
			Unit ( 4 )
			Control ( 2 )
			Headlight ( 4 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( -0.89 1.39 7.67 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Predni prave bile LC )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 1 )
			Service ( 1 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFF99 )
				Position ( -0.64 1.39 7.67 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni leve bile ZK )
			Type ( 0 )
			Conditions (
			Unit ( 5 )
			Control ( 2 )
			Service ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( 0.64 1.39 -7.67 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni leve bile posun PK )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 2 )
			Headlight ( 1 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( 0.64 1.39 -7.67 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni leve cervene PK )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 2 )
			Headlight ( 4 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( 0.89 1.39 -7.67 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni leve cervene TR )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 1 )
			Service ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( 0.89 1.39 -7.67 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni leve bile LC )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 1 )
			Service ( 1 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFF99 )
				Position ( 0.64 1.39 -7.67 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni prave bile ZK )
			Type ( 0 )
			Conditions (
			Unit ( 5 )
			Control ( 2 )
			Service ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( -0.64 1.39 -7.67 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni prave bile posun PK )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 2 )
			Headlight ( 1 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( -0.64 1.39 -7.67 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni prave cervene PK )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 2 )
			Headlight ( 4 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( -0.89 1.39 -7.67 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni prave cervene TR )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 1 )
			Service ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( -0.89 1.39 -7.67 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.3 )
	)	)	)	)
	Sound ( "../../common.snd/snd754/754eng.sms" )
)
Engine ( cd_754007_old
	Effects (
		DieselSpecialEffects (
			Exhaust1 (  0.25 4.65 2.25 0 1 0 0.3 )
			Exhaust2 ( -0.25 4.65 2.25 0 1 0 0.3 )
	)		)
	Wagon ( cd_754007_old )
	Type ( Diesel )
	MaxPower ( 1200kW )
	MaxForce ( 190kN )
	MaxContinuousForce ( 140kN )
	MaxVelocity ( 100km/h )
	RunUpTimeToMaxForce ( 18 )
	MaxCurrent ( 4400A )
	WheelRadius ( 0.5m )
	Sanding ( 15km/h )
	MaxSandingTime ( 900 )
	NumWheels ( 4 )
	MaxTemperature ( 120 )
	MaxOilPressure ( 90 )

	CabView ( "../../common.cab/cab754/754cd_green.cvf" )
	HeadOut ( 1.7 3 6.8 )

	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 0.5 )
	AirBrakesIsCompressorElectricOrMechanical ( 1 )
	AirBrakesCompressorRestartPressure ( 122 )
	AirBrakesAirCompressorPowerRating ( 4 )
	AirBrakesAirCompressorWattage ( 19000 )
	AirBrakesMainMinResAirPressure ( 50 )
	AirBrakesMainMaxAirPressure ( 145 )
	AirBrakesHasLowPressureTest ( 0 )
	AirBrakesMainResVolume ( 40 )

	EngineBrakesControllerEmergencyApplicationRate ( 40 )
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	EngineBrakesControllerFullServicePressureDrop ( 24 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesControllerMinPressureReduction ( 6 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 1.5 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxReleaseRate ( 2.5 )
      EngineBrakesProportionalBrakeLag( 0.5 )

	TrainBrakesControllerEmergencyApplicationRate( 40 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainBrakesControllerFullServicePressureDrop( 24 )
	TrainBrakesControllerMinPressureReduction( 6 )
	TrainBrakesControllerMaxApplicationRate( 1.5 )
	TrainBrakesControllerMaxSystemPressure( 73 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxReleaseRate( 2.0 )

	BrakesEngineControllers ( "Train,Independent" )
	BrakeCutsPowerAtBrakeCylinderPressure ( 15 )
	BrakesEngineBrakeType ( Air_single_pipe )
	BrakesTrainBrakeType ( Air_single_pipe )
	DoesHornTriggerBell ( 0 )
	DoesBrakeCutPower ( 1 )

	DieselEngineType ( Electric )
	DieselUsedPerHourAtMaxPower ( 210l )
	DieselUsedPerHourAtIdle ( 21l )
	EngineVariables ( 3600l )

	DieselEngineSpeedOfMaxTractiveEffort ( 35km/h )
	DieselSmokeEffectInitialMagnitude ( 0.8 )
	DieselSmokeEffectInitialSmokeRate ( 0.5 )
	DieselSmokeEffectMaxMagnitude ( 1.2 )
	DieselSmokeEffectMaxSmokeRate ( 1.5 )
	DieselEngineMaxRPMChangeRate ( 50 )
	DieselEngineIdleRPM ( 500 )
	DieselEngineMaxRPM ( 1150 )

	EmergencyStopMonitor (
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
	)
	VigilanceMonitor (
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
		MonitoringDeviceMonitorTimeLimit ( 48 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 35 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
	)
	OverspeedMonitor(
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 2 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 67.11 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceResetOnResetButton ( 0 )
		MonitoringDeviceCriticalLevel ( 62.14 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDeviceResetLevel ( 0 )
	)
	EngineControllers (
		Brake_Engine ( 0 1 0.125 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
		)		)
		Brake_Hand ( 0 1 0.1 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
		)		)
		Brake_Train ( 0 1 0.055 0.8
			NumNotches ( 5
				Notch ( 0.00	0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.40	0 TrainBrakesControllerReleaseStart )
				Notch ( 0.60	0 TrainBrakesControllerApplyStart )
				Notch ( 0.80	0 TrainBrakesControllerContinuousServiceStart )
				Notch ( 0.99	0 TrainBrakesControllerEmergencyStart )
		)		)
		Throttle ( 0 1 0.05 0
			NumNotches ( 0 )
		)
		EmergencyStopToggle ( 0 1 0 )
		Headlights ( 0 0.25 1 0 )
		DirControl ( -1 0 1 1 )
		BailOffButton ( 0 1 0 )
		BellToggle ( 0 1 0 )
		Vigilance ( 0 1 0 )
		Sanding ( 0 1 0 )
		Wipers ( 0 1 0 )
		Horn ( 0 1 0 )
		AWS ( 0 1 0 )
	)
	Sound ( "../../common.snd/snd754/754cab.sms" )
	MaxDieselLevel ( 996l )
	Name ( "CD 754.007-3 Old" )

	Description (
		"Lokomotiva CD 754.007-3 , DKV Brno .\n"+
		"Upraveno pro MSTS-BIN.\n"+
		"Rada CD 754 je univerzalni dieselelektricka skrinova lokomotiva, pouzivana v osobni i nakladni doprave.\n"+
		"Lokomotiva je vybavena generatorem 3000V pro vytapeni vlakovych souprav.\n"+
		"Prenos vykonu: elektricky.\n"+
		"Zdroj vykonu: naftovy motor CKD K 12 V 230 DR .\n"+
		"Max. vykon motoru: 1470 kW.\n"+
		"Max. trakcni vykon: 1200 kW.\n"+
		"Max. vyska: 4.5 m.\n"+
		"Max. sirka: 3.1 m.\n"+
		"Delka pres narazniky: 16.5m.\n"+
		"Hmotnost: 74.4 t.\n"+
		"Max. rychlost: 100 km/h."
	)
	EngineOperatingProcedures (
		"Lokomotiva CD 754.044-6 , DKV Praha .\n"+
		"Upraveno pro MSTS-BIN. Max.rychlost: 100 km/h . \n"+
		"POZOR ! Aktivace zachranne brzdy pri prekroceni 100 km/h.\n"+
		"Jak se rozjet : \n"+
		"1.Stisknete W na prestaveni reverzniho kontoleru do polohy 'vpred'.\n"+
		"2.Stisknete a drzte ; pro odbrzdeni vlakove brzdy.\n"+
		"3.Stisknete a drzte [ pro odbrzdeni lokomotivni brzdy.\n"+
		"4.Stisknete D pro zvyseni pozadovaneho vykonu.\n"+
		"5.Pomalu zvysujte vykon stiskem D, dokud vlak nedosahne pozadovane rychlosti\n"+
		"Jak zpomalit : \n"+
		"1.Stisknete A pro snizeni pozadovaneho vykonu (postupne az na 0).\n"+
		"2.Jestlize je to nutne tak pouzijte brzdy pro postupne rychlejsi snizovani rychlosti.\n"+
		"Jak pouzit vlakovou brzdu : \n"+
		"1.Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosahnete pozadovaneho brzdneho tlaku.\n"+
		"2.Po dosazeni pozadovaneho brzd. tlaku stiskem ; presunte rukojet brzdy do polohy ZAVER.\n"+
		"Jak odbrzdit vlakovou brzdu : \n"+
		"1.Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENÍ.\n"+
		"2.Pockejte, az klesne tlak v brzdovych valcich na 0.\n"+
		"3.Stisknete ' pro presunuti rukojeti brzdy do polohy ZAVER.\n"+
		"Jak pouzit lokomotvni brzdu : \n"+
		"1.Stisknete a drzte ] pro zabrzdeni lokomotivni brzdy (0-100%).\n"+
		"Jak odbrzdit lokomotivni brzdu\n"+
		"1.Stisknete a drzte [ pro odbrzdeni lokomotivni brzdy.\n"+
		"Jak pouzit zachrannou brzdu : \n"+
		"1.Stisknete a drzte A pro snizeni vykonu az na 0.\n"+
		"2.Stisknete BACKSPACE pro aktivaci zachrane brzdy.\n"+
		"Jak zrusit zachrannou brzdu : \n"+
		"1.Pockejte na úplne zastaveni vlaku.\n"+
		"2.Stisknete Z pro odblokovani ovladani lokomotivy.\n"+
		"3.Stisknete ; a [ pro odbrzdeni brzdnych systemu.\n"+
		"4.Pomalu zvysuj vykon stiskem D .\n"+
		"Vystup a nastup cestujicich : \n"+
		"1.Zastavte ve stanici.\n"+
		"2.Stisknete ENTER.\n"+
		"3.Pockejte na signal k odjezdu.\n"+
		"TIP: Pro zobrazeni casu prijezdu a odjezdu u teto a nasledujici stanice pouzijte klavesu F10.\n"+
		"Jak zmenit smer : \n"+
		"1.Zastavte.\n"+
		"2.Presunte paku reverzniho kontroleru do polohy vzad dvojitym stiskem S.\n"+
		"3.Odbrzdete brzdy.\n"+
		"4.Pomalu zvysujte vykon stiskem D .\n"+
		"Jak zmenit ridici stanoviste : \n"+
		"1.Zastavte.\n"+
		"2.Presunte paku reverzniho kontroleru do polohy nezarazeno stiskem S.\n"+
		"3.Zabrzdete vlakovou brzdu.\n"+
		"4.Stisknete 1.\n"+
		"Jak prejit na jinou lokomotivu ve vlaku : \n"+
		"1.Zastavte.\n"+
		"2.Presunte paku reverzniho kontroleru do polohy nezarazeno stiskem S.\n"+
		"3.Zabrzdete vlakovou brzdu.\n"+
		"4.Stisknete F9 pro otevreni okna se seznamem lokomotiv a vozu ve vlaku.\n"+
		"5.Oznacte lokomotivu mysi a stisknete 1.\n"+
		"6.Stisknete F9 pro zavreni okna se seznamem lokomotiv a vozu ve vlaku.\n"+
		"Jak zmenit pohled cestujiciho z jineho os.vozu : \n"+
		"1.Stisknete F9 pro otevreni okna se seznamem lokomotiv a vozu ve vlaku.\n"+
		"2.Oznacte vuz se svetle modre podbarvenymi okny mysi a stisknete 5.\n"+
		"3.Stisknete F9 pro zavreni okna se seznamem lokomotiv a vozu ve vlaku.\n"+
		"Jak pripojit vozy/lokomotivy : \n"+
		"1.K vozu musite prijet velmi pomalu, posledni 2 m nizsi rychlosti nez 1 km/h.\n"+
		"Tip: Pro zobrazeni pohledu na sprahlo stisknete klavesu 6.\n"+
		"2.Stisknete F9 pro otevreni okna se seznamem lokomotiv a vozu ve vlaku.\n"+
		"3.Jestlize je ikona vozu cervena, je zatazena rucni brzda. Dvojtuk mysi na voze uvolni/zatahne rucni brzdu.\n"+
		"4.Zavrete okno sestaveni vlaku stiskem F9.\n"+
		"Odpojeni vozu nebo lokomotivy : \n"+
		"POZOR! Melo by se provadet jen tehdy, pokud VLAK STOJI!\n"+
		"1.Otevrete okno sestavy vlaku [F9].\n"+
		"2.Poklepejte 2x na ikonu vozu, ktery (-e) se ma(ji) odpojit, pokud chcete, aby mely zatazenou ruc. brzdu.\n"+
		"3.Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
		"4.Zavrete okno sestaveni vlaku stiskem F9.\n"+
		"5.Pomalu odjedte od odpojenych vozu na 1-2 m a pak jiz muzete zvysit rychlost.\n"+
		"TIP : Pri znovu spojeni vozu postup opakujte a odjizdejte od odpojenych vozu pomaleji.\n"+
		"Jak doplnit naftu :\n"+
		"1.Zastavte u naftoveho stojanu stredem nadrze.\n"+
		"2.Stisknete klavesu T a drzte ji po dobu doplnovani nafty stisknutou.\n"+
		"TIP: Pro zobrazeni prubehu plneni nadrze stisknete F9 a klepnete mysi na ikonu lokomotivy. "
	)	)
