SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( zssk_750032_2014



Comment ( "Sekce vozidlo" )
Comment ( "Popis fyziky vozu pro OR" )
Comment ( "Bez parniho agregatu, dobalastovano" )
Comment ( "Josef Vogeltanz - 26.07.2018" )
Comment ( "Uprava - 02.03.2021" )



Comment ( "Obecne informace vozu" )
Type ( Engine )
WagonShape ( zssk_750032_2014.s )

Size ( 3.096m 4.605m 16.54m )
Mass ( 74t )
WheelRadius ( 0.5m )
ORTSNumberAxles ( 0 )

ORTSFreightAnims (
MSTSFreightAnimEnabled ( 1 )
FreightAnimStatic (
SubType ( Default )
Shape ( zssk_750032_2014fg.s )
Offset ( 0.0, 0.0, 0.0 )
Flip ( 0 )
)
)

Comment ( "Sprahla" )
Coupling (
Type ( Chain )
Spring ( Stiffness (  6.7e6N/m 4.4e8N/m ) Break ( 850kN 850kN ) r0 ( 0cm 2.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Coupling (
Type ( Chain )
Spring ( Stiffness (  6.7e6N/m 4.4e8N/m ) Break ( 850kN 850kN ) r0 ( 0cm 2.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )


BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

Comment ( Brzda v režimu G - nákladní )

	MaxBrakeForce( 75kN )
	MaxHandbrakeForce( 14kN )
	NumberOfHandbrakeLeverSteps( 100 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 2.5 )
	MaxApplicationRate( 2.5 )
	MaxAuxilaryChargingRate( 3 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
        EmergencyResVolumeMultiplier ( 11 )
        EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 ) 

ORTSBrakeShoeFriction (
0   0.310
8   0.238
16  0.193
24  0.168
32  0.152
40  0.140
48  0.131
56  0.123
64  0.116
72  0.109
80  0.105
88  0.101
96  0.098
104 0.096
112 0.094
120 0.093
128 0.092
136 0.092
144 0.092
152 0.092
160 0.092
)

Comment ( "Jizdni odpory a treni" )
CentreOfGravity ( 0m 2.3m  0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 2m 400mm )
ORTSUnbalancedSuperelevation ( 150mm )

ORTSBearingType ( Roller )
ORTSDavis_A ( 987.6 )
ORTSDavis_B ( 24.34 )
ORTSDavis_C ( 6.325 )
ORTSWagonFrontalArea ( 12.1m^2 )

ORTSAdhesion (
ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
ORTSSlipWarningThreshold ( 60 )
)

ORTS3DCab (
ORTS3DCabFile ( "..//..//common.cab//3DCab750//cab750.s" )
ORTS3DCabHeadPos ( 0.76 3.1 6.1 )
RotationLimit ( 40 60 0 )
StartDirection ( 12 0 0 )
)

ORTS3DCab (
ORTS3DCabFile ( "..//..//common.cab//3DCab750//cab750.s" )
ORTS3DCabHeadPos ( -0.76 3.1 -6.1 )
RotationLimit ( 40 60 0 )
StartDirection ( 12 180 0 )
)

Comment ( Dve pozicky + stary reflektor )

Lights ( 23
		Light (
			comment ( Svetelny kuzel dialkovy )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFF9FFFF )
					Position ( 0 3.6 7.82 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 50 )
				)
			)
		)
		Light (
			comment ( Svetelny kuzel tlmeny )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE58F )
					Position ( 0 3.6 7.82 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 20 )
				)
			)
		)
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( Reflektor plny )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5  )
			FadeOut ( 0.5  )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.0 3.797 7.82 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.8 )
				)
			)
		)
                 Light (
			comment ( Reflektor tlmeny )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5  )
			FadeOut ( 0.5  )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFDFB17F )
					Position ( 0.0 3.797 7.82 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		
		Light (
			comment ( predne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.76 1.389 7.66 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( predne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.76 1.389 7.66 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadne lave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.76 1.389 -7.66 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadne prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.76 1.389 -7.66 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		comment ( Definicia svetiel pre zadne stanoviste )

		Light (
			comment ( Reflektor plny )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5  )
			FadeOut ( 0.5  )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.0 3.797 -7.82 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 1.8 )
				)
			)
		)
                Light (
			comment ( Reflektor tlmeny )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5  )
			FadeOut ( 0.5  )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFDFB17F )
					Position ( 0.0 3.797 -7.82 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		Light (
			comment ( predne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.76 1.389 -7.66 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( predne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.76 1.389 -7.66 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadne lave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( 0.76 1.389 7.66 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadne prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( -0.76 1.389 7.66 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                comment ( Definicia svetiel pre posunujuci diel )

		Light (
			comment ( Predne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.76 1.389 7.66 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Zadne lave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.76 1.389 -7.66 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		
		comment ( Definicia svetiel pre Loose consist )

		Light	(
			comment( Predne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.76 1.389 7.66 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( Zadne lave pozicne)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.76 1.389 -7.66 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		

		comment ( Definicia svetiel pre PC )

		Light (
			comment ( Predne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.76 1.389 7.66 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Predne lave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.76 1.389 7.66 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Reflektor tlmeny )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFDFB17F )
					Position ( 0.0 3.797 7.82 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		Light (
			comment ( Zadne lave pozicne )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( -0.76 1.389 -7.66 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Zadne prave pozicne )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( 0.76 1.389 -7.66 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)
	
Comment ( "Ostatni informace" )
Sound ( "..//..//common.snd//snd754//750eng.sms" )
IntakePoint ( 0 2 FuelDiesel )
)


Engine ( zssk_750032_2014
Wagon ( zssk_750032_2014  )
Name ( "ZSSK 750 032-5 2014" )


Effects (
DieselSpecialEffects (
Exhaust1 ( -0.23 4.63 2.23 0 1 0 0.2 )
Exhaust2 ( 0.23 4.63 2.23 0 1 0 0.2 )
)
)


Type ( Diesel )
MaxVelocity ( 110km/h )
WheelRadius ( 0.5m )
Sanding ( 35km/h )
ORTSNumberDriveAxles ( 4 )
ORTSDriveWheelWeight ( 76.8t )
ORTSSpeedOfMaxContinuousForce ( 35km/h )
MaxForce ( 928kN )
MaxContinuousForce ( 928kN )
MaxPower ( 1325kW )
MaxDieselLevel ( 2500l )
DieselEngineType ( electric )
MaxCurrent ( 20000A )



Comment ( "Agregat" )
ORTSDieselEngines ( 1
Diesel (
IdleRPM ( 480 )
MaxRPM ( 1100 )
StartingRPM ( 321 )
StartingConfirmRPM ( 528 )
ChangeUpRPMpS ( 100 )
ChangeDownRPMpS ( 75 )
RateOfChangeUpRPMpSS ( 10 )
RateOfChangeDownRPMpSS ( 10 )
MaximalPower ( 1325kW )
IdleExhaust ( 4 )
MaxExhaust ( 11 )
ExhaustDynamics ( 1.2 )
ExhaustDynamicsDown ( 0.5 )
ExhaustColor ( 00999792 )
ExhaustTransientColor ( FF5B5851 )
DieselPowerTab (
0 0
480 79500
500 132500
530 218625
600 397500
700 632688
810 871188
910 1036813
1000 1185875
1100 1325000
)
DieselConsumptionTab (
0 0
480 31.5
500 57.7
530 78.7
600 98
700 122.5
810 157.5
910 224.1
1000 280.1
1100 350.1
)
ThrottleRPMTab (
0 480
3 500
8 530
19 600
35 700
53 810
69 910
84 1000
100 1100
)
DieselTorqueTab (
0 0
480 7338
1100 8783
)
MinOilPressure ( 200kPa )
MaxOilPressure ( 600kPa )
MaxTemperature ( 85 )
Cooling ( 3 )
TempTimeConstant ( 720 )
OptTemperature ( 70 )
IdleTemperature ( 60 )
)
)



BrakesTrainBrakeType ( "Air_single_pipe" )
BrakesEngineControllers ( "Independent, Train" )



comment (1x kompresor 3DSK 100 a tlaky v jimkach, vlastnosti potrubi)

	AirBrakesMainMaxAirPressure( 10bar )
	AirBrakesCompressorRestartPressure( 7.5bar )
	AirBrakesMainResVolume( 900l )
	ORTSMainResChargingRate ( 0.04bar/s )
	ORTSBrakePipeChargingRate ( 4.6bar/s )

	comment (unik vzduchu netesnosti brzdoveho potrubi)
	TrainPipeLeakRate ( 0.00066bar/s )

	ORTSBrakePipeTimeFactor ( 0.003 )
	ORTSBrakeServiceTimeFactor ( 1.009 )
	ORTSBrakeEmergencyTimeFactor ( 0.1 )




	comment ( Lokomotivní (přímočinná) brzda typ DAKO BP)

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 22 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )




	comment ( Vlaková (samočinná) brzda typ DAKO BS2)

	TrainBrakesControllerMinPressureReduction ( 3 )
	TrainBrakesControllerMaxApplicationRate ( 0.2bar/s )
	TrainBrakesControllerMaxReleaseRate ( 0.2bar/s )
	TrainBrakesControllerMaxQuickReleaseRate ( 0.4bar/s )
	TrainBrakesControllerEmergencyApplicationRate ( 0.8bar/s )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 5bar )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )

	TrainPipeLeakRate ( 0.033 )
	TrainBrakesControllerFullServicePressureDrop ( 5bar )


Comment ( "Ovladani jizdy" )

Comment ( "Vlakovy zabezpecovac - pouze KBS" )
VigilanceMonitor (
MonitoringDeviceMonitorTimeLimit ( 16 )
MonitoringDeviceAlarmTimeLimit ( 6 )
MonitoringDevicePenaltyTimeLimit ( 0 )
MonitoringDeviceCriticalLevel ( 0 )
MonitoringDeviceResetLevel ( 0 )
MonitoringDeviceAppliesFullBrake ( 0 )
MonitoringDeviceAppliesEmergencyBrake ( 1 )
MonitoringDeviceAppliesCutsPower ( 1 )
MonitoringDeviceAppliesShutsDownEngine ( 0 )
MonitoringDeviceResetOnResetButton ( 1 )
MonitoringDeviceResetOnZeroSpeed ( 1 )
)


Comment ( "Rizeni" )

EngineControllers (
Throttle ( 0 1 0.125 0
NumNotches ( 9
Notch ( 0 0 Dummy )
Notch ( 0.03 0 Dummy )
Notch ( 0.08 0 Dummy )
Notch ( 0.19 0 Dummy )
Notch ( 0.35 0 Dummy )
Notch ( 0.53 0 Dummy )
Notch ( 0.69 0 Dummy )
Notch ( 0.84 0 Dummy )
Notch ( 1.00 0 Dummy )
)
)

Comment ( "Primocinna brzda typu DAKO BP" )
Brake_Engine ( 0 1 0.2 0.8
NumNotches  ( 1 
Notch ( 0 1 Dummy ) )
)

Comment ( "Prubezna brzda typ DAKO-BS2" )
Brake_Train ( 0 1 0.06 0.21
NumNotches ( 8
Notch ( 0 0 TrainBrakesControllerFullQuickReleaseStart )
Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
Notch ( 0.95 0 TrainBrakesControllerNeutralhandleOffStart )
Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
)
)

Brake_Hand ( 0 1 0.025 0
NumNotches ( 0 )
)

DirControl ( -1 0 1 1 )
Sanding ( 0 1 0 )
Horn ( 0 1 0 )
Wipers ( 0 1 0 )
EmergencyStopToggle ( 0 1 1 )
Vigilance ( 0 1 0 )
Headlights ( 0 0.25 1 0 )
)

Comment ( "Ostatni informace" )
Sound ( "..//..//common.snd//snd754//750cab.sms" )
CabView ( "..//..//common.cab//3DCab750//cab750.cvf" )
HeadOut ( 1.7 3.2 6.45 )

Comment ( "Poznamky" )
Description (
"Pokyny pro obecne nastaveni OR:\n"+
"-> Karta Obecne: Rychlost plneni brzdoveho potrubi 1000 PSI/s (nutne aby OR akceptoval hodnoty engu!)\n"+
"-> Karta Simulace: Pokrocily model adheze\n"+
"-> Karta Experimentalni: Faktor korekce adheze 100%\n"+
"-> Karta Experimentalni: Nahodna zmena faktoru adheze 10%\n\n"+ 
"Rada 750 CD je dieselelektricka skrinova lokomotiva, pouzivana dnes uz vetsinou jen v nakladni doprave.\n\n"+
"Lokomotivy vznikly jako rekonstrukce rady 753 nahrazenim parniho generatoru topnym alternatorem.\n\n"+
"Prenos vykonu: elektricky\n\n"+
"Zdroj vykonu: naftovy motor CKD K 12 V 230 DR\n\n"+
"Max. vykon motoru: 1325 kW\n\n"+
"Max. trakcni vykon: 1200 kW\n\n"+
"Max. vyska: 4,335 m\n\n"+
"Max. sirka: 3,074 m\n\n"+
"Delka pres narazniky: 16,540 m\n\n"+
"Hmotnost: 76,8 t\n\n"+
"Max. rychlost: 100 km/h"
)

EngineOperatingProcedures (
"Viz. manual Open Rails.\n\n"+
"TIP: V prubehu jizdy pomoc na klavese F1."
)
)