SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cd_163070_hk
	Comment ( verze: 8.10.2006 definice svetel MSTS Bin )
	
        Comment ( Verze: 1.19 )
        Comment ( Datum: 6/4/2009 )
        Comment ( Uprava vykonove charakteristiky - plocha do 60 kmh dle skutecnosti )
        Comment ( Mez adhese: 182kN )
        Comment ( Antislip odstranen )
        Comment ( Uprava kompletnich brzd + nastaveni do polohy P 44kN, pro N je 24kN )
        Comment ( Trvala tazna sila: 173 kN = 715 A = 65% polohy ridiciho kontroleru )
        Comment ( Od B57 pridana EDB nereverzni )	
	
	Type ( Engine )
	WagonShape ( "cd_163070_hk.s" )
    Freightanim ( cd_163070fg_hk.s 1 1 ) 
	Size ( 3.00m 4.69m 16.556m )
	CentreOfGravity ( 0m 2.25m 0m )
	Mass ( 84t )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box (3.00m 4.69m 16.556m) )
Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Adheasion ( 0.114 0.77 1.3 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 307.5kN )
	DerailBufferForce ( 300kN )
	NumWheels ( 4 )
	Friction (
		1070.5N/m/s    -0.10    1.3mph    12.951N/m/s    1.891
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	)
	Comment ( AntiSlip () )
	
	MaxBrakeForce( 44kN )
	MaxHandbrakeForce( 8kN )
	NumberOfHandbrakeLeverSteps( 100 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 1.3 )
	MaxApplicationRate( 10 )
	MaxAuxilaryChargingRate( 3 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
        EmergencyResVolumeMultiplier ( 11 )
        EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 )

comment	( Lights )
	Lights ( 28
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFFF )
					Position ( 0 1 8 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 120 )
				)
			)
		)
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.73 1.68 7.82 )
					Azimuth ( 0.0 0.0 0.0 )
                                        Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.73 1.68 7.82 )
					Azimuth ( 0.0 0.0 0.0 )
                                        Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                Light (
			comment ( Horna LED )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFE0FFFF )
					Position ( 0.0 2.59 7.91 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.6 )
				)
			)
		)
                Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( -0.98 1.68 7.82 )
					Azimuth ( 0.0 0.0 0.0 )
                                        Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( 0.98 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 -7.86 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 -7.86 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )
                 
		Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.73 1.68 -7.86 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.73 1.68 -7.86 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                Light (
			comment ( Horna LED )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFE0FFFF )
					Position ( 0.0 2.59 -7.91 )
					Azimuth ( 180 180 180 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.6 )
				)
			)
		)
                Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( 0.98 1.68 -7.86 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( -0.98 1.68 -7.86 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                comment ( Definicia svetiel pre posunujuci diel )
                Light (
			comment ( Prední lave pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( -0.98 1.68 7.82 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( 0.98 1.68 7.82 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( -0.98 1.68 -7.86 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní prave pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( 0.98 1.68 -7.86 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		comment ( Definice svetel pro Loose consist )
                Light	(
			comment( Pravé přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( 0.98 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                Light	(
			comment( Lave přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( -0.98 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light	(
			comment( Levé zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( -0.98 1.68 -7.86 )
                                        Elevation ( 10 10 10 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                Light	(
			comment( Prave zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFE0FFFF )
					Position ( 0.98 1.68 -7.86 )
                                        Elevation ( 10 10 10 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( PC prední pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFE0FFFF )
					Position ( 0.98 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( PC prední levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFE0FFFF )
					Position ( -0.98 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                Light (
			comment ( PC horna LED)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFE0FFFF )
					Position ( 0.0 2.59 7.91 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 -7.83 )
                                        Elevation ( -10 -10 -10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 -7.83 )
                                        Elevation ( -10 -10 -10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
	)

	Sound ( "..\\..\\common.snd\\sndX6X\\163IIeng.sms" )
)

Engine ( cd_163070_hk
	Wagon ( "cd_163070_hk" )
	Type ( Electric )
	MaxPower ( 3480kW )
	MaxForce ( 266kN )
	MaxContinuousForce ( 266kN )
	MaxVelocity ( 132km/h )
	DieselEngineSpeedOfMaxTractiveEffort	( 41.44mph )    
	MaxCurrent ( 1100A )
	WheelRadius ( 0.625m )
	Sanding ( 40km/h )
	MaxSandingTime ( 600 )
	NumWheels ( 4 )

	HeadOut ( 1.6 3.0 6.6 )

	AirBrakesAirCompressorPowerRating ( 1.18 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 144 )	
	AirBrakesMainResVolume ( 31.78 )
	AirBrakesAirCompressorWattage ( 15000 )
	AirBrakesCompressorRestartPressure ( 121 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 3 )
	TrainBrakesControllerMaxApplicationRate ( 1.7 )
	TrainBrakesControllerMaxReleaseRate ( 1.5 )
	TrainBrakesControllerMaxQuickReleaseRate ( 2.5 )
	TrainBrakesControllerEmergencyApplicationRate ( 2.5 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )

	TrainPipeLeakRate ( 0.033 )
	TrainBrakesControllerFullServicePressureDrop ( 73 )

comment ( EDB s reverzem
	DynamicBrakesMaximumForce						( 140kN )
	DynamicBrakesResistorCurrentLimit				( 715 )
	DynamicBrakesDelayTimeBeforeEngaging			( 0 )
	DynamicBrakesNumberOfControllerNotches			( 20 )
	DynamicBrakesMaxAirBrakePressure				( 20 )
	DynamicBrakeHasAutoBailOff						( 1 )

	DynamicBrakesMaximumSpeedForFadeOut				( 137 )
	DynamicBrakesMaximumEffectiveSpeed				( 50 )
	DynamicBrakesHigherSpeedCurveExponent			( 1 )
	DynamicBrakesEffectAtMaximumFadeOut				( 0 )
	DynamicBrakesLowerSpeedCurveExponent			( 1 )
	DynamicBrakesCutInSpeed							( -50 )
	DynamicBrakesFadingSpeed						( -50 )
	DynamicBrakesMinUsableSpeed						( -137 )
konec komentu )

comment ( EDB bez reverzu )
	DynamicBrakesMaximumForce	 ( 118kN )
	DynamicBrakesResistorCurrentLimit	 ( 715 )
	DynamicBrakesDelayTimeBeforeEngaging	 ( 2 )
	DynamicBrakesNumberOfControllerNotches	 ( 20 )
	DynamicBrakesMaxAirBrakePressure	 ( 100 )
	DynamicBrakeHasAutoBailOff	 ( 0 )

	DynamicBrakesMaximumSpeedForFadeOut	 ( 100 )
	DynamicBrakesMaximumEffectiveSpeed	 ( 50 )
	DynamicBrakesHigherSpeedCurveExponent	 ( 1 )
	DynamicBrakesEffectAtMaximumFadeOut	 ( 2 )
	DynamicBrakesLowerSpeedCurveExponent	 ( 1 )
	DynamicBrakesCutInSpeed	 ( 8 )
	DynamicBrakesFadingSpeed	 ( 8 )
	DynamicBrakesMinUsableSpeed	 ( 3 )

	BrakesEngineBrakeType( "Air_single_pipe" )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train, Dynamic, Blended" )
	
	DoesBrakeCutPower ( 1 )

	CabView ( "..\\..\\common.cab\\cab163cd\\cd_163.cvf" )

	DoesHornTriggerBell ( 0 )

EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 20 )
		MonitoringDeviceAlarmTimeLimit ( 10 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 77.5 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 77.6 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 0 )
	)

	EngineControllers (
		AWS ( 0 1 0 )
		BailOffButton 	( 0 1 0 )
		BellToggle 	( 0 1 0 )
		Brake_Dynamic 	( 0 1 0.1 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		Brake_Engine 	( 0 1 0.1 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		Brake_Hand 	( 0 1 0.1 0
			NumNotches ( 0 )
		)
		Brake_Train 	( 0 1 0.05 0.8
			NumNotches ( 5
				Notch ( 0 0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.4 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.6 0 TrainBrakesControllerApplyStart )
				Notch ( 0.8 0 TrainBrakesControllerContinuousServiceStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)
		Throttle 	( 0 1 0.05 0
			NumNotches ( 0 )
		)
		DirControl 		( -1 0 1 1 )
		EmergencyStopToggle	( 0 1 0 )
		Headlights 		( 0 0.5 1 0 )
		Horn 			( 0 1 0 )
		PantographToggle1	( 0 1 0 )
	        PantographToggle2	( 0 1 0 )
	        PantographsToggle_4	( 0 1 0 ) 
		Sanding 		( 0 1 0 )
		Vigilance 		( 0 1 0 )
		Wipers 			( 0 1 0 )
	)

	Name ( "CD 163 070-6 HK" )
	Sound ( "..\\..\\common.snd\\sndX6X\\163IIcabCD.sms" )

	Description (
		"Rada ZSSK 163 je univerzalni elektricka skrinova lokomotiva, pouzivana v osobni a nákladní doprave.\nTyp Bo'-Bo', napeti 3kV ss , 25kV 50Hz str.\n\nDelka pres narazniky: 16,8 m\n\nPrumer hnacich kol: 1250 mm\n\nHmotnost ve sluzbe: 87 t\n\n" +
		"Trvaly vykon trakcnich motoru: 3480 kW ss , 3060kW str.\n\n" +
		"Max. rychlost 120 km/h\n" +
		""
	)
)
