SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cdc_182168
	Type ( Engine )
	WagonShape ( cdc_182168.s )

	Comment ( Model: Pikku 2009 )
  Comment ( Textury Acatus na skin od Pikku, mates.zscs )
  Comment ( Popis fyziky vozu pro OR )
	Comment ( Sberace: 2 )
	Comment ( Eng je vykonostni charakteristiku vhodny pro radu 181.001 - 181.080 )
	Comment ( Eng obsahuje ovladani dvou sberacu )
	Comment ( nastaveni Engu Josef Vogeltanz - 03.02.2020" , upraveno 2020-03-22-b57, klon ze 181.008 Acatus - 2020-10-12 )
	
comment	( Overall physics )

	Size ( 3.2m 4.7m 18.8m )
	Mass ( 120t )
  CentreOfGravity ( 0m 2.25m 0m )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box (3.15m 4.71m 18.46m) )
  
comment	( Coupling )

	Coupling (
	Type ( Chain )
  Spring ( Stiffness ( 4e5N/m 2.64e7N/m ) Break ( 8.5e5N 8.5e5N ) r0 ( 0cm 2.5cm ) )
  CouplingHasRigidConnection ( 0 )
  Velocity ( 0.01m/s ) )

  Coupling (
  Type ( Chain )
  Spring ( Stiffness ( 4e5N/m 2.64e7N/m ) Break ( 8.5e5N 8.5e5N ) r0 ( 0cm 2.5cm ) )
  CouplingHasRigidConnection ( 0 )
  Velocity ( 0.01m/s ) )
	
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	

Comment ( "Brzdy" )
Comment ( "Brzdovy system DAKO, zdrze, Bv.: 66t" )
Comment ( "Rezim brzdeni P" )
BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

MaxBrakeForce ( 201kN )
MaxHandbrakeForce ( 75kN )
NumberOfHandbrakeLeverSteps ( 10 )

TripleValveRatio ( 2.53 )
MaxReleaseRate ( 0.212bar/s )
MaxApplicationRate ( 0.475bar/s )
MaxAuxilaryChargingRate ( 0.405bar/s )
EmergencyResChargingRate ( 0.405bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 3.8bar )
EmergencyResVolumeMultiplier ( 1.0 )
EmergencyResCapacity ( 300l )
BrakePipeVolume ( 16.3l )

ORTSBrakeShoeFriction ( 
0 0.31 
1 0.30 
2 0.28 
3 0.27 
4 0.26 
5 0.25 
7 0.24 
8 0.23 
9 0.22 
12 0.21 
14 0.20 
17 0.19 
20 0.18 
24 0.17 
29 0.16 
34 0.15 
40 0.14 
47 0.13 
55 0.12 
66 0.11 
84 0.10 
115 0.09 
160 0.09 
 )

Comment ( "Jizdni odpory a treni" )
CentreOfGravity ( 0m 2.35m  0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 4m 800mm )
ORTSUnbalancedSupErelevation ( 150mm )
ORTSTrackSuperElevation (
0.0 0.0
80.0 20.0
90.0 26.7
100.0 33.3
110.0 40.0
120.0 46.7
130.0 53.3
140.0 60.0
150.0 66.7
160.0 73.3
170.0 80.0
180.0 86.7
190.0 93.3
200.0 100.0
210.0 106.7
220.0 113.3
230.0 120.0
240.0 126.7
250.0 133.3
260.0 140.0
270.0 146.7
280.0 153.3
290.0 160.0
)

ORTSBearingType ( Roller )
ORTSDavis_A ( 1565.6 )
ORTSDavis_B ( 40.86 )
ORTSDavis_C ( 6.3825 )

ORTSAdhesion (
ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
ORTSSlipWarningThreshold ( 70 )
)

Comment ( "Pantografy" )
ORTSPantographs ( 
Pantograph ( Delay ( 2s ) ) 
Pantograph ( Delay ( 2s ) ) 
 )
	
Comment ( "Ostatni informace" )
Sound ( 181008eng.sms )
	
    	
	Inside (
		PassengerCabinFile ( 183028.s )
		PassengerCabinHeadPos ( -1.7 3.1 7.2 )
		RotationLimit ( 0 190 0 )
		StartDirection ( 0 180 0 )
	)

Lights	(	26
              Light	(
			comment( kuzel plny )
			Type		( 1 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.1 )
			FadeOut  ( 0.1 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.0 3.5 1.8 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 300.0 )
					Angle ( 25.0 )
					)
				)
			) 
                Light	(
			comment( kuzel tlmeny)
			Type		( 1 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.1 )
			FadeOut  ( 0.1 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.0 3.5 1.8 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 100.0 )
					Angle ( 25.0 )
					)
				)
			)
comment ( Definicia svetiel pre predne stanoviste )
                Light	(
			comment( Reflektor lavy plny )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.11 3.67 8.65 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)
		Light	(
			comment( Reflektor pravy plny )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.11 3.67 8.65 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)
	     Light	(
			comment( Reflektor lavy tlmeny )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.11 3.67 8.65 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)
		Light	(
			comment( Reflektor pravy tlmeny )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.11 3.67 8.65 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)	    
             Light	(
			comment( Predne lave pozicne )
			Type		( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.8 1.93 8.84 )
					Azimuth ( 0 0 5 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
            Light	(
			comment( Predne prave pozicne )
			Type		( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.8 1.93 8.84 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
                Light	(
			comment( Zadne lave biele )
			Type		( 0 )
			Conditions	(
				Headlight ( 1 )
				Unit ( 3 )
                                Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.8 1.93 -8.84 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
                Light	(
			comment( Zadne lave cervene )
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 3 )
                                Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 0.8 1.93 -8.84 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( Zadne prave cervene )
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 3 )
                                Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -0.8 1.93 -8.84)
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
comment ( Definicia svetiel pre zadne stanoviste )
             Light	(
			comment( Reflektor lavy plny )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.11 3.67 -8.65 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)
		Light	(
			comment( Reflektor pravy plny )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.11 3.67 -8.65 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)
	     Light	(
			comment( Reflektor lavy tlmeny )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.11 3.67 -8.65 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)
		Light	(
			comment( Reflektor pravy tlmeny )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.11 3.67 -8.65 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)	    
             Light	(
			comment( Predne lave pozicne )
			Type		( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.8 1.93 -8.84 )
					Azimuth ( -180 -180 -175 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
            Light	(
			comment( Predne prave pozicne )
			Type		( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 5 )
				Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.8 1.93 -8.84 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
                Light	(
			comment( Zadne lave biele )
			Type		( 0 )
			Conditions	(
				Headlight ( 1 )
				Unit ( 4 )
                                Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.8 1.93 8.84 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
                Light	(
			comment( Zadne lave cervene )
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 4 )
                                Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -0.8 1.93 8.84 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( Zadne prave cervene )
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 4 )
                                Control ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 0.8 1.93 8.84 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
comment ( Definicia svetiel pre loko ovladanu PC )
                Light	(
			comment( Reflektor lavy tlmeny )
			Type		( 0 )
			Conditions	(
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.11 3.67 8.65 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)
		Light	(
			comment( Reflektor pravy tlmeny )
			Type		( 0 )
			Conditions	(
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.11 3.67 8.65 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)	    
             Light	(
			comment( Predne lave pozicne )
			Type		( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.8 1.93 8.84 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)
            Light	(
			comment( Predne prave pozicne )
			Type		( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.8 1.93 8.84 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)
                Light	(
			comment( Zadne lave cervene )
			Type		( 0 )
			Conditions	(
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 0.8 1.93 -8.84 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)
		Light	(
			comment( Zadne prave cervene )
			Type		( 0 )
			Conditions	(
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
				)
			FadeIn  ( 0.1 )
			FadeOut  ( 0.1 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -0.8 1.93 -8.84 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				)
			)
                )
	)

Engine ( cdc_182168  

comment	( Description )

	Wagon ( cdc_182168 )

Comment ( "Pohon" ) 
Type ( Electric ) 
MaxVelocity ( 90km/h ) 
WheelRadius ( 0.625m ) 
Sanding ( 40km/h ) 
NumWheels ( 6 ) 
ORTSDriveWheelWeight ( 124.2t ) 
MaxForce ( 4300kN ) 
MaxContinuousForce ( 4300kN ) 
MaxPower ( 2820kW ) 
MaxCurrent ( 6600A ) 
BrakeCutsPowerAtBrakeCylinderPressure ( 0.4bar ) 
 
ORTSCircuitBreaker ( Manual ) 
ORTSCircuitBreakerClosingDelay ( 2s ) 
ORTSPowerOnDelay ( 2s ) 
 
  comment ( 0     1     2     3     4     5     6     7      8     9     10   11    12    13    14    15    16    17    18    19    20    21-S  22    23    24    25    26    27    28    29    30    31    32    33-SP 34    35    36    37    38    39    40    41    42-P  PI    PII   PIII ) 
ORTSContinuousForceTimeFactor ( 3600 )
ORTSTractionCharacteristics ( 22 47
Throttle ( 0.00  0.04  0.05  0.07  0.09  0.11  0.13  0.14   0.15  0.16  0.17 0.18  0.19  0.20  0.21  0.22  0.23  0.24  0.25  0.26  0.27  0.28  0.29  0.30  0.31  0.32  0.33  0.35  0.37  0.39  0.41  0.44  0.47  0.50  0.52  0.54  0.56  0.58  0.60  0.63  0.67  0.71  0.75  0.85  0.95  1.00 ) 
 table ( 
  0.0km/h 0.0kN 100kN 142kN 183kN 240kN 290kN 345kN 400kN 450kN 500kN 600kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
  5.0km/h 0.0kN  70kN  92kN 117kN 157kN 179kN 220kN 245kN 270kN 290kN 325kN 360kN 420kN 490kN 590kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 10.0km/h 0.0kN  48kN  56kN  75kN  95kN 115kN 130kN 144kN 160kN 170kN 185kN 200kN 220kN 245kN 265kN 288kN 320kN 355kN 395kN 440kN 500kN 600kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 15.0km/h 0.0kN  25kN  33kN  45kN  55kN  65kN  70kN  75kN  80kN  87kN  92kN 100kN 108kN 116kN 123kN 130kN 137kN 144kN 161kN 170kN 190kN 212kN 240kN 280kN 325kN 395kN 440kN 500kN 600kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 20.0km/h 0.0kN  15kN  22kN  33kN  35kN  37kN  40kN  43kN  46kN  49kN  52kN  55kN  58kN  61kN  64kN  67kN  70kN  73kN  77kN  81kN  85kN  92kN 170kN 195kN 230kN 262kN 320kN 380kN 440kN 500kN 600kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 25.0km/h 0.0kN  10kN  12kN  22kN  24kN  25kN  26kN  27kN  28kN  29kN  30kN  31kN  32kN  34kN  36kN  38kN  40kN  42kN  44kN  46kN  48kN  50kN 125kN 138kN 160kN 177kN 208kN 234kN 258kN 295kN 345kN 420kN 500kN 600kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 30.0km/h 0.0kN   9kN  10kN  12kN  14kN  15kN  16kN  17kN  18kN  19kN  20kN  21kN  22kN  23kN  24kN  25kN  26kN  27kN  28kN  30kN  31kN  32kN  92kN 100kN 112kN 124kN 135kN 148kN 164kN 174kN 185kN 198kN 220kN 244kN 262kN 295kN 335kN 420kN 500kN 600kN 700kN 700kN 700kN 700kN 700kN 700kN  
 35.0km/h 0.0kN   8kN   8kN   8kN   9kN  10kN  11kN  12kN  13kN  14kN  15kN  16kN  17kN  18kN  19kN  20kN  21kN  22kN  23kN  24kN  25kN  26kN  80kN  85kN  90kN  95kN 100kN 105kN 114kN 122kN 131kN 140kN 134kN 146kN 198kN 228kN 250kN 296kN 330kN 374kN 490kN 600kN 600kN 700kN 700kN 700kN  
 40.0km/h 0.0kN   7kN   7kN   7kN   8kN   9kN  10kN  10kN  11kN  12kN  13kN  14kN  15kN  16kN  17kN  18kN  19kN  20kN  21kN  22kN  23kN  24kN  40kN  45kN  50kN  55kN  60kN  65kN  70kN  75kN  80kN  85kN  90kN  95kN 153kN 168kN 184kN 212kN 234kN 256kN 308kN 368kN 456kN 520kN 700kN 700kN  
 45.0km/h 0.0kN   4kN   5kN   5kN   7kN   7kN   9kN   9kN   9kN   9kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  35kN  40kN  42kN  44kN  46kN  50kN  53kN  56kN  60kN  62kN  65kN  68kN 120kN 128kN 136kN 153kN 168kN 176kN 225kN 238kN 269kN 394kN 600kN 700kN  
 50.0km/h 0.0kN   1kN   2kN   2kN   3kN   3kN   3kN   3kN   3kN   4kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   8kN   9kN  10kN  30kN  35kN  37kN  39kN  41kN  42kN  44kN  46kN  47kN  48kN  50kN  52kN 100kN 105kN 110kN 116kN 124kN 132kN 144kN 158kN 172kN 268kN 432kN 700kN  
 55.0km/h 0.0kN   1kN   1kN   1kN   2kN   2kN   2kN   2kN   2kN   2kN   2kN   2kN   2kN   2kN   3kN   3kN   4kN   4kN   5kN   7kN   8kN   9kN  25kN  30kN  32kN  33kN  34kN  35kN  36kN  37kN  38kN  39kN  40kN  42kN  70kN  74kN  80kN  84kN  90kN  96kN 104kN 118kN 124kN 185kN 285kN 600kN  
 60.0km/h 0.0kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   2kN   2kN   2kN   2kN   3kN   4kN   6kN   7kN   8kN  20kN  24kN  25kN  26kN  27kN  28kN  29kN  30kN  31kN  32kN  33kN  34kN  62kN  65kN  69kN  72kN  76kN  80kN  84kN  92kN  98kN 138kN 196kN 475kN  
 65.0km/h 0.0kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   2kN   2kN   3kN   5kN   6kN   7kN  15kN  20kN 20.5kN 21kN  21kN  22kN  22kN  23kN  23kN  24kN  24kN  25kN  54kN  56kN  58kN  61kN  63kN  65kN  68kN  72kN  80kN 108kN 147kN 222kN  
 70.0km/h 0.0kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   2kN   4kN   5kN   6kN  10kN  15kN  15kN  16kN  16kN  17kN  17kN  18kN  18kN  19kN  20kN  21kN  42kN  44kN  46kN  48kN  51kN  53kN  57kN  60kN  65kN  92kN 120kN 168kN  
 75.0km/h 0.0kN 0.9kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   3kN   4kN   5kN   9kN  10kN  10kN  11kN  11kN  12kN  13kN  14kN  15kN  16kN  17kN  18kN  36kN  38kN  40kN  42kN  44kN  46kN  48kN  50kN  54kN  77kN  95kN 138kN  
 80.0km/h 0.0kN 0.8kN 0.9kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   2kN   3kN   4kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  14kN  15kN  28kN  30kN  32kN  34kN  36kN  38kN  40kN  42kN  45kN  65kN  83kN 117kN  
 85.0km/h 0.0kN 0.5kN 0.6kN 0.7kN 0.8kN 0.9kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   2kN   3kN   7kN   8kN   8kN   9kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  20kN  23kN  25kN  27kN  29kN  31kN  33kN  36kN  38kN  54kN  70kN 103kN   
 90.0km/h 0.0kN 0.4kN 0.5kN 0.6kN 0.7kN 0.8kN 0.9kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   2kN   6kN   7kN   7kN   8kN   8kN   8kN   9kN   9kN   9kN  10kN  10kN  10kN  14kN  16kN  18kN  20kN  22kN  24kN  26kN  28kN  32kN  45kN  60kN  86kN  
 95.0km/h 0.0kN 0.3kN 0.4kN 0.5kN 0.6kN 0.7kN 0.8kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   8kN   8kN   8kN   9kN   9kN  10kN  12kN  14kN  16kN  18kN  20kN  22kN  24kN  26kN  38kN  52kN  78kN  
100.0km/h 0.0kN 0.2kN 0.3kN 0.4kN 0.5kN 0.6kN 0.7kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   3kN   3kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   8kN   8kN   9kN  14kN  15kN  16kN  17kN  18kN  19kN  20kN  22kN  32kN  48kN  69kN  
105.0km/h 0.0kN 0.1kN 0.2kN 0.3kN 0.4kN 0.5kN 0.6kN 0.7kN 0.8kN 0.9kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   1kN   2kN   2kN   3kN   3kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   8kN  13kN  14kN  15kN  16kN  17kN  18kN  19kN  21kN  30kN  43kN  65kN  
 ) )


	
Comment ( "Brzdy" ) 
Comment ( "Brzdovy system DAKO, brzdice DAKO BS2, DAKO BP, kompresor K2 lok" ) 
Comment ( "Brzdeni I.zpusob, rezim brzdeni P" ) 
BrakesEngineBrakeType ( "Air_single_pipe" ) 
BrakesTrainBrakeType ( "Air_single_pipe" ) 
BrakesEngineControllers ( "Independent, Train" ) 
 
DoesBrakeCutPower ( 1 ) 
 
ORTSMainResChargingRate ( 0.06bar/s ) 
ORTSBrakePipeChargingRate ( 20.7bar/s ) 
AirBrakesMainMinResAirPressure ( 6bar ) 
AirBrakesMainMaxAirPressure ( 8bar )
AirBrakesMainResVolume ( 1330l ) 
AirBrakesAirCompressorWattage ( 38000W ) 
AirBrakesCompressorRestartPressure ( 6bar ) 
AirBrakesIsCompressorElectricOrMechanical ( 0 ) 
ORTSTrainPipeLeakRate ( 0.0042bar/s ) 
 
ORTSEngineBrakeReleaseRate ( 1.0bar/s ) 
ORTSEngineBrakeApplicationRate ( 1.3bar/s ) 
EngineBrakesControllerMinPressureReduction ( 0.3bar ) 
EngineBrakesControllerFullServicePressureDrop ( 1.0bar ) 
EngineBrakesControllerMaxApplicationRate ( 1.33bar/s ) 
EngineBrakesControllerMaxReleaseRate ( 1.0bar/s ) 
EngineBrakesControllerMaxSystemPressure ( 5bar ) 

TrainBrakesControllerMinPressureReduction ( 0.3bar ) 
TrainBrakesControllerFullServicePressureDrop ( 2.0bar ) 
TrainBrakesControllerMaxReleaseRate ( 0.5bar/s ) 
TrainBrakesControllerMaxApplicationRate ( 0.5bar/s ) 
TrainBrakesControllerMaxQuickReleaseRate ( 2.0bar/s ) 
TrainBrakesControllerEmergencyApplicationRate ( 1.86bar/s ) 
TrainBrakesControllerMaxSystemPressure ( 5bar ) 
 
ORTSBrakePipeTimeFactor ( 0.003 ) 
ORTSBrakeServiceTimeFactor ( 1.009 ) 
ORTSBrakeEmergencyTimeFactor ( 0.1 ) 
 
 Comment ( "Ovladani jizdy" ) 
 
Comment ( "Vlakovy zabezpecovac - KBS" ) 
VigilanceMonitor ( 
MonitoringDeviceMonitorTimeLimit ( 16 ) 
MonitoringDeviceAlarmTimeLimit ( 6 ) 
MonitoringDevicePenaltyTimeLimit ( 0 ) 
MonitoringDeviceCriticalLevel ( 0 ) 
MonitoringDeviceResetLevel ( 0 ) 
MonitoringDeviceAppliesFullBrake ( 0 ) 
MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
MonitoringDeviceAppliesCutsPower ( 1 ) 
MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
MonitoringDeviceResetOnResetButton ( 1 ) 
MonitoringDeviceResetOnZeroSpeed ( 1 ) 
) 
 
 Comment ( "Rizeni" ) 
 EngineControllers ( 
 
Throttle ( 0 1 0.005 0 
NumNotches ( 46 
Notch ( 0.00 0 Dummy ) comment( 0 ) 
Notch ( 0.04 0 Dummy ) comment( 1 ) 
Notch ( 0.05 0 Dummy ) comment( 2 ) 
Notch ( 0.07 0 Dummy ) comment( 3 ) 
Notch ( 0.09 0 Dummy ) comment( 4 ) 
Notch ( 0.11 0 Dummy ) comment( 5 ) 
Notch ( 0.13 0 Dummy ) comment( 6 480A 345kN 0kMh ) 
Notch ( 0.14 0 Dummy ) comment( 7 ) 
Notch ( 0.15 0 Dummy ) comment( 8 ) 
Notch ( 0.16 0 Dummy ) comment( 9 ) 
Notch ( 0.17 0 Dummy ) comment( 10 ) 
Notch ( 0.18 0 Dummy ) comment( 11 ) 
Notch ( 0.19 0 Dummy ) comment( 12 ) 
Notch ( 0.20 0 Dummy ) comment( 13 ) 
Notch ( 0.21 0 Dummy ) comment( 14 ) 
Notch ( 0.22 0 Dummy ) comment( 15 ) 
Notch ( 0.23 0 Dummy ) comment( 16 ) 
Notch ( 0.24 0 Dummy ) comment( 17 ) 
Notch ( 0.25 0 Dummy ) comment( 18 ) 
Notch ( 0.26 0 Dummy ) comment( 19 ) 
Notch ( 0.27 0 Dummy ) comment( 20 ) 
Notch ( 0.28 0 Dummy ) comment( 21 Serie ) 
Notch ( 0.29 0 Dummy ) comment( 22 ) 
Notch ( 0.30 0 Dummy ) comment( 23 ) 
Notch ( 0.31 0 Dummy ) comment( 24 ) 
Notch ( 0.32 0 Dummy ) comment( 25 ) 
Notch ( 0.33 0 Dummy ) comment( 26 ) 
Notch ( 0.35 0 Dummy ) comment( 27 ) 
Notch ( 0.37 0 Dummy ) comment( 28 ) 
Notch ( 0.39 0 Dummy ) comment( 29 ) 
Notch ( 0.41 0 Dummy ) comment( 30 ) 
Notch ( 0.44 0 Dummy ) comment( 31 ) 
Notch ( 0.47 0 Dummy ) comment( 32 ) 
Notch ( 0.50 0 Dummy ) comment( 33 Serioparalel ) 
Notch ( 0.52 0 Dummy ) comment( 34 ) 
Notch ( 0.54 0 Dummy ) comment( 35 ) 
Notch ( 0.56 0 Dummy ) comment( 36 ) 
Notch ( 0.58 0 Dummy ) comment( 37 ) 
Notch ( 0.60 0 Dummy ) comment( 38 ) 
Notch ( 0.63 0 Dummy ) comment( 39 ) 
Notch ( 0.67 0 Dummy ) comment( 40 ) 
Notch ( 0.71 0 Dummy ) comment( 41 ) 
Notch ( 0.75 0 Dummy ) comment( 42 Paralel ) 
Notch ( 0.85 0 Dummy ) comment( PI ) 
Notch ( 0.95 0 Dummy ) comment( PII ) 
Notch ( 1.00 0 Dummy ) comment( PIII ) 
) ) 
 
 Comment ( "Primocinna brzda typu DAKO BP" ) 
Brake_Engine ( 0 1 0.1 0.8 
NumNotches  ( 1 
Notch ( 0 1 Dummy ) ) 
) 
 
 Comment ( "Prubezna brzda typ DAKO-BS2" ) 
Brake_Train ( 0 1 0.04 0.21 
NumNotches ( 6 
Notch ( 0 0 TrainBrakesControllerFullQuickReleaseStart ) 
Notch ( 0.14 0 TrainBrakesControllerReleaseStart ) 
Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart ) 
Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart ) 
Notch ( 0.95 0 TrainBrakesControllerSuppressionStart ) 
Notch ( 0.99 0 TrainBrakesControllerEmergencyStart ) 
 ) ) 
 
Brake_Hand ( 0 1 0.025 0 
NumNotches ( 0 ) 
 ) 
 
DirControl ( -1 0 1 1 ) 
BellToggle ( 0 1 0 ) 
Sanding ( 0 1 0 ) 
Horn ( 0 1 0 ) 
Wipers ( 0 1 0 ) 
EmergencyStopToggle ( 0 1 1 ) 
Vigilance ( 0 1 0 ) 
 PantographToggle1 ( 0 1 0 ) 


Headlights ( 0 0.25 1 0 ) 
BailOffButton ( 0 1 0 ) 
) 
	
Comment	( Operations )

	 Name ( " CDC 182 168-5" )
   
Comment	( CabSound and Views )

  Sound ( 181008cab.sms ) 
  CabView ( 181008.cvf )
  HeadOut ( 1.7 2.8 7.5 ) 

	 Description (
	 "Ovladani\n\n"+ 
	 "Lokomotiva ma oba sberace ovladatelne pomoci 4-polohoveho prepinace s koncovou polohou, ovlada se standardne klavesou P\n\n"+ 
	 "Vykon 26% odpovida hospodarnemu seriovemu stupni\n\n"+ 
	 "Vykon 40% odpovida hospodarnemu serioparalelnimu stupni\n\n"+
	 "Vykon 80% odpovida hospodarnemu serioparalelnimu stupni\n\n"+
	 "Po kazdem hospodarne stupni nasleduji 3 stupne shuntovaci a pak se kontroler vraci zpet postupne na hospodarny stupen\n\n"+
	  "Rozjezdove stupne muzete zatezovat pouze po dobu 6s, proto lokomotivy vzdy prevedte na hospodarne nebo shuntovaci stupne co nejrychleji\n\n"+ 
	"Pretizeni:\n"+
	"Proud trvaly : 307A\n\n"+
    		"60min: 332A\n\n"+
    	"Nadproudova ochrana : 650A\n\n"+
	"Brzdic prubezne vlakove brzdy DAKO BS2\n\n"+
	"Brzdic lokomotivni brzdy DAKO-BP\n\n"+	  
	  "Elektrická lokomotiva r.183 3. serie /E 669.3/ CD urcená pro nákladní vlaky.\n\n"+ 
	  "Rok vyroby: 1961 - 1962\n\n"+ 
	  "Napetí: 3 kV ss\n\n"+ 
	  "Trvaly vykon: 2610 kW\n\n"+ 
	  "Hodinovy vykon: 2820 kW\n\n"+ 
	  "Hmotnost: 120 t\n\n"+ 
	  "Max.rychlost: 90 km/h\n\n"+ 
	  "Usp.pojezdu: Co´- Co´\n\n"+
	  "Délka pres nárazniky: 18,92 m"

    	)

   	EngineOperatingProcedures (
		"Stupne kontroleru:\n"+
		"1.-20.	Rozjezdove stupne seriove\n"+
		"21.	Hospodarny seriovy stupen (odporniky vyrazeny)\n"+
		"I.-III.	Shuntovaci rozjedove stupne, vsechny motory v serii\n"+
		"22.-32.Odporove serioparalelni stupne (vzdy dva motory v serii)\n"+
		"33.	Hospodarny serioparalelni stupen (odporniky vyrazeny)\n"+
		"I.-III.	Shuntovaci stupne pro serioparalelni zapojeni motoru\n\n"+
		"34.-41.Odporove paralelni stupne (vzdy dva motory v serii)\n"+		
		"42.	Hospodarny paralelni stupen (odporniky vyrazeny)\n"+
		"I.-III.	Shuntovaci stupne pro paralelni zapojeni motoru\n\n"		
	)
)
