SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( CD_140085

	Type ( Engine ) 
	WagonShape ( "CD_140085.s" ) 
	FreightAnim ( rv.s 1 1 ) 
	Size ( 3.08m 4.58m 15.24m ) 
	CentreOfGravity ( 0m 2.25m 0m ) 
	Mass ( 82t ) 
	WheelRadius ( 0.625m ) 
	InertiaTensor ( Box ( 3.08m 4.58m 15.24m ) ) 

	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)

	Adheasion ( 0.4 0.72 1.4 0 ) 

	BrakeCylinderPressureForMaxBrakeBrakeForce ( 56 ) 
	BrakeEquipmentType ( "handbrake,graduated_release_triple_valve,auxilary_reservoir, Emergency_brake_reservoir" ) 
	BrakeSystemType ( Air_single_pipe ) 

	DerailBufferForce ( 350kN ) 
	DerailRailForce ( 2.5*80t )
	DerailRailHeight ( 6cm ) 

	EmergencyBrakeResMaxPressure ( 73 ) 
	EmergencyResCapacity ( 1 ) 
	EmergencyResChargingRate ( 3 ) 
	EmergencyResVolumeMultiplier ( 1 ) 

	Friction ( 800N/m/s 0.05 1mph 10N/m/s 2 5.1N/rad/s 1 1rad/s	0N/rad/s 1 ) 

	comment	( Lights )
        comment	( Created by Robo )
 
comment ( svetelne kuzely ) 
	
	Lights ( 23
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0 1 8 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 120 )
				)
			)
		)
		Light (
			comment ( Svetelný kuzel tlumený )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FF666666 )
					Position ( 0 2 -1 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 60 )
				)
			)
		)
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( reflektor dálkový )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 0.0 3.567 7.03 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.9 )
				)
			)
		)
            	Light (
			comment ( reflektor tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.0 3.567 7.03 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D  )
					Position ( -0.875 1.768 7.16 )
					Azimuth ( -17 -17 -17 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D  )
					Position ( 0.875 1.768 7.16 )
					Azimuth ( 17 17 17 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.875 1.768 -7.16 )
					Azimuth ( -163 -163 -163 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.875 1.768 -7.16 )
					Azimuth ( 163 163 163 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )

		Light (
			comment ( reflektor dálkový )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 0.0 3.567 -7.03 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.9 )
				)
			)
		)
            	Light (
			comment ( reflektor tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.0 3.567 -7.03 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D  )
					Position ( 0.875 1.768 -7.16 )
					Azimuth ( 163 163 163 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D  )
					Position ( -0.875 1.768 -7.16 )
					Azimuth ( -163 -163 -163 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.875 1.768 7.16 )
					Azimuth ( 17 17 17 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.875 1.768 7.16 )
					Azimuth ( -17 -17 -17 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
                comment ( Definicia svetiel pre posunujuci diel )

		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D  )
					Position ( 0.875 1.768 7.16 )
					Azimuth ( 17 17 17 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
                Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D  )
					Position ( -0.875 1.768 -7.16 )
					Azimuth ( -163 -163 -163 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		
		comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Pravé přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D  )
					Position ( 0.875 1.768 7.16 )
					Azimuth ( 17 17 17 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
                Light	(
			comment( Levé zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D  )
					Position ( -0.875 1.768 -7.16 )
					Azimuth ( -163 -163 -163 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
                

		comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( PC prední pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D  )
					Position ( 0.875 1.768 7.16 )
					Azimuth ( 17 17 17 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC prední levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D  )
					Position ( -0.875 1.768 7.16 )
					Azimuth ( -17 -17 -17 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC reflektor tlumený )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.0 3.567 7.03 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.875 1.768 -7.16 )
					Azimuth ( -163 -163 -163 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.875 1.768 -7.16 )
					Azimuth ( 163 163 163 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
	)

	MaxApplicationRate ( 2 ) 
	MaxAuxilaryChargingRate ( 4 ) 
	MaxBrakeForce ( 55kN ) 
	MaxHandbrakeForce ( 14kN ) 
	MaxReleaseRate ( 2 ) 
	NumberOfHandbrakeLeverSteps ( 100 ) 
	NumWheels ( 4 ) 
	PassengerCapacity ( 10 ) 
	Sound ( "..//..//common.snd//sndelok//141eng.sms" ) 
	TripleValveRatio ( 2.55 ) 
) 

Engine ( CD_140085
	Wagon ( "CD_140085" ) 
	Type ( Electric ) 
	Name ( "CD 140 085-2" ) 
	Sound ( "..//..//common.snd//sndelok//141cab.sms" ) 
	CabView ( "..//..//common.cab//cab140//140_001.cvf" ) 
	HeadOut ( 1.65m 3.0m 5.85m ) 

	AirBrakesAirCompressorPowerRating ( 1.09 ) 
	AirBrakesAirCompressorWattage ( 25200 ) 
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 2 ) 
	AirBrakesCompressorRestartPressure ( 87 ) 
	AirBrakesHasLowPressureTest ( 0 ) 
	AirBrakesIsCompressorElectricOrMechanical ( 0 ) 
	AirBrakesMainMaxAirPressure ( 116 ) 
	AirBrakesMainMinResAirPressure ( 50 ) 
	AirBrakesMainResVolume ( 30 ) 

	BrakeCutsPowerAtBrakeCylinderPressure ( 10 ) 
	BrakesEngineBrakeType ( Air_single_pipe ) 
	BrakesEngineControllers ( "Train,Independent,Hand" ) 
	BrakesTrainBrakeType ( Air_single_pipe ) 

	DieselEngineSpeedOfMaxTractiveEffort ( 0mph ) 

	DoesBrakeCutPower ( 1 ) 
	DoesHornTriggerBell ( 0 ) 

	EngineBrakesControllerMaxQuickReleaseRate ( 5 ) 
	EngineBrakesControllerMaxReleaseRate ( 3 ) 
	EngineBrakesControllerMinPressureReduction ( 3 ) 
	EngineBrakesControllerMaxApplicationRate ( 3 ) 
	EngineBrakesControllerEmergencyApplicationRate ( 5 ) 
	EngineBrakesControllerMinSystemPressure ( 0 ) 
	EngineBrakesControllerMaxSystemPressure ( 73 ) 
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 ) 
	EngineBrakesControllerFullServicePressureDrop ( 12 ) 
	EngineBrakesControllerHasProportionalBrake ( 0 ) 
	EngineBrakesProportionalBrakeLag ( 1 ) 

	MaxContinuousForce ( 5200kN ) 
	MaxCurrent ( 15600A ) 
	MaxForce ( 5200kN ) 
	MaxPower ( 2300kW ) 
	MaxSandingTime ( 600 ) 
	MaxVelocity ( 132km/h ) 
	NumWheels ( 4 ) 
	Sanding ( 60km/h ) 
	WheelRadius ( 0.625m ) 

	TrainBrakesControllerEmergencyApplicationRate ( 8 ) 
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 ) 
	TrainBrakesControllerFullServicePressureDrop ( 36 ) 
	TrainBrakesControllerMaxApplicationRate ( 2 ) 
	TrainBrakesControllerMaxQuickReleaseRate ( 4 ) 
	TrainBrakesControllerMaxReleaseRate ( 2 ) 
	TrainBrakesControllerMaxSystemPressure ( 73 ) 
	TrainBrakesControllerMinPressureReduction ( 1 ) 
	TrainBrakesControllerMinSystemPressure ( 0 ) 
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 36 ) 
	TrainPipeLeakRate ( 0.02 ) 

 	OverspeedMonitor ( 
		MonitoringDeviceMonitorTimeLimit ( 0 ) 
		MonitoringDeviceAlarmTimeLimit ( 0 ) 
		MonitoringDevicePenaltyTimeLimit ( 0 ) 
		MonitoringDeviceCriticalLevel ( 81 ) 
		MonitoringDeviceResetLevel ( 0 ) 
		MonitoringDeviceAppliesFullBrake ( 0 ) 
		MonitoringDeviceAppliesEmergencyBrake ( 0 ) 
		MonitoringDeviceAppliesCutsPower ( 1 ) 
		MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
		MonitoringDeviceTriggerOnHighCurrent ( 700 ) 
		MonitoringDeviceResetOnDirectionNeutral ( 1 ) 
	) 

	EmergencyStopMonitor ( 
		MonitoringDeviceMonitorTimeLimit ( 0 ) 
		MonitoringDeviceAlarmTimeLimit ( 0 ) 
		MonitoringDevicePenaltyTimeLimit ( 0 ) 
		MonitoringDeviceCriticalLevel ( 0 ) 
		MonitoringDeviceResetLevel ( 0 ) 
		MonitoringDeviceAppliesFullBrake ( 1 ) 
		MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
		MonitoringDeviceAppliesCutsPower ( 0 ) 
		MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
		MonitoringDeviceResetOnResetButton ( 1 ) 
	) 

	VigilanceMonitor ( 
		MonitoringDeviceMonitorTimeLimit ( 20 ) 
		MonitoringDeviceAlarmTimeLimit ( 10 ) 
		MonitoringDevicePenaltyTimeLimit ( 5 ) 
		MonitoringDeviceCriticalLevel ( 0 ) 
		MonitoringDeviceResetLevel ( 0 ) 
		MonitoringDeviceAppliesFullBrake ( 1 ) 
		MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
		MonitoringDeviceAppliesCutsPower ( 0 ) 
		MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
		MonitoringDeviceResetOnResetButton ( 1 ) 
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
	)

EngineControllers ( 

	AWS ( 0 1 0 ) 
	BailOffButton ( 0 1 0 ) 
	BellToggle ( 0 1 0 ) 

	Brake_Engine ( 0 0.76 0.05 0.3 
		NumNotches ( 5 
		Notch ( 0.0 0 EngineBrakesControllerFullQuickReleaseStart ) 
		Notch ( 0.3 0 EngineBrakesControllerReleaseStart ) 
		Notch ( 0.5 0 EngineBrakesControllerRunningStart ) 
		Notch ( 0.7 0 EngineBrakesControllerContinuousServiceStart ) 
		Notch ( 1.0 0 EngineBrakesControllerEmergencyStart ) 
		) ) 

	Brake_Hand ( 0 1 0.05 0 
		NumNotches	( 1 
		Notch ( 0 1 Dummy ) 
		) )

	Brake_Train ( 0 1 0.03 0.2 
		NumNotches ( 5 
		Notch ( 0.00 0 TrainBrakesControllerFullQuickReleaseStart ) 
		Notch ( 0.20 0 TrainBrakesControllerReleaseStart ) 
		Notch ( 0.30 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart ) 
		Notch ( 0.90 0 TrainBrakesControllerSuppressionStart ) 
		Notch ( 1.00 0 TrainBrakesControllerEmergencyStart ) 
		) ) 

	Throttle ( 0 1 0.0001 0 
		NumNotches ( 48 
		Notch ( 0.000 0 Dummy ) 
		Notch ( 0.0001 0 Dummy ) 

		Notch ( 0.010 0 Dummy ) 
		Notch ( 0.020 0 Dummy ) 
		Notch ( 0.030 0 Dummy ) 
		Notch ( 0.040 0 Dummy ) 
		Notch ( 0.050 0 Dummy ) 

		Notch ( 0.065 0 Dummy ) 
		Notch ( 0.080 0 Dummy ) 
		Notch ( 0.095 0 Dummy ) 
		Notch ( 0.110 0 Dummy ) 
		Notch ( 0.125 0 Dummy ) 

		Notch ( 0.140 0 Dummy ) 
		Notch ( 0.160 0 Dummy ) 
		Notch ( 0.180 0 Dummy ) 
		Notch ( 0.200 0 Dummy ) 
		Notch ( 0.225 0 Dummy ) 

		Notch ( 0.250 0 Dummy ) 
		Notch ( 0.275 0 Dummy ) 
		Notch ( 0.300 0 Dummy ) 
		Notch ( 0.330 0 Dummy ) 
		Notch ( 0.360 0 Dummy ) 

		Notch ( 0.395 0 Dummy ) 
		Notch ( 0.430 0 Dummy ) 
		Notch ( 0.465 0 Dummy ) 
		Notch ( 0.500 0 Dummy ) 

		Notch ( 0.520 0 Dummy ) 
		Notch ( 0.540 0 Dummy ) 
		Notch ( 0.560 0 Dummy ) 
		Notch ( 0.580 0 Dummy ) 

		Notch ( 0.585 0 Dummy ) 
		Notch ( 0.590 0 Dummy ) 
		Notch ( 0.595 0 Dummy ) 

		Notch ( 0.600 0 Dummy ) 
		Notch ( 0.650 0 Dummy ) 
		Notch ( 0.700 0 Dummy ) 
		Notch ( 0.750 0 Dummy ) 
		Notch ( 0.800 0 Dummy ) 
		Notch ( 0.850 0 Dummy ) 
		Notch ( 0.900 0 Dummy ) 
		Notch ( 0.950 0 Dummy ) 
		Notch ( 1.000 0 Dummy ) 

		Notch ( 1.005 0 Dummy ) 
		Notch ( 1.010 0 Dummy ) 
		Notch ( 1.015 0 Dummy ) 
		Notch ( 1.020 0 Dummy ) 
		Notch ( 1.025 0 Dummy ) 
		Notch ( 1.030 0 Dummy ) 
		) ) 

	DirControl ( -1 0 1 1 ) 
	EmergencyStopToggle ( 0 1 0 ) 
	Headlights ( 0 0.25 1 0 ) 
	Horn ( 0 1 0 ) 
	PantographToggle1 ( 0 1 0 ) 
	PantographToggle2 ( 0 1 0 ) 
	PantographsToggle_4 ( 0 1 0 ) 
	Sanding ( 0 1 0 ) 
	Vigilance ( 0 1 0 ) 
	Wipers ( 0 1 0 ) 
	) 

	Description ( 
		"Rada E499.0/140 je univerzalni elektricka lokomotiva \n"+
		"Trvaly vykon: 2032kW, proud : 360A \n"+
		"Hodinovy vykon: 2344kW, proud : 415A \n"+
		"Max. provozni rychlost: 120km/h \n"+
		"Hmotnost lokomotivy: 82tun \n"+
		"Nastaveni 50% odpovida hospodarnemu seriovemu stupni \n"+
		"pritom je hodinovy proud 415A, rychlost 30km/h, tazna sila 138kN \n"+
		"Nastaveni 100% odpovida hospodarnemu serioparalelnimu stupni \n"+
		"pritom je hodinovy proud 415A, rychlost 60km/h, tazna sila 138kN \n"+
		"Nastaveni 103% odpovida 6.sh.stupni se zeslabenym polem na 44% \n"+
		"pritom je hodinova rychlost 100km/h, tazna sila 85kN \n"+
		"Stupne kontroleru: \n"+
		"1.-23.	Rozjezdove stupne seriove \n"+
		"24. Hospodarny seriovy stupen (odporniky vyrazeny) \n"+
		"I.-IV.	Shuntovaci rozjedove stupne, vsechny motory v serii \n"+
		"A.B.C. Prechodove stupne serie - > serioparalel \n"+
		"25.-32.Odporove serioparalelni stupne (vzdy dva motory v serii) \n"+
		"33. Hospodarny serioparalelni stupen (odporniky vyrazeny) \n"+
		"I.-VI.	Shuntovaci stupne pro serioparalelni zapojeni motoru \n"+
		"Autor modelu CSD_E499005 a zscs_140001 Tomi \n"+
		"verze nastaveni pro bin 2P 2007-10-02-b57"
	)
	EngineOperatingProcedures (
		" Ovladani podle vlastniho nastaveni klaves v simulatoru\n\n" +
		" Pri zapnutych monitorech (VZ=ctrl+num4) po zvednuti sberace nebo zasahu nadproudu je nutno pred dalsi jizdou pohnout pakou smeru\n\n" +
	)
)
