SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cd_263002_hk
 Type ( Engine )
 WagonShape ( "cd_263002_hk.s" )
 Size ( 3.00m 4.69m 16.556m )
        Comment (verze ladeni 20-11-2006 - dle norem Ppoollll nastavil Semora)
        
        Comment ( Verze: 1.15 )
        Comment ( Datum: 18/4/2007 )
        Comment ( Uprava vykonove charakteristiky - plocha do 60 kmh dle skutecnosti )
        Comment ( Mez adhese: 188kN )
        Comment ( Antislip odstranen )        
        Comment ( Vykon nastaven pro stridavou cast = 3060 kW )
        Comment ( Uprava kompletnich brzd + nastaveni do polohy P 44kN, pro N je 24kN )
        Comment ( Trvala tazna sila: 173 kN = 715 A = 65% polohy ridiciho kontroleru )
        Comment ( Od B57 pridana EDB nereverzni )
        Comment (  Svetla: Robo)
        
 CentreOfGravity ( 0m 2.25m 0m )
 Mass ( 84.2t )
 WheelRadius ( 0.625m )
 InertiaTensor ( Box (3.00m 4.69m 16.556m) )
 Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Adheasion ( 0.114 0.77 1.3 0 )
 DerailRailHeight ( 10cm )
 DerailRailForce ( 84.2*2.5t )
 DerailBufferForce ( 300kN )
 NumWheels ( 4 )
 Friction (
		1070.5N/m/s    -0.10    1.3mph    12.951N/m/s    1.891
  5.1N/rad/s  1  -1rad/s  0  1
 )
	Comment ( AntiSlip () )
	MaxBrakeForce( 44kN )
	MaxHandbrakeForce( 8kN )
	NumberOfHandbrakeLeverSteps( 100 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	TripleValveRatio( 1.24 )
	MaxReleaseRate( 2 )
	MaxApplicationRate( 2 )
	MaxAuxilaryChargingRate( 5 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 35 )
        EmergencyResVolumeMultiplier ( 11 )
        EmergencyResCapacity( 7 )
	EmergencyResChargingRate( 30 )
	EmergencyBrakeResMaxPressure( 73 )

comment	( Lights )
	Lights ( 23
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFFF )
					Position ( 0 1 8 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 120 )
				)
			)
		)
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.1 2.54 7.91 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.1 2.54 7.91 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
                Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 7.82 )
					Azimuth ( 0.0 0.0 0.0 )
                                        Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )

		Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.1 2.54 -7.91 )
                                        Elevation ( -10 -10 -10 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.1 2.54 -7.91 )
                                        Elevation ( -10 -10 -10 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		) 
                Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 7.82 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                comment ( Definicia svetiel pre posunujuci diel )

		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 7.82 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		
		comment ( Definice svetel pro Loose consist )
                Light	(
			comment( Pravé přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light	(
			comment( Levé zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( PC prední pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( PC prední levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
	)

      Sound ( "../../common.snd/sndX6X/263eng.sms" )
)
Engine ( cd_263002_hk
Wagon ( cd_263002_hk )
 Type ( Electric )
	MaxPower ( 3060kW )
	MaxForce ( 285kN )
	MaxContinuousForce ( 285kN )
	MaxVelocity ( 132km/h )
	DieselEngineSpeedOfMaxTractiveEffort	( 41.44mph )    
	MaxCurrent ( 1100A )
    WheelRadius ( 0.625m )
    Sanding ( 25km/h )
    NumWheels ( 4 )

	AirBrakesAirCompressorPowerRating ( 1.18 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 144 )	
	AirBrakesMainResVolume ( 31.78 )
	AirBrakesAirCompressorWattage ( 15000 )
	AirBrakesCompressorRestartPressure ( 121 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 3 )
	TrainBrakesControllerMaxApplicationRate ( 1.7 )
	TrainBrakesControllerMaxReleaseRate ( 1.5 )
	TrainBrakesControllerMaxQuickReleaseRate ( 2.5 )
	TrainBrakesControllerEmergencyApplicationRate ( 2.5 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )

	TrainPipeLeakRate ( 0.033 )
	TrainBrakesControllerFullServicePressureDrop ( 73 )

comment ( EDB s reverzem 
	DynamicBrakesMaximumForce						( 182kN )
	DynamicBrakesResistorCurrentLimit				( 715 )
	DynamicBrakesDelayTimeBeforeEngaging			( 0 )
	DynamicBrakesNumberOfControllerNotches			( 20 )
	DynamicBrakesMaxAirBrakePressure				( 20 )
	DynamicBrakeHasAutoBailOff						( 1 )

	DynamicBrakesMaximumSpeedForFadeOut				( 137 )
	DynamicBrakesMaximumEffectiveSpeed				( 50 )
	DynamicBrakesHigherSpeedCurveExponent			( 1 )
	DynamicBrakesEffectAtMaximumFadeOut				( 0 )
	DynamicBrakesLowerSpeedCurveExponent			( 1 )
	DynamicBrakesCutInSpeed							( -50 )
	DynamicBrakesFadingSpeed						( -50 )
	DynamicBrakesMinUsableSpeed						( -137 )
	)

comment ( EDB bez reverzu )
	DynamicBrakesMaximumForce						( 182kN )
	DynamicBrakesResistorCurrentLimit				( 715 )
	DynamicBrakesDelayTimeBeforeEngaging			( 0 )
	DynamicBrakesNumberOfControllerNotches			( 20 )
	DynamicBrakesMaxAirBrakePressure				( 20 )
	DynamicBrakeHasAutoBailOff						( 1 )

	DynamicBrakesMaximumSpeedForFadeOut				( 100 )
	DynamicBrakesMaximumEffectiveSpeed				( 50 )
	DynamicBrakesHigherSpeedCurveExponent			( 1 )
	DynamicBrakesEffectAtMaximumFadeOut				( 2 )
	DynamicBrakesLowerSpeedCurveExponent			( 1 )
	DynamicBrakesCutInSpeed							( 8 )
	DynamicBrakesFadingSpeed						( 8 )
	DynamicBrakesMinUsableSpeed						( 3 )


	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train, Dynamic" )


 
EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 20 )
		MonitoringDeviceAlarmTimeLimit ( 10 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 78.7 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 0 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 77.6 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 0 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 0 )
	)

    CabView ( ..//..//common.cab//cab263//263.cvf )
    HeadOut ( 1.6 3.0 6.6 )

 DoesBrakeCutPower( 1 )
 MaxSandingTime( 600 )
 DoesHornTriggerBell( 0 )
  
        EngineControllers (
            Throttle ( 0 1 0.045 0 
                NumNotches ( 0 )
            )
  Brake_Train 	( 0 1 0.05 0.8
   NumNotches ( 5
    Notch ( 0 0 TrainBrakesControllerFullQuickReleaseStart )
    Notch ( 0.4 0 TrainBrakesControllerReleaseStart )
    Notch ( 0.6 0 TrainBrakesControllerApplyStart )
    Notch ( 0.8 0 TrainBrakesControllerContinuousServiceStart )
    Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
   )
  )
            Brake_Engine ( 0 1 0.070 0 
                 NumNotches ( 1
                    Notch ( 0       1 Dummy )                    
                )
            )            
            Brake_Dynamic ( 0 1 0.100 0 
                NumNotches ( 0 )
            )
            DirControl ( -1 0 1 1 )
            EmergencyStopToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            BellToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
		PantographToggle2 ( 0 1 0 )
		PantographToggle_4 ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            Wipers ( 0 1 0 )
            BailOffButton( 0 1 0 )
        )
    Name ( "CD 263 002-8 HK" )
    Description (
 "Rada 263 CD je stridava elektricka skrinova lokomotiva, pouzivana v nakladni i osobni doprave.\n"+
 "Typ Bo'-Bo', napeti 25kV 50Hz \n\n"+
 "Delka pres narazniky: 16,8 m\n\n"+
 "Prumer hnacich kol: 1250 mm\n\n"+
 "Hmotnost ve sluzbe: 84,2 t\n\n"+
 "Trvaly vykon trakcnich motoru: 3060 kW\n\n"+
 "Max. rychlost 120 km/h\n\n"
    )
        EngineOperatingProcedures (
        "To move forward\n"+
        "1. The pantograph has been raised for you. (If it is not up for some reason, press the P key to raise it.)\n"+
 "2. Press the W key to move the Reverser to Forward.\n"+
 "3. Press the ; (SEMICOLON) key to release the train brakes.\n"+
 "4.  Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
 "5. Press the D key to move increase the Throttle setting.\n\n"+  
 "To slow the train\n"+
 "1. Press the A key to move the throttle to a lower setting.\n"+
 "2. Use the brakes to further reduce speed if desired.\n\n"+
 "To apply the train brakes\n"+
 "1. Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
 "To release the train brakes\n"+
 "1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
 "To bail off the train brakes on the locomotive\n"+
 "1. Press the / (FORWARD SLASH) key.\n\n"+
 "To apply the locomotive brake\n"+
 "1. Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
  "To release the locomotive brake\n"+
 "1. Press the [ (LEFT BRACKET) to release the locomotive brake.\n\n"+
 "To activate emergency braking\n"+
 "1. Press the A key to reduce the throttle to Idle.\n"+
 "2. Press the BACKSPACE key to activate emergency braking.\n\n"+
 "To back up\n"+
 "1. Bring your train to a full stop.\n"+
 "2. Press the S key to move the Reverser to the Reverse position.\n"+
 "3. Press the ; (SEMICOLON) key and the [ (LEFT BRACKET) key to release the brakes.\n"+
 "4. Slowly advance the throttle lever (D key).\n\n"+
 "To load and unload passengers\n"+
 "1. Stop at a station.\n"+
 "2. Press the ENTER key.\n"+
 "3. Wait for the 'permission to depart' signal.\n"+
 "TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
 "To couple to a car or locomotive\n"+
 "1. Coast into the unit at a very slow speed, about 2 mph.\n"+
 "TIP: To use the Coupling view, press the 6 key.\n"+
 "2. Press F9 to open the Train Operations window.\n"+
 "3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
 "4. Close the Train Operations window.\n\n"+
 "To uncouple from a car or locomotive\n"+
 "1. Press F9 to open the Train Operations window.\n"+
 "2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
 "3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
 "4. Close the Train Operations window."
        ) 
      Sound ( "../../common.snd/sndX6X/263cab.sms" )
)
