SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cdc_130001
	Comment ( pro BP upravil David Hajek verze ladeni 20-11-2006 - dle norem Ppoollll nastavil Semora)
	Comment ( Verze: 1.09 )
	Comment ( Datum: 24.7.2009 )
	Comment ( Model: Pikku 2009 )
	Comment ( Svetla : 2 halogeny )
	Comment ( Sberace: 2 )
	Comment ( Uprava vozidloveho odporu - plochy do 30 kmh dle skutecnosti )
	Comment ( Mez adhese: 180kN normalne, v prokluzu 46kN )
	Comment ( Uprava kompletnich brzd + nastaveni do polohy P 50kN, pro N je 36kN )
	Comment ( Brzda podle predpisu V15/I )
	Comment ( verze ladeni 30-07-2007 - Bob oprava svetel )
	Comment ( Update pro BIN 1.7x )
	Type ( Engine )
	WagonShape ( cdc_130001.s )
	Size ( 3.15m 4.67m 17.00m )
	CentreOfGravity ( 0m 2.25m 0m )
	Mass ( 85t )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box ( 3.15m 4.67m 17.00m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)

	Adheasion ( 0.4 0.785 1.1 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 85*2.5t )
	DerailBufferForce ( 350kN )
	NumWheels ( 4 )
	Friction (
		4000N/m/s  0  18.7mph  10.000N/m/s  1.879
		5.1N/rad/s  1  1rad/s  0  1
	)
	BrakeEquipmentType ( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" )
	BrakeSystemType ( "Air_single_pipe" )

	MaxBrakeForce ( 50kN )
	MaxHandbrakeForce ( 14kN )
	NumberOfHandbrakeLeverSteps ( 100 )

	TripleValveRatio ( 2.5 )
	MaxReleaseRate ( 1.3 )
	MaxApplicationRate ( 3 )
	MaxAuxilaryChargingRate ( 2.5 )
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 55 )
	EmergencyResVolumeMultiplier ( 11 )
	EmergencyResCapacity ( 0.88 )
	EmergencyResChargingRate ( 1 )
	EmergencyBrakeResMaxPressure ( 73 )

	Inside (
	PassengerCabinFile ( cdc_130001.s )
	PassengerCabinHeadPos ( -1.6 3.0 6.58 )
		RotationLimit ( 0 190 0 )
		StartDirection ( 0 180 0 )
	)

comment	( Lights )


 
comment ( svetelne kuzely ) 

	Lights ( 36
		Light (
			  comment ( Svetelny kuzel dalkovy )
			  Type ( 1 )
				  Conditions (
					  Headlight ( 3 )
					  Unit ( 2 )
					  Control ( 2 )
			  )
			  FadeIn ( 1 )
			  FadeOut ( 1 )
			  Cycle ( 0 )
			  States ( 1
				  State (
					  Duration ( 0 )
					  LightColour ( FFFFEBA4 )
					  Position ( 0.0 3 3 )
					  Angle ( 10 )
					  Transition ( 1 )
					  Radius ( 300 )
			  		)
			  	)
			)
		Light (
			  comment ( Svetelny kuzel tlumeny )
			  Type ( 1 )
			  Conditions (
				  Headlight ( 2 )
				  Unit ( 2 )
				  Control ( 2 )
			  )
			  FadeIn ( 0.5 )
			  FadeOut ( 0.5 )
			  States ( 1
				  State (
					  Duration ( 0 )
					  LightColour ( FF444444 )
					  Position ( 0.0 3 3 )
					  Angle ( 30 )
					  Transition ( 1 )
					  Radius ( 150 )
					)
				)
			)

comment ( Definice svetel pro predni stanoviste v cele vlaku )



		Light (
			comment ( reflektor dalkovy pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEBA4 )
					Position ( 0.07 3.7 7.95  )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)		
		Light (
			comment ( reflektor dalkovy levy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEBA4 )
					Position ( -0.07 3.7 7.98  )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor tlumeny pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( 0.07 3.7 7.95  )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( reflektor tlumeny levy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( -0.07 3.7 7.98  )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)		
		

		
		Light (
			comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.557 1.92 8.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.557 1.92 8.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.557 1.92 8.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.557 1.92 8.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)		
		Light (
			comment ( Zadni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.557 1.92 -8.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Zadni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.557 1.92 -8.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		
comment ( Definice svetel pro predni stanoviste na postrku )

		Light (
			comment ( Zadni prave koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.8 1.92 -8.050 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Zadni leve koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.8 1.92 -8.050 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)


comment ( Definice svetel pro zadni stanoviste v cele vlaku )

		Light (
			comment ( reflektor dalkovy pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEBA4 )
					Position ( 0.07 3.7 -7.95  )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor dalkovy levy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEBA4 )
					Position ( -0.07 3.7 -7.98  )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)

		Light (
			comment ( reflektor tlumeny pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( 0.07 3.7 -7.95  )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( reflektor tlumeny levy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( -0.07 3.7 -7.98  )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)


		
		Light (
			comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.557 1.92 -8.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.557 1.92 -8.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
comment ( Definice svetel pro zadni stanoviste na postrku )
		
		Light (
			comment ( Zadni prave koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.8 1.92 8.050 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light ( 
			comment ( zadni leve koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.8 1.92 8.050 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)



		
comment ( Definice svetel pro loko ovladanou PC v normanim smeru )


		Light (
			comment ( PC reflektor pravy predni tlumeny v noci )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( 0.07 3.7 7.95  )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC reflektor levy predni tlumeny v noci )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( -0.07 3.7 7.98  )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)		
		
		Light (
			comment ( PC reflektor pravy predni tlumeny ve dne za deste )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 1 )
				Weather ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( 0.07 3.7 7.95  )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC reflektor levy predni tlumeny ve dne za deste )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 1 )
				Weather ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( -0.07 3.7 7.98  )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)

		
		Light (
			comment ( PC reflektor pravy predni tlumeny ve dne za snehu )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 1 )
				Weather ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( 0.07 3.7 7.95  )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC reflektor levy predni tlumeny ve dne za snehu )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 1 )
				Weather ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( -0.07 3.7 7.95  )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)

	
		
		Light (
			comment ( PC predni leve v cele soupravy normalni smer )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFFE085 )
					Position ( -0.557 1.92 8.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		Light (
			comment ( PC predni prave v cele soupravy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.557 1.92 8.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC koncove leve na konci soupravy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.8 1.92 -8.050 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC koncove prave na konci soupravy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.8 1.92 -8.050 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		

comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Leve predni pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.557 1.92 8.05 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( Prave predni pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position (0.557 1.92 8.05 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( Leve zadni pozicni - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.557 1.92 -8.05 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( Prave zadni pozicni - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.557 1.92 -8.05 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
			)
		)
	)
	Sound ( "..\\..\\common.snd\\sndelok\\130eng.sms" )
)
Engine ( cdc_130001
	Wagon ( cdc_130001 )
	Type ( Electric )
	MaxPower ( 2457kW )
	MaxForce ( 1651kN )
	MaxContinuousForce ( 1651kN )
	MaxVelocity ( 110km/h )
	DieselEngineSpeedOfMaxTractiveEffort ( 0mph )
	MaxCurrent ( 6127A )
	WheelRadius ( 0.625m )
	Sanding ( 1e9mph )
	NumWheels ( 4 )

	AirBrakesAirCompressorPowerRating ( 1.18 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 144 )
	AirBrakesMainResVolume ( 38.85 )
	AirBrakesAirCompressorWattage ( 15000 )
	AirBrakesCompressorRestartPressure ( 121 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 3 )
	TrainBrakesControllerMaxApplicationRate ( 1 )
	TrainBrakesControllerMaxReleaseRate ( 0.5 )
	TrainBrakesControllerMaxQuickReleaseRate ( 1.5 )
	TrainBrakesControllerEmergencyApplicationRate ( 3 )
	TrainBrakesControllerMinSystemPressure ( 3 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22 )
	TrainPipeLeakRate ( 0.033 )
	TrainBrakesControllerFullServicePressureDrop ( 22 )

	BrakesEngineBrakeType ( "Air_single_pipe"  )
	BrakesTrainBrakeType ( "Air_single_pipe" )
	BrakesEngineControllers ( "Independent, Train" )

	EngineBrakesControllerDirectControlExponent ( 1 )

	DoesBrakeCutPower ( 1 )
	
	EmergencyStopMonitor (
	  MonitoringDeviceMonitorTimeLimit ( 0 )
	  MonitoringDeviceAlarmTimeLimit ( 0 )
	  MonitoringDevicePenaltyTimeLimit ( 0 )
	  MonitoringDeviceCriticalLevel ( 0 )
	  MonitoringDeviceResetLevel ( 0 )
	  MonitoringDeviceAppliesFullBrake ( 0 )
	  MonitoringDeviceAppliesEmergencyBrake ( 0 )
	  MonitoringDeviceAppliesCutsPower ( 1 )
	  MonitoringDeviceAppliesShutsDownEngine ( 0 )
	  MonitoringDeviceResetOnZeroSpeed ( 1 ) 

	 )
	 VigilanceMonitor (
	  MonitoringDeviceMonitorTimeLimit ( 27 )
	  MonitoringDeviceAlarmTimeLimit ( 17 )
	  MonitoringDevicePenaltyTimeLimit ( 0 )
	  MonitoringDeviceCriticalLevel ( 0 )
	  MonitoringDeviceResetLevel ( 0 )

	  MonitoringDeviceAppliesFullBrake ( 0 )
	  MonitoringDeviceAppliesEmergencyBrake ( 1 )
	  MonitoringDeviceAppliesCutsPower ( 1 )
	  MonitoringDeviceAppliesShutsDownEngine ( 0 )
	  MonitoringDeviceResetOnZeroSpeed ( 1 )
	  MonitoringDeviceResetOnResetButton ( 1 )
	  MonitoringDeviceResetOnDirectionNeutral ( 1 )
	 )
	 OverspeedMonitor (
	  MonitoringDeviceMonitorTimeLimit ( 0 )
	  MonitoringDeviceAlarmTimeLimit ( 5 )
	  MonitoringDevicePenaltyTimeLimit ( 0 )
	  MonitoringDeviceCriticalLevel ( 65 )
	  MonitoringDeviceResetLevel ( 0 )
	  Comment ( MonitoringDeviceTriggerOnHighCurrent ( 800 ) )
	  MonitoringDeviceAppliesFullBrake ( 0 )
	  MonitoringDeviceAppliesEmergencyBrake ( 1 )
	  MonitoringDeviceAppliesCutsPower ( 0 )
	  MonitoringDeviceAppliesShutsDownEngine ( 0 )
	  MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
	  MonitoringDeviceDoesSuppressionReset ( 0 )
	  MonitoringDeviceTriggerOnOverspeed ( 65.1 )
	  MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
	  MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
	  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
	  MonitoringDeviceResetOnResetButton ( 0 )
	 )

	CabView ( "../../common.cab/cab130/130.cvf" )
	HeadOut (1.7 3.2 6.5 )

	DoesBrakeCutPower ( 1 )
	MaxSandingTime ( 600 )
	DoesHornTriggerBell ( 0 )

	EngineControllers (
		Throttle ( 0 1 0.005 0
			NumNotches ( 44
				Notch ( 0.000 0 Dummy )
				Notch ( 0.004 0 Dummy )

				Notch ( 0.01  0 Dummy )
				Notch ( 0.03  0 Dummy )
				Notch ( 0.05  0 Dummy )
				Notch ( 0.06  0 Dummy )
				Notch ( 0.08  0 Dummy )

				Notch ( 0.09  0 Dummy )
				Notch ( 0.11  0 Dummy )
				Notch ( 0.12  0 Dummy )
				Notch ( 0.13  0 Dummy )
				Notch ( 0.14  0 Dummy )

				Notch ( 0.15  0 Dummy )
				Notch ( 0.17  0 Dummy )
				Notch ( 0.19  0 Dummy )
				Notch ( 0.20  0 Dummy )
				Notch ( 0.22  0 Dummy )

				Notch ( 0.23  0 Dummy )
				Notch ( 0.25  0 Dummy )
				Notch ( 0.26  0 Dummy )
				Notch ( 0.28  0 Dummy )
				Notch ( 0.29  0 Dummy )

				Notch ( 0.31  0 Dummy )
				Notch ( 0.32  0 Dummy )
				Notch ( 0.34  0 Dummy )
				Notch ( 0.35  0 Dummy )

				Notch ( 0.36  0 Dummy )

				Notch ( 0.38  0 Dummy )
				Notch ( 0.41  0 Dummy )
				Notch ( 0.44  0 Dummy )
				Notch ( 0.46  0 Dummy )
				Notch ( 0.49  0 Dummy )

				Notch ( 0.52  0 Dummy )
				Notch ( 0.55  0 Dummy )
				Notch ( 0.58  0 Dummy )
				Notch ( 0.61  0 Dummy )
				Notch ( 0.64  0 Dummy )

				Notch ( 0.66  0 Dummy )
				Notch ( 0.69  0 Dummy )

				Notch ( 0.75  0 Dummy )
				Notch ( 0.81  0 Dummy )
				Notch ( 0.87  0 Dummy )

				Notch ( 0.93  0 Dummy )
				Notch ( 1     0 Dummy )
			)
		)
		comment (***Primocinna brzda typ DAKO-BP***)
		Brake_Engine ( 0 0.76 0.05 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		comment (***Prubezna brzda typ DAKO-BS2***)
		Brake_Train ( 0 1 0.04 0.87
			NumNotches ( 7
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
				Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)
		Brake_Hand ( 0 1 0.125 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		DirControl ( -1 0 1 1 )
		EmergencyStopToggle ( 0 1 0 )
		AWS ( 0 1 0 )
		Sanding ( 0 1 0 )
		Horn ( 0 1 0 )
		BellToggle ( 0 1 0 )
		Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
 		PantographToggle2 ( 0 1 0 )
 		PantographsToggle_4 ( 0 1 0 )
		Headlights ( 0 0.25 1 0 )
		Wipers ( 0 1 0 )
		BailOffButton ( 0 1 0 )
	)
	Name ( "CDC 130 001-1" )
	Description (
		"Rada 130 CDC je univerzalni elektricka skrinova lokomotiva, pouzivana v nakladni i osobni doprave.\n\n"+
		"Typ Bo'-Bo', napeti 3 kV ss.\n\n"+
		"Delka pres narazniky: 17,21 m\n\n"+
		"Prumer hnacich kol: 1250 mm\n\n"+
		"Hmotnost ve sluzbe: 85 t\n\n"+
		"Trvaly vykon trakcnich motoru: 2040 kW\n\n"+
		"Max. rychlost 100 km/h\n\n"
	)
	EngineOperatingProcedures (
	"Ovladani dle vlastniho nastaveni klavesnice"
	)
	Sound ( "..\\..\\common.snd\\sndelok\\130cab.sms" )
)