SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( csd_350015_hk
	Type ( Engine ) 
	WagonShape ( csd_350015_hk.s )
        Freightanim ( csd_350015fg_hk.s 1 1 ) 
        Size ( 3.08m 4.63m 16.857m ) 
	Comment ( autor eng souboru bob57_cz - dne 22-12-2007 upravil dle norem TBP Radim Hamr )
	Comment ( upraveno bylo smerovani zvuku a kabiny a vychozi poloha brzdice BSE )
        Comment ( Upravil Robo 10/2011 )
	CentreOfGravity ( 0m 2.25m 0m ) 
	Mass ( 89t ) 
	WheelRadius ( 0.625m ) 
	InertiaTensor ( Box ( 3.08m 4.63m 16.557m ) ) 

	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)

comment ( sucho mez=160kN=860A skluz=65kN ) 
	Adheasion ( 0.25 0.61 1.2 0 ) 

        NumWheels ( 4 ) 
	PassengerCapacity ( 10 ) 

	DerailBufferForce ( 350kN ) 
	DerailRailForce ( 2.5*89t ) 
	DerailRailHeight ( 10cm ) 

	Friction ( 900N/m/s 0.05 1mph 18N/m/s 1.8 5.1N/rad/s 1 -1rad/s 0 1 ) 

	MaxBrakeForce( 29kN )
	MaxHandbrakeForce( 25kN )
	NumberOfHandbrakeLeverSteps( 100 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" ) 
	BrakeSystemType( "Air_single_pipe" )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 1.3 )
	MaxApplicationRate( 4 )
	MaxAuxilaryChargingRate( 3 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 11 )
	EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 )
	
	
	
comment	( Freight, Inside, IntakePoint )

		
   	
	Inside (
		PassengerCabinFile ( csd_350009_hk.s )
		PassengerCabinHeadPos ( -1.56 3.1 6.7 )
		RotationLimit ( 45 90 0 )
		StartDirection ( 0 -90 0 )
	)


comment ( Svetla Robo ) 

comment	( Lights )

	Lights ( 29
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFFF )
					Position ( 0 1 8 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 120 )
				)
			)
		)
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.12 3.714 7.363 )
					Azimuth ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.108 3.714 7.363 )
					Azimuth ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
                Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.768 1.747 7.816 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.768 1.747 7.816 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80FF0000 )
					Position ( -1.012 1.747 -7.816 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80FF0000 )
					Position ( 1.012 1.747 -7.816 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )

		Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.108 3.714 -7.363 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.108 3.714 -7.363 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
                Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.768 1.747 -7.816 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.768 1.747 -7.816 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( 1.012 1.747 7.816 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( -1.012 1.747 7.816 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                comment ( Definicia svetiel pre posunujuci diel )

		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.768 1.747 7.816 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.768 1.747 -7.816 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Pravé p?ední pozi?ní - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.768 1.747 7.816 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( Levé zadní pozi?ní - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.768 1.747 -7.816 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
               comment ( Definicia svetiel pre podvozky )
                Light (
			comment ( Prave predne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 1.470 0.86 5.209 )
					Azimuth ( 0 0 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		) 
                Light (
			comment ( Lave predne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -1.470 0.86 5.3 )
					Azimuth ( 0 -180 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)   
                Light (
			comment ( Prave zadne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 1.470 0.86 -5.3 )
					Azimuth ( 0 0 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		) 
                Light (
			comment ( Lave zadne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -1.470 0.86 -5.209 )
					Azimuth ( 0 -180 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)   
		

		comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( PC prední pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.768 1.747 7.816 )
					Azimuth ( 0 -5 5 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC prední levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.768 1.747 7.816 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( -1.012 1.747 -7.816 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( 1.012 1.747 -7.816 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)


	
	Sound ( "../../common.snd/sndX5X_OR/350eng_25kV.sms" )
	
) 

Engine ( csd_350015_hk
	Wagon ( csd_350015_hk ) 
	Type ( Electric ) 
	Name ( "CSD 350 015-4 HK" )
	Sound ( "../../common.snd/sndX5X_OR/350cab_25kV.sms" )
 	CabView ( ..//..//common.cab//cab350//350006.cvf )
        HeadOut ( 1.7 3.1 6.6 ) 

	MaxContinuousForce ( 1900kN ) 
	MaxCurrent ( 10180A ) 
	MaxForce ( 1900kN ) 
	MaxPower ( 4200kW ) 
	MaxSandingTime ( 600 ) 
	MaxVelocity ( 155km/h ) 
	NumWheels ( 4 ) 
	Sanding ( 160km/h ) 
	WheelRadius ( 0.625m ) 

	AirBrakesAirCompressorPowerRating ( 1.5 ) 
	AirBrakesAirCompressorWattage ( 34kW ) 
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 2 ) 
	AirBrakesCompressorRestartPressure ( 116 ) 
	AirBrakesHasLowPressureTest ( 0 ) 
	AirBrakesIsCompressorElectricOrMechanical ( 0 ) 
	AirBrakesMainMaxAirPressure ( 144 ) 
	AirBrakesMainMinResAirPressure ( 116 ) 
	AirBrakesMainResVolume ( 38 ) 

	BrakeCutsPowerAtBrakeCylinderPressure ( 25 ) 
	BrakesEngineBrakeType ( "Air_single_pipe" ) 
	BrakesEngineControllers	( "Independent, Train, Dynamic" ) 
	BrakesTrainBrakeType ( "Air_single_pipe" ) 

	DieselEngineSpeedOfMaxTractiveEffort ( 0km/h ) 

	DoesBrakeCutPower ( 1 ) 
	DoesHornTriggerBell ( 0 ) 

	DynamicBrakeHasAutoBailOff ( 1 ) 
	DynamicBrakesDelayTimeBeforeEngaging ( 0 ) 
	DynamicBrakesMaxAirBrakePressure ( 8 ) 
	DynamicBrakesMaximumForce ( 100kN ) 
	DynamicBrakesNumberOfControllerNotches ( 10 ) 
	DynamicBrakesResistorCurrentLimit ( 600 ) 

	DynamicBrakesMaximumSpeedForFadeOut ( 165 ) 
	DynamicBrakesHigherSpeedCurveExponent ( 1.5 ) 
	DynamicBrakesMaximumEffectiveSpeed ( 70 ) 
	DynamicBrakesFadingSpeed ( 32 ) 
	DynamicBrakesLowerSpeedCurveExponent ( 1.5 ) 
	DynamicBrakesMinUsableSpeed ( 15 ) 
	DynamicBrakesCutInSpeed ( 14.5 ) 
	DynamicBrakesEffectAtMaximumFadeOut ( 1 ) 

	EngineBrakesControllerDirectControlExponent ( 1 ) 
	EngineBrakesControllerEmergencyApplicationRate ( 3 ) 
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 ) 
	EngineBrakesControllerFullServicePressureDrop ( 73 ) 
	EngineBrakesControllerHasProportionalBrake ( 0 ) 
	EngineBrakesControllerMaxApplicationRate ( 3 ) 
	EngineBrakesControllerMaxReleaseRate ( 3 ) 
	EngineBrakesControllerMaxSystemPressure ( 73 ) 
	EngineBrakesControllerMinPressureReduction ( 1 ) 
	EngineBrakesControllerMinSystemPressure ( 0 ) 
	EngineBrakesProportionalBrakeLag ( 1.0 ) 

	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 ) 
	TrainBrakesControllerMaxQuickReleaseRate ( 4 ) 
	TrainBrakesControllerMaxReleaseRate ( 2 ) 
	TrainBrakesControllerMinPressureReduction ( 1 ) 
	TrainBrakesControllerMaxApplicationRate ( 2 ) 
	TrainBrakesControllerEmergencyApplicationRate ( 10 ) 
	TrainBrakesControllerMaxSystemPressure ( 73 ) 
	TrainBrakesControllerFullServicePressureDrop ( 73 ) 
	TrainBrakesControllerMinSystemPressure ( 0 ) 
	TrainPipeLeakRate ( 0.01 ) 

	OverspeedMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0 )
  MonitoringDeviceAlarmTimeLimit ( 5 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 103.7 )
  MonitoringDeviceResetLevel ( 0 )
  Comment ( MonitoringDeviceTriggerOnHighCurrent ( 1150 )  )
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  Comment ( MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 ) )
  MonitoringDeviceDoesSuppressionReset ( 0 )
  MonitoringDeviceTriggerOnOverspeed ( 103.7 )
  MonitoringDeviceTriggerOnTrackOverspeed ( 0 )
  MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnResetButton ( 0 )
 )		

	comment ( Monitors )


EmergencyStopMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0 )
  MonitoringDeviceAlarmTimeLimit ( 0 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 0 )
  MonitoringDeviceResetLevel ( 0 )
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  
 )
 VigilanceMonitor (
  MonitoringDeviceMonitorTimeLimit ( 27 )
  MonitoringDeviceAlarmTimeLimit ( 17 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 0 )
  MonitoringDeviceResetLevel ( 0 )
  
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceResetOnZeroSpeed ( 1 )
  MonitoringDeviceResetOnResetButton ( 1 )
  MonitoringDeviceResetOnDirectionNeutral ( 1 )
 )

 OverspeedMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0 )
  MonitoringDeviceAlarmTimeLimit ( 5 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 103.7 )
  MonitoringDeviceResetLevel ( 0 )
  Comment ( MonitoringDeviceTriggerOnHighCurrent ( 1150 )  )
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  Comment ( MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 ) )
  MonitoringDeviceDoesSuppressionReset ( 0 )
  MonitoringDeviceTriggerOnOverspeed ( 103.7 )
  MonitoringDeviceTriggerOnTrackOverspeed ( 0 )
  MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnResetButton ( 0 )
 )		

	EngineControllers ( 

	AWS ( 0 1 0 ) 
	BailOffButton ( 0 1 0 ) 
	BellToggle ( 0 1 0 ) 

	Brake_Engine ( 0 1 0.08 0 
	NumNotches ( 1 
	Notch ( 0 1 Dummy ) 
	) ) 
    
	Brake_Dynamic ( 0 1 0.01 0 
	NumNotches ( 13 
	Notch ( 0.00 0 Dummy ) 
	Notch ( 0.10 0 Dummy ) 
	Notch ( 0.20 0 Dummy ) 
	Notch ( 0.30 0 Dummy ) 
	Notch ( 0.40 0 Dummy ) 
	Notch ( 0.50 0 Dummy ) 
	Notch ( 0.60 0 Dummy ) 
	Notch ( 0.70 0 Dummy ) 
	Notch ( 0.80 0 Dummy ) 
	Notch ( 0.90 0 Dummy ) 
	Notch ( 1.00 0 Dummy ) 
	Notch ( 1.10 0 Dummy ) 
	Notch ( 1.20 0 Dummy ) 
	) ) 

	Brake_Hand ( 0 1 0.05 0 
	NumNotches	( 1 
	Notch ( 0 1 Dummy ) 
	) )

	Brake_Train ( 0 1 0.1 0.7 
	NumNotches ( 5 
	Notch ( 0.0 0 TrainBrakesControllerFullQuickReleaseStart ) 
	Notch ( 0.3 0 TrainBrakesControllerReleaseStart ) 
	Notch ( 0.5 0 TrainBrakesControllerApplyStart ) 
	Notch ( 0.7 0 TrainBrakesControllerContinuousServiceStart ) 
	Notch ( 0.9 0 TrainBrakesControllerEmergencyStart ) 
	) ) 

	Combined_Control ( 0 2 1 1  throttle dynamic ) 
	DirControl ( -1 0 1 1 ) 
	EmergencyStopToggle ( 0 1 0 ) 
	Headlights ( 0 0.25 1 0 ) 
	Horn ( 0 1 0 ) 
	PantographToggle1 	( 0 1 0 )
        PantographToggle2 	( 0 1 0 )
        PantographsToggle_4 	( 0 1 0 )
	Sanding ( 0 1 0 ) 

	Throttle ( 0 1 0.01 0 
	NumNotches ( 113 
	Notch ( 0.000 0 Dummy ) 
	Notch ( 0.001 0 Dummy ) 
	Notch ( 0.002 0 Dummy ) 
	Notch ( 0.019 1 Dummy ) 
	Notch ( 0.020 0 Dummy ) 
	Notch ( 0.039 1 Dummy ) 
	Notch ( 0.040 0 Dummy ) 
	Notch ( 0.059 1 Dummy ) 
	Notch ( 0.060 0 Dummy ) 
	Notch ( 0.079 1 Dummy ) 
	Notch ( 0.080 0 Dummy ) 

	Notch ( 0.099 1 Dummy ) 
	Notch ( 0.100 0 Dummy ) 
	Notch ( 0.119 1 Dummy ) 
	Notch ( 0.120 0 Dummy ) 
	Notch ( 0.139 1 Dummy ) 
	Notch ( 0.140 0 Dummy ) 
	Notch ( 0.159 1 Dummy ) 
	Notch ( 0.160 0 Dummy ) 
	Notch ( 0.179 1 Dummy ) 
	Notch ( 0.180 0 Dummy ) 

	Notch ( 0.199 1 Dummy ) 
	Notch ( 0.200 0 Dummy ) 
	Notch ( 0.209 1 Dummy ) 
	Notch ( 0.210 0 Dummy ) 
	Notch ( 0.219 1 Dummy ) 
	Notch ( 0.220 0 Dummy ) 
	Notch ( 0.239 1 Dummy ) 
	Notch ( 0.240 0 Dummy ) 
	Notch ( 0.259 1 Dummy ) 
	Notch ( 0.260 0 Dummy ) 

	Notch ( 0.279 1 Dummy ) 
	Notch ( 0.280 0 Dummy ) 
	Notch ( 0.299 1 Dummy ) 
	Notch ( 0.300 0 Dummy ) 
	Notch ( 0.319 1 Dummy ) 
	Notch ( 0.320 0 Dummy ) 
	Notch ( 0.339 1 Dummy ) 
	Notch ( 0.340 0 Dummy ) 
	Notch ( 0.359 1 Dummy ) 
	Notch ( 0.360 0 Dummy ) 

	Notch ( 0.379 1 Dummy ) 
	Notch ( 0.380 0 Dummy ) 
	Notch ( 0.399 1 Dummy ) 
	Notch ( 0.400 0 Dummy ) 
	Notch ( 0.419 1 Dummy ) 
	Notch ( 0.420 0 Dummy ) 
	Notch ( 0.439 1 Dummy )	
	Notch ( 0.440 0 Dummy ) 
	Notch ( 0.459 1 Dummy ) 
	Notch ( 0.460 0 Dummy ) 

	Notch ( 0.479 1 Dummy ) 
	Notch ( 0.480 0 Dummy ) 
	Notch ( 0.499 1 Dummy ) 
	Notch ( 0.500 0 Dummy ) 


	Notch ( 0.529 1 Dummy ) 
	Notch ( 0.530 0 Dummy ) 
	Notch ( 0.559 1 Dummy ) 
	Notch ( 0.560 0 Dummy ) 
	Notch ( 0.589 1 Dummy ) 
	Notch ( 0.590 0 Dummy ) 
	Notch ( 0.619 1 Dummy ) 
	Notch ( 0.620 0 Dummy ) 
	Notch ( 0.649 1 Dummy ) 
	Notch ( 0.650 0 Dummy ) 

	Notch ( 0.659 1 Dummy ) 
	Notch ( 0.660 0 Dummy ) 
	Notch ( 0.669 1 Dummy ) 
	Notch ( 0.670 0 Dummy ) 
	Notch ( 0.679 1 Dummy ) 
	Notch ( 0.680 0 Dummy ) 

	Notch ( 0.699 1 Dummy ) 
	Notch ( 0.700 0 Dummy ) 
	Notch ( 0.719 1 Dummy ) 
	Notch ( 0.720 0 Dummy ) 
	Notch ( 0.739 1 Dummy ) 
	Notch ( 0.740 0 Dummy ) 
	Notch ( 0.759 1 Dummy ) 
	Notch ( 0.760 0 Dummy ) 
	Notch ( 0.779 1 Dummy ) 
	Notch ( 0.780 0 Dummy ) 

	Notch ( 0.799 1 Dummy ) 
	Notch ( 0.800 0 Dummy ) 
	Notch ( 0.819 1 Dummy ) 
	Notch ( 0.820 0 Dummy ) 
	Notch ( 0.839 1 Dummy ) 
	Notch ( 0.840 0 Dummy ) 
	Notch ( 0.859 1 Dummy ) 
	Notch ( 0.860 0 Dummy ) 
	Notch ( 0.879 1 Dummy ) 
	Notch ( 0.880 0 Dummy ) 

	Notch ( 0.899 1 Dummy ) 
	Notch ( 0.900 0 Dummy ) 
	Notch ( 0.919 1 Dummy ) 
	Notch ( 0.920 0 Dummy ) 
	Notch ( 0.939 1 Dummy ) 
	Notch ( 0.940 0 Dummy ) 
	Notch ( 0.959 1 Dummy ) 
	Notch ( 0.960 0 Dummy ) 
	Notch ( 0.979 1 Dummy ) 
	Notch ( 0.980 0 Dummy ) 

	Notch ( 0.999 1 Dummy ) 
	Notch ( 1.000 0 Dummy ) 

	Notch ( 1.049 1 Dummy ) 
	Notch ( 1.050 0 Dummy ) 
	Notch ( 1.099 1 Dummy ) 
	Notch ( 1.100 0 Dummy ) 
	Notch ( 1.149 1 Dummy ) 
	Notch ( 1.150 0 Dummy ) 
	Notch ( 1.199 1 Dummy ) 
	Notch ( 1.200 0 Dummy ) 
	Notch ( 1.249 1 Dummy ) 
	Notch ( 1.250 0 Dummy ) 
	) ) 

	Vigilance ( 0 1 0 ) 
	Wipers ( 0 1 0 ) 
	) 

	Description ( 
	"Rada ZSSK 350 je elektricka skrinova lokomotiva, pouzivana zejmena v rychlikove doprave.\n"+ 
	"Typ Bo'Bo', napeti 3kV ss. 25kV 50hz\n\n"+ 
	"Delka pres narazniky: 16,74 m\n\n"+ 
	"Prumer hnacich kol: 1250 mm\n\n"+ 
	"Hmotnost ve sluzbe: 89 t\n\n"+ 
	"Trvaly vykon trakcnich motoru: 4000 kW\n\n"+ 
	"Max. rychlost 160 km/h\n\n"+ 
	" "+ 
	"Autor modelu ZSSK 350 002 Jiri Tovacovsky \n\n"+ 
	"verze chovani bob57_cz 2007-11-07-bin 2P4c\n"+ 
	" "
	) 

	EngineOperatingProcedures (
		" Ovladani podle vlastniho nastaveni klaves v simulatoru\n\n" +
		" "
	) 
) 
