SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( "CSD_M152-0461"
	comment( upravil Ppoollll, Jacek, Frinta - verze 3.0 )
	comment( elektricky prenos vykonu )
	Type ( Engine )
	WagonShape ( "CSD_M152-0461.s" )

	Size ( 3.47m 3.73m 13.54m )
	Mass ( 24t )
	WheelRadius ( 46cm )
	CentreOfGravity ( 0m 1.5m 0m )
	InertiaTensor ( Box ( 3.47m 3.73m 13.54m ) )
        Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5E6N/m 1E7N/m )
			Damping ( 1E6N/m/s 2E6N/m/s )
			Break ( 1.1E7N 5E7N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5E6N/m 1E7N/m )
			Damping ( 1E6N/m/s 2E6N/m/s )
			Break ( 1.1E7N 5E7N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1E6N/m 5E6N/m )
			Damping ( 1E6N/m/s 1E6N/m/s )
			r0 ( 60cm 30cm )
		)
		Centre ( 0.5m )
		Radius ( 1m )
		Angle ( 0.5deg )
	)

	Adheasion ( 0.2 0.35 0.8 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*22t )
	DerailBufferForce ( 100kN )
	NumWheels ( 1 )
	Friction (
		398.2N/m/s		-0.1		1mph		7.366N/m/s		2.0
		5.1N/rad/s		1		-1rad/s		0		1
	)
	
	BrakeEquipmentType( "Handbrake, Graduated_release_Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 20kN )
	MaxHandbrakeForce( 8kN )
	NumberOfHandbrakeLeverSteps( 100 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 1.3 )
	MaxApplicationRate( 4 )
	MaxAuxilaryChargingRate( 3 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 8 )
	EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate ( 1 )
	EmergencyBrakeResMaxPressure( 73 )

	Inside (
		PassengerCabinFile ( "810int.s" )
		PassengerCabinHeadPos ( 1.08 2.3 0.237 )
		RotationLimit ( 60 80 0 )
		StartDirection ( 0 0 0 )
	)

	IntakePoint ( 2 2 FuelDiesel )
	
	PassengerCapacity ( 8.0 )

	Lights ( 36
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				TimeOfDay ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( 0 3.38 18 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 400 )
				)
			)
		)
		Light (
			comment ( Svetelný kuzel tlumený )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				TimeOfDay ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( 0 3.38 15 )
					Angle ( 30 )
					Transition ( 1 )
					Radius ( 50 )
				)
			)
		)

		comment ( Definice svetel pro prední stanoviste )

		Light (
			comment ( reflektor levý dálkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff  )
					Position ( -0.14 3.38 6.45 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.4 )
				)
			)
		)
		Light (
			comment ( reflektor pravý dálkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( 0.14 3.38 6.45 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.4 )
				)
			)
		)
		Light (
			comment ( reflektor levý tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( -0.14 3.38 6.45 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( reflektor pravý tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( 0.14 3.38 6.45 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( Prední levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFFF )
					Position ( -0.98 1.7 6.43 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFFF )
					Position ( 0.98 1.7 6.43 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( -0.98 1.7 6.43 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( 0.98 1.7 6.43 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFFF )
					Position ( -0.98 1.7 -6.43 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( zadní pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFFF )
					Position ( 0.98 1.7 -6.43 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -1.31 1.7 -6.43 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 1.31 1.7 -6.43 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )

		Light (
			comment ( reflektor levý dálkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( -0.16 3.38 -6.45 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.4 )
				)
			)
		)
		Light (
			comment ( reflektor pravý dálkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( 0.16 3.38 -6.45 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.4 )
				)
			)
		)
		Light (
			comment ( reflektor levý tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( -0.16 3.38 -6.45 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( reflektor pravý tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( 0.16 3.38 -6.45 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.4 )
				)
			)
		)
		Light (
			comment ( Prední levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFFF )
					Position ( -0.98 1.7 -6.43 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFFF )
					Position ( 0.98 1.7 -6.43 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( -0.98 1.7 -6.43 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( 0.98 1.7 -6.43 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFFF )
					Position ( -0.98 1.7 6.43 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( zadní pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFFF )
					Position ( 0.98 1.7 6.43 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -1.31 1.7 6.43 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 1.31 1.7 6.43 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Levé přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 70FFFFFF )
					Position ( -0.98 1.7 6.43 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( Pravé přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 70FFFFFF )
					Position ( 0.98 1.7 6.43 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( Levé zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 70FFFFFF )
					Position ( -0.98 1.7 -6.43 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( Pravé zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 70FFFFFF )
					Position ( 0.98 1.7 -6.43 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.4 )
					)
			)
		)

		comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( PC prední pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( 0.98 1.7 6.43 )
					Azimuth ( 0 -5 5 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( PC prední levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( -0.98 1.7 6.43 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( PC reflektor prední levý )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( -0.14 3.38 6.45 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC reflektor prední pravý )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffffffff )
					Position ( 0.14 3.38 6.45 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -1.31 1.7 -6.43 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 1.31 1.7 -6.43 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)

	Sound ( "../../common.snd/sndMlok/810eng.sms" )
)

Engine ( "CSD_M152-0461"
	Effects(
		DieselSpecialEffects(
			Exhaust1( -0.72 3.8 3.12
			0 1 0 
			0.15	)
		)
	)
	Wagon ( "CSD_M152-0461" )
	Type ( Diesel )
	MaxPower ( 135kW )
	MaxForce ( 29kN )
	MaxContinuousForce ( 16kN )
	MaxVelocity ( 80km/h )
	RunUpTimeToMaxForce ( 5 )
	WheelRadius ( 46cm )
	Sanding ( 10km/h )
	comment( pocet vsech naprav )
	NumWheels ( 2 )
	MaxTemperature ( 120 )
	MaxOilPressure ( 90 )

	AirBrakesAirCompressorPowerRating( 1.18 )
	AirBrakesMainMinResAirPressure( 56 )
	AirBrakesMainMaxAirPressure( 142 )
	AirBrakesMainResVolume( 7 )
	AirBrakesAirCompressorWattage( 19000 )
	AirBrakesCompressorRestartPressure( 121 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.5 )
	AirBrakesHasLowPressureTest( 1 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 3 )
	TrainBrakesControllerMaxApplicationRate ( 1 )
	TrainBrakesControllerMaxReleaseRate ( 0.5 )
	TrainBrakesControllerMaxQuickReleaseRate ( 1.5 )
	TrainBrakesControllerEmergencyApplicationRate ( 3 )
	TrainBrakesControllerMinSystemPressure ( 3 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22 )
	TrainPipeLeakRate ( 0.033 )
	TrainBrakesControllerFullServicePressureDrop ( 22 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train" )

	EngineBrakesControllerDirectControlExponent( 1 )

	CabView ( "../../common.cab/cab810/810.cvf" )
	HeadOut ( 1.9 2.8 6 )

	MaxDieselLevel( 300l )
	EngineVariables ( 280 )
	DieselUsedPerHourAtMaxPower ( 45l )
	DieselUsedPerHourAtIdle ( 4.5l )

	DieselSmokeEffectInitialMagnitude( 0.5 )
	DieselSmokeEffectMaxMagnitude( 1.1 )
	DieselSmokeEffectInitialSmokeRate( 0.2 )
	DieselSmokeEffectMaxSmokeRate( 2.1 )

	DieselEngineIdleRPM( 250 )
	DieselEngineStallRPM( 300 )
	DieselEngineMaxRPM( 2150 )
	DieselEngineSpeedOfMaxTractiveEffort( 19km/h )
	DieselEngineMaxRPMChangeRate( 500 )
	DieselEngineType( elektric )


	MaxSandingTime( 800 )
	comment( 320kg )

EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 20 )
		MonitoringDeviceAlarmTimeLimit ( 10 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 52.8 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 52.9 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 0 )
	)
	
	EngineControllers (
		Throttle ( 0 1 0.05 0
			NumNotches ( 0 )
		)
		Brake_Engine ( 0 1 0.05 0.0
			NumNotches( 1
				Notch( 0 1 Dummy )
			)
		)            
comment (***Prubezna brzda typ DAKO-BS2***)
		Brake_Train ( 0 1 0.04 0.85
			NumNotches ( 8
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
				Notch ( 0.34 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.76 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.85 0 TrainBrakesControllerContinuousServiceStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)
		Brake_Hand ( 0 1 0.025 0 
			NumNotches( 0 )
		)
		EngineBrakingButton( 0 1 0 )
		DirControl ( -1 0 1 1 )
		BellToggle( 0 1 0 )
		AWS ( 0 1 0 )
		Sanding ( 0 1 0 )
		Horn ( 0 1 0 )
		Wipers ( 0 1 0 )
		EmergencyStopToggle( 0 1 0 )
		Vigilance ( 0 1 0 )
		Headlights ( 0 0.25 1 0 )
		BailOffButton( 0 1 0 )
	)
	Name ( "CSD M152.0461" )
	Description (
		"Rada 810 Ceskych drah\n"+ 
		"Lehky motorovy vuz rady 810\n\n"+  
		"Prenos vykonu: hydromechanicky\n\n"+
		"Vykon: 155kW \n\n"+
		"Max. rychlost: 80km/h\n\n"+
		"Delka pres narazniky: 13970mm\n\n"+
		"Hmotnost: 19-25t\n\n"+
		"Napravy: 2 v usporadani 1'A'"
	)
	EngineOperatingProcedures (
		"Jak se rozjet\n"+
		"1.	Stisknete W na prepnutí prepinace smeru do polohy 'vpred'.\n"+
		"2.	Stisknete a drzte ; pro odbrzdení vlakové brzdy.\n"+
		"(3.	Stisknete a drzte [ pro odbrzdení lokomotivní brzdy.)\n"+
		"4.	Stisknete D pro zvýsení pozadovaného výkonu.\n"+
		"5.	Pomalu zvysujte výkon stiskem D, dokud vlak nedosáhne pozadované rychlosti. Pozor na prokluz! (F5 zobrazí jízdní údaje.)\n\n"+
		"Jak zpomalit\n"+
		"1.	Stisknete A pro snízení pozadovaného výkonu (postupne az na 0%).\n"+
		"2.	Jestlize je to nutné, tak pouzijte brzdy pro postupné rychlejsí snizování rychlosti.\n\n"+
		"Jak pouzít vlakovou brzdu\n"+
		"1.	Stisknete a drzte ' a dosáhnete pozadovaného brzdného tlaku (0-100%).\n\n"+
		"Jak odbrzdit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ; az presunete rukojet brzdy do polohy JÍZDA.\n\n"+
		"Jak pouzít lokomotvní brzdu\n"+
		"1.	Stisknete a drzte ] pro zabrzdení lokomotivní brzdy (0-100%).\n\n"+
		"Jak odbrzdit lokomotivní brzdu\n"+
		"1.	Stisknete a drzte [ pro odbrzdení lokomotivní brzdy (0-100%).\n\n"+
		"Jak pouzít zachrannou brzdu\n"+
		"1.	Stisknete BACKSPACE pro aktivaci záchrané brzdy.\n"+
		"2.	Stisknete a drzte A pro snízení výkonu az na 0%.\n\n"+
		"Jak zrusit záchrannou brzdu\n"+
		"1.	Pockejte na úplné zastavení vlaku.\n"+
		"2.	Stisknete Z pro odblokování ovládání lokomotivy.\n"+
		"3.	Stisknete ; a [ pro odbrzdení brzdných systému.\n\n"+
		" (Pozn.: Je-li rychlobrzda zavedena sama (pri prekroceni rychlosti nebo neobslouzeni zivaka), je po zastaveni nutno pockat 90s. Dríve nelze odbrzdit.\n\n"+
		"Výstup a nástup cestujících\n"+
		"1.	Zastavte ve stanici.\n"+
		"2.	Stisknete ENTER.\n"+
		"3.	Pockejte na signál k odjezdu.\n"+
		"TIP: Pro zobrazení casu príjezdu a odjezdu u této a následující stanice pouzijte klávesu F10.\n\n"+
		"Jak zmenit smer\n"+
		"1.	Zastavte.\n"+
		"2.	Stisknete 2x S na prepnutí prepinace smeru do polohy 'vzad'.\n"+
		"3.	Odbrzdete brzdy.\n"+
		"4.	Pomalu zvysujte výkon stiskem D.\n\n"+
		"Jak pripojit vagony/lokomotivy\n"+
		"1.	Najedte pomalu na soupravu (optimální rychlost 1 km/h).\n"+
		"Tip: Pro zobrazení pohledu na spráhlo stisknete klávesu 6.\n"+
		"2.	Stisknete F9 pro otevrení okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
		"3.	Jestlize je ikona vozu cervená, je zatazena rucní brzda. Dvojtukem mysí na voze uvolníte/zatáhne rucní brzdu.\n"+
		"4.	Zavrete okno sestavení vlaku stiskem F9.\n"+
		"5.	Pockejte az odbrzdíte pripojené vozy.\n\n"+
		"Odpojení vozu nebo lokomotivy\n"+
		"POZOR! Melo by se provádet jen tehdy, pokud VLAK STOJÍ!\n"+
		"1.	Otevrete okno sestavy vlaku F9.\n"+
		"2.	Poklepejte 2x na ikonu vozu, ktery se má odpojit, pokud chcete, aby mel vuz zatazenou rucní brzdu.\n"+
		"3.	Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
		"4.	Pomalu se rozjedte smerem od odpojene casti vlaku.\n"+
		" (Pozn.: V nekterých prípadech pri rychlejsím odjezdu dojde k opetovnému spojení spráhel. Pokud se toto stane tak soupravu opet rozpojte a velmi pomalu odjízdejte az do vzdálenosti jednoho prazce. Pak jiz muzete zacít zrychlovat.)\n"+
		"5.	Zavrete okno sestavení vlaku stiskem F9.\n\n"+
		"Jak doplnit naftu\n"+
		"1.	Zastavte u naftového stojanu stredem nádrze.\n"+
		"2.	Stisknete klávesu T a drzte ji po dobu doplnování nafty stisknutou.\n"+
		"TIP: Pro zobrazení prubehu plnení nádrze stisknete F9 a klepnete mysí na ikonu lokomotivy."
	)
	Sound ( "../../common.snd/sndMlok/810cab.sms" )
)
