SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( CSD_810-084ms_on
Comment ( "Sekce vozidlo" )
Comment ( "Popis fyziky vozu pro OR" )
Comment ( "Josef Vogeltanz - 01.06.2019" )
Comment ( "Upravy 19.12.2022" )
Comment ( "Upravy Dan J. 16.1.2023" )

Comment ( "Obecne informace vozu" )
Type ( Freight )
WagonShape ( CSD_810-084on.s )
Name ( "CSD 810.084-4 ms odst.noc ORCZ" )
Size ( 3.47m 3.824m 13.97m )
Mass ( 20t )
WheelRadius ( 0.42m )
ORTSNumberAxles ( 2 )


Comment ( "Sprahla" )
Coupling (
Type ( Chain )
Spring ( Stiffness ( 1.6e6N/m 1.1e8N/m ) Break ( 380kN 380kN ) r0 ( 0cm 2.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Coupling (
Type ( Chain )
Spring ( Stiffness ( 1.6e6N/m 1.1e8N/m ) Break ( 380kN 380kN ) r0 ( 0cm 2.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Comment ( "Brzdy" )
Comment ( "Brzdovy system DAKO, zdrze, Bv.: 20t" )
Comment ( "Rezim brzdeni P" )
BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

BrakeMassP ( 27t )
MaxBrakeForce ( 58kN )
MaxHandbrakeForce ( 12kN )
NumberOfHandbrakeLeverSteps ( 10 )

TripleValveRatio ( 2.5 )
MaxReleaseRate ( 0.2bar/s )
MaxApplicationRate ( 0.45bar/s )
MaxAuxilaryChargingRate ( 1.621bar/s )
EmergencyResChargingRate ( 1.621bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 3.8bar )
EmergencyResVolumeMultiplier ( 2.5 )
EmergencyResCapacity ( 75l )
BrakePipeVolume ( 12.5l )

ORTSBrakeShoeFriction (
0   0.310
8   0.238
16  0.193
24  0.168
32  0.152
40  0.140
48  0.131
56  0.123
64  0.116
72  0.109
80  0.105
88  0.101
96  0.098
104 0.096
112 0.094
120 0.093
128 0.092
136 0.092
144 0.092
152 0.092
160 0.092
)
Comment ( "Jizdni odpory a treni" )
CentreOfGravity ( 0m 1.91m  0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 8m 0mm )
ORTSUnbalancedSuperelevation ( 150mm )

ORTSBearingType ( Roller )
ORTSDavis_A ( 385.4 )
ORTSDavis_B ( 13.16 )
ORTSDavis_C ( 5.4625 )
ORTSWagonFrontalArea ( 8.9m^2 )

ORTSLengthBogieCentre ( 0m )
ORTSLengthCarBody ( 13.103m )
ORTSLengthCouplerFace ( 13.97m )
ORTSNumAxles ( 2 )
ORTSNumBogies ( 0 )
ORTSWheelFlangeLength ( 0.02m )
ORTSMaximumWheelFlangeAngle ( 70deg )

Comment ( "Ostatni informace" )
Sound  ( "..//..//common.snd//Vozy//010-OR.sms" )
)
