SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cd_Bt278_160  
	comment( sestavil Ondra Janis na zaklade poznatku o ladeni eng&wag souboru od Ppoolllla, Jacka, O.Frinty, ZSR  - verze 1.0; sprahla na 30cm )
	Type ( Carriage )
	Name ("CD Bt278 160")
	WagonShape ( cd_Bt278_160.s )
	Size ( 3m 4.2m 24.2m )
	CentreOfGravity ( 0m 1.9m 0m )
	Mass ( 38t )
	comment (hmotnost prazdneho vozu 34t, obsazeni 50 os.)
	WheelRadius ( 0.46m )
	InertiaTensor ( Box ( 3m 4.2m 24.2m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Adheasion ( 0.1 0.3 1.8 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*38t )
	DerailBufferForce ( 350kN )
	NumWheels ( 4 )
	
	Friction (
		1026N/m/s		0		0.625mph		0.84N/m/s		2
		5.1N/rad/s		1		-1rad/s		0		1
	)
	
	PassengerCapacity ( 150.0 )
	
	Inside (
		PassengerCabinFile ( "cd_Btee285_353_int.s" )
		PassengerCabinHeadPos ( 1.1 2.5 5.9 )
		RotationLimit ( 40 90 0 )
		StartDirection ( 0 0 0 )
		Sound ( "../../common.snd/Vozy/CDvuzOs4nIn.sms" )
	)


	Lights	(	10	
		Light	(
			comment( Koncova svetla - predni cvf 1 )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Service ( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.96 1.61 -12.103 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Koncova svetla - predni cvf 2 )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Service ( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.96 1.61 -12.103 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)	
		Light	(
			comment( Celni svetla/sunuty vlak - predni cvf 1 )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Service ( 2 )
				Unit ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.96 1.61 12.103 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Celni svetla/sunuty vlak - predni cvf 2 )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Service ( 2 )
				Unit ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.96 1.61 12.103 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)	
   	Light	(
			comment( Koncova svetla - zadni cvf 1 )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Service ( 2 )
				Unit ( 4 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.96 1.61 12.103 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Koncova svetla - zadni cvf 2 )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Service ( 2 )
				Unit ( 4 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.96 1.61 12.103 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Celni svetla/sunuty vlak - zadni cvf 1 )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Service ( 2 )
				Unit ( 5 )
				TimeOfDay ( 2 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.96 1.61 -12.103 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Celni svetla/sunuty vlak - zadni cvf 2 )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Service ( 2 )
				Unit ( 5 )
				TimeOfDay ( 2 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.96 1.61 -12.103 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)	
		Light	(
			comment( Koncova svetla - traffic 1 )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Control ( 1 )
				Service ( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.96 1.61 -12.103 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Koncova svetla - traffic 2 )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Control ( 1 )
				Service ( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.96 1.61 -12.103 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)	
	)

	BrakeEquipmentType( "handbrake, graduated_release_triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 33kN )
	comment(38t v rezimu P - zabrzdna draha 720m ze 120 km/h)
	comment(55t v rezimu R - zabrzdna draha 540m ze 120 km/h)

	MaxHandbrakeForce( 15kN )
	NumberOfHandbrakeLeverSteps( 100 )

	EmergencyBrakeResMaxPressure( 73 )	TripleValveRatio( 2.48 )
	MaxReleaseRate( 2.85 )
	comment (brzda v rezimu P - odbrzdeni cca. 16s)
	MaxApplicationRate( 4 )
  comment (brzda v rezimu P - plneni cca. 5s)
	MaxAuxilaryChargingRate( 10 )
	EmergencyResCapacity( 14 )
	EmergencyResChargingRate( 10 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 0.05 )

	Sound ( "../../common.snd/Vozy/CDvuzOs4nEx.sms" )
)

