SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cdc_230028
	Type ( Engine )
	WagonShape ( cdc_230028.s )
        Freightanim ( cdc_230028_2.s 1 1 )

	Comment ( 3D model a mapovanie textúr: p.Starý )
	Comment ( reSkin: Acatus 4/2022 )
  	Comment ( Svetla, strojvedoucí v cab: Tomazo )
	Comment ( Mezistěna: nebulus )
  	Comment ( uprava 1/2023 - doplneni trakcni charakteristiky a nastavení trakčního výkonu, adheze: Acatus )
	Comment ( 5/2020 uprava brzd - klon z rady 242 od Josefa Vogeltanze )

comment	( Overall physics )

	Mass ( 85t )
	Size  ( 3.03m 4.55m 16.48m )
	CentreOfGravity ( 0m 2.25m 0m )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box ( 3.03m 4.55m 16.48m ) )	

  ORTSFreightAnims (
   FreightAnimStatic (
   SubType ( Default )
   Shape   ( "vl_mecanoassis.s" )
   Offset  ( 0.44 1.75 -6.49 )
   )
   FreightAnimStatic (
   SubType ( Default )
   Shape ( "stin.s" )
   Offset ( 0.0 0.0 0.0 )
   )
   FreightAnimStatic (
   SubType ( Default )
   Shape   ( "240_medzistena.s" )
   Offset  ( 0.0 0.0 0.0 )
   )
   )
   
comment	( Coupling )

	Coupling (
            Type ( Chain )
            Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 0cm 5cm )
    )
    CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
            Type ( Chain )
            Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 0cm 10cm )
            )
    CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)

ORTSAdhesion (
ORTSCurtius_Kniffler ( 7.0 31 0.196 0.7 )
ORTSSlipWarningThreshold ( 60 )
ORTSWeatherCoefficients ( 1.0 0.63 0.6 )
)

DerailRailHeight ( 4cm )
DerailRailForce ( 307kN )
DerailBufferForce ( 400kN )

comment (** pocet naprav - vypocet adheze pro brzdeni **)
NumWheels ( 4 )

comment ( "jizdni odpor - treni" )
	Friction (
		1070.5N/m/s    -0.10    1.3mph    12.951N/m/s    1.891
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	)

comment	( Wagon Brakes )

 	Comment ( P=47kN, G=24kN )
 	
	MaxBrakeForce( 134kN )
	MaxHandbrakeForce( 48kN )
	NumberOfHandbrakeLeverSteps( 100 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 4 )
	MaxApplicationRate( 12.5 )
	MaxAuxilaryChargingRate( 3 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 11 )
	EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 )

  Comment ( "Pantografy" )
ORTSPantographs (
Pantograph (
Delay ( 5s )
)
Pantograph (
Delay ( 3s )
)
)


comment	(** Svetla - CDC 230.028-3 **)
	
	Lights ( 56
	        Light (
			comment ( svetelny kuzel dalkovy )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FFE8C0 )
					Position ( 0 2.5 8 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 120 )
				)
			)
		)
                Light (
			comment ( svetelny kuzel tlumeny )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
                                TimeOfDay ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 66FFE8C0 )
					Position ( 0 2.5 8 )
					Angle ( 15 )
					Transition ( 0 )
					Radius ( 20 )
				)
			)
		)
                Light (
                         comment ( svetelny kuzel posun )
                         Type ( 1 )
                         Conditions (
				Headlight ( 1 )
                                TimeOfDay ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
                         FadeIn ( 0.5 )
                         FadeOut ( 0.5 )
                         Cycle ( 0 )
                         States ( 1
                                 State (
                                         Duration ( 0 )
                                         LightColour ( 66FFE8C0 )
                                         Position ( 0 1.4 7.7 )
                                         Angle ( 50 )
                                         Elevation ( 0 10 0 )
                                         Transition ( 0 )
                                         Radius ( 10 )
                                )
                        )
                )

-----------------------------------------------------------------
                comment ( Definice svetel pro predni stanoviste )
-----------------------------------------------------------------

		Light (
			comment ( Reflektor levy dalkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEA99 )
					Position ( -0.08 3.835 7.48 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.31 )
				)
			)
		)
                Light (
			comment ( Reflektor levy tlumeny 1 )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( CCFFEA99 )
					Position ( -0.08 3.835 7.48 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                Light (
			comment ( Reflektor levy tlumeny 2 )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( BFFFF9E0 )
					Position ( -0.08 3.825 7.479 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.1 )
				)
			)
		)	
		Light (
			comment ( Reflektor pravy dalkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEA99 )
					Position ( 0.075 3.835 7.48 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.31 )
				)
			)
		)
                Light (
			comment ( Reflektor pravy tlumeny 1 )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( CCFFEA99 )
					Position ( 0.075 3.835 7.48 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                Light (
			comment ( Reflektor pravy tlumeny 2 )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( BFFFF9E0 )
					Position ( 0.075 3.825 7.479 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.1 )
				)
			)
		)
		Light (
			comment ( Predni prave zapnute 1 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( 0.63 1.73 7.52 )
					Azimuth ( 15 15 15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light (
			comment ( Predni prave zapnute 2 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( 0.63 1.705 7.518 )
					Azimuth ( 15 15 15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light (
			comment ( Predni leve zapnute 1 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( -0.63 1.73 7.52 )
					Azimuth ( -15 -15 -15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light (
			comment ( Predni leve zapnute 2 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( -0.63 1.705 7.518 )
					Azimuth ( -15 -15 -15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)		
		Light (
			comment ( Zadni prave koncove A )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( 0.73 1.73 -7.485 )
					Azimuth ( 160 160 160 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.27 )
				)
			)
		)
                Light (
			comment ( Zadni prave koncove B )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80FFE5C9 )
					Position ( 0.73 1.705 -7.483 )
					Azimuth ( 160 160 160 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light (
			comment ( Zadni leve koncove A )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( -0.73 1.73 -7.485 )
					Azimuth ( -160 -160 -160 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.27 )
				)
			)
		)
                Light (
			comment ( Zadni leve koncove B )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80FFE5C9 )
					Position ( -0.73 1.705 -7.483 )
					Azimuth ( -160 -160 -160 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)

----------------------------------------------------------------
                comment ( Definice svetel pro zadni stanoviste )
----------------------------------------------------------------

		Light (
			comment ( Reflektor levy dalkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEA99 )
					Position ( 0.08 3.835 -7.48 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.31 )
				)
			)
		)
                Light (
			comment ( Reflektor levy tlumeny 1 )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( CCFFEA99 )
					Position ( 0.08 3.835 -7.48 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                Light (
			comment ( Reflektor levy tlumeny 2 )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( BFFFF9E0 )
					Position ( 0.08 3.825 -7.479 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.1 )
				)
			)
		)
                Light (
			comment ( Reflektor pravy dalkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEA99 )
					Position ( -0.075 3.835 -7.48 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.31 )
				)
			)
		)
                Light (
			comment ( Reflektor pravy tlumeny 1 )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( CCFFEA99 )
					Position ( -0.075 3.835 -7.48 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                Light (
			comment ( Reflektor pravy tlumeny 2 )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.3 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( BFFFF9E0 )
					Position ( -0.075 3.825 -7.479 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 0 7 0 )
					Transition ( 0 )
					Radius ( 0.1 )
				)
			)
		)
		Light (
			comment ( Predni prave zapnute 1 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( 0.63 1.73 -7.52 )
					Azimuth ( 165 165 165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light (
			comment ( Predni prave zapnute 2 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( 0.63 1.705 -7.518 )
					Azimuth ( 165 165 165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light (
			comment ( Predni leve zapnute 1 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( -0.63 1.73 -7.52 )
					Azimuth ( -165 -165 -165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light (
			comment ( Predni leve zapnute 2 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( -0.63 1.705 -7.518 )
					Azimuth ( -165 -165 -165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)	
		Light (
			comment ( Zadni prave koncove A )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( 0.74 1.73 7.485 )
					Azimuth ( 20 20 20 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.27 )
				)
			)
		)
                Light (
			comment ( Zadni prave koncove B )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80FFE5C9 )
					Position ( 0.74 1.705 7.483 )
					Azimuth ( 20 20 20 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light ( 
			comment ( zadni leve koncove A )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( -0.74 1.73 7.485 )
					Azimuth ( -20 -20 -20 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.27 )
				)
			)
		)
                Light ( 
			comment ( zadni leve koncove B )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80FFE5C9 )
					Position ( -0.74 1.705 7.483 )
					Azimuth ( -20 -20 -20 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)

--------------------------------------------------------------
                comment ( Definice svetel pro posunujici dil )
--------------------------------------------------------------

                Light (
			comment ( Predni prave pozicni 1 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( 0.63 1.73 7.52 )
					Azimuth ( 15 15 15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light (
			comment ( Predni prave pozicni 2 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( 0.63 1.705 7.518 )
					Azimuth ( 15 15 15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light (
			comment ( Predni leve pozicni 1 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( -0.63 1.73 7.52 )
					Azimuth ( -15 -15 -15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light (
			comment ( Predni leve pozicni 2 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( -0.63 1.705 7.518 )
					Azimuth ( -15 -15 -15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light (
			comment ( Zadni prave pozicni 1 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( 0.63 1.73 -7.52 )
					Azimuth ( 165 165 165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light (
			comment ( Zadni prave pozicni 2 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( 0.63 1.705 -7.518 )
					Azimuth ( 165 165 165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light (
			comment ( Zadni leve pozicni 1 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( -0.63 1.73 -7.52 )
					Azimuth ( -165 -165 -165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light (
			comment ( Zadni leve pozicni 2 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( -0.63 1.705 -7.518 )
					Azimuth ( -165 -165 -165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)

-------------------------------------------------------------
                comment ( Definice svetel pro Loose consist )
-------------------------------------------------------------

		Light	(
			comment( Leve predni pozicni 1 - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( -0.63 1.73 7.52 )
					Azimuth ( -15 -15 -15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light	(
			comment( Leve predni pozicni 2 - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( -0.63 1.705 7.518 )
					Azimuth ( -15 -15 -15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light	(
			comment( Prave predni pozicni 1 - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( 0.63 1.73 7.52 )
					Azimuth ( 15 15 15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light	(
			comment( Prave predni pozicni 2 - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( 0.63 1.705 7.518 )
					Azimuth ( 15 15 15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light	(
			comment( Leve zadni pozicni 1 - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( -0.63 1.73 -7.52 )
					Azimuth ( -165 -165 -165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light	(
			comment( Leve zadni pozicni 2 - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( -0.63 1.705 -7.518 )
					Azimuth ( -165 -165 -165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light	(
			comment( Prave zadni pozicni 1 - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( 0.63 1.73 -7.52 )
					Azimuth ( 165 165 165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light	(
			comment( Prave zadni pozicni 2 - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( 0.63 1.705 -7.518 )
					Azimuth ( 165 165 165 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)

-----------------------------------------------------------------
                comment ( Definice svetel pro loko ovladanou PC )
-----------------------------------------------------------------

		Light (
			comment ( PC predni leve 1 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( -0.63 1.73 7.52 )
					Azimuth ( -15 -15 -15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light (
			comment ( PC predni leve 2 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( -0.63 1.705 7.518 )
					Azimuth ( -15 -15 -15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)	
		Light (
			comment ( PC predni prave 1 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( CCEED15D )
					Position ( 0.63 1.73 7.52 )
					Azimuth ( 15 15 15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.29 )
				)
			)
		)
                Light (
			comment ( PC predni prave 2 )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFAEAAF )
					Position ( 0.63 1.705 7.518 )
					Azimuth ( 15 15 15 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light (
			comment ( PC koncove leve A )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( -0.74 1.73 -7.485 )
					Azimuth ( -160 -160 -160 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.27 )
				)
			)
		)
                Light (
			comment ( PC koncove leve B )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80FFE5C9 )
					Position ( -0.74 1.705 -7.483 )
					Azimuth ( -160 -160 -160 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
		)
		Light (
			comment ( PC koncove prave A )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( 0.74 1.73 -7.485 )
					Azimuth ( 160 160 160 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.27 )
				)
			)
		)
                Light (
			comment ( PC koncove prave B )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80FFE5C9 )
					Position ( 0.74 1.705 -7.483 )
					Azimuth ( 160 160 160 )
                                        Elevation ( 0 10 0 )
					Transition ( 0 )
					Radius ( 0.12 )
				)
			)
    )
 )

comment	( EngSound )

	Sound ( "..\\..\\common.snd\\sndelok\\230engcd.sms" )
)

Engine ( cdc_230028 

comment	( Description )

	Wagon ( cdc_230028 )

	
comment	( Basic physical engine data )

	Type ( Electric )
	MaxPower ( 3200kW )
	MaxForce ( 4070kN )	
	MaxContinuousForce ( 3490kN )
	MaxCurrent ( 23900A ) 
	MaxVelocity ( 110km/h )
	DieselEngineSpeedOfMaxTractiveEffort( 0mph )                                                                            
	WheelRadius ( 0.625m )
  ORTSDriveWheelWeight ( 84t )
  
    comment ( 0     1     1     2     2     3     3     4     4     5     5     6     6     7     7     8     8     9     9    10    10    11    11    12    12    13    13    14    14    15    15    16    16    17    17    18    18    19    19    20    20    21    21    22    22    23    23    24    24    25    25    26    26    27    27    28    28    29    29    30    30    31    31    32    32    SI   SII  SIII  SIV ) 
ORTSContinuousForceTimeFactor ( 3600 )
ORTSTractionCharacteristics ( 24 70
Throttle ( 0.0   0.01  0.011 0.02 0.021 0.025 0.026  0.03 0.031  0.04 0.041  0.05 0.051  0.08 0.081  0.1  0.101  0.12 0.121  0.14 0.141  0.16 0.161  0.19 0.191  0.21 0.211  0.24 0.241  0.26 0.261  0.29 0.291  0.32 0.321  0.35 0.351  0.37 0.371  0.40 0.401  0.43 0.431  0.46 0.461  0.48 0.481  0.51 0.511  0.54 0.541  0.58 0.581  0.61 0.611  0.64 0.641  0.67 0.671  0.70 0.701  0.73 0.731  0.75 0.751  0.81  0.86  0.92  1 ) 
 table ( 
  0.0km/h 0.0kN  34kN  34kN  65kN  65kN 100kN 100kN 136kN 136kN 185kN 185kN 227kN 227kN 290kN 290kN 360kN 360kN 450kN 450kN 570kN 570kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN
  5.0km/h 0.0kN  15kN  15kN  31kN  31kN  45kN  45kN  57kN  57kN  77kN  77kN  97kN  97kN 123kN 123kN 165kN 165kN 200kN 200kN 290kN 290kN 400kN 400kN 550kN 550kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 10.0km/h 0.0kN   5kN   5kN  17kN  17kN  25kN  25kN  33kN  33kN  45kN  45kN  56kN  56kN  74kN  74kN  90kN  90kN 113kN 113kN 145kN 145kN 180kN 180kN 220kN 220kN 350kN 350kN 500kN 500kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 15.0km/h 0.0kN   4kN   4kN   7kN   7kN  14kN  14kN  20kN  20kN  27kN  27kN  34kN  34kN  46kN  46kN  57kN  57kN  71kN  71kN  84kN  84kN 102kN 102kN 120kN 120kN 155kN 155kN 190kN 190kN 240kN 240kN 290kN 290kN 400kN 400kN 550kN 550kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 20.0km/h 0.0kN   3kN   3kN   2kN   2kN   5kN   5kN  10kN  10kN  16kN  16kN  22kN  22kN  30kN  30kN  38kN  38kN  47kN  47kN  57kN  57kN  69kN  69kN  79kN  79kN  97kN  97kN 115kN 115kN 144kN 144kN 170kN 170kN 215kN 215kN 260kN 260kN 350kN 350kN 500kN 500kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 25.0km/h 0.0kN   2kN   2kN   1kN   1kN   4kN   4kN   5kN   5kN  11kN  11kN  17kN  17kN  22kN  22kN  27kN  27kN  34kN  34kN  40kN  40kN  48kN  48kN  56kN  56kN  67kN  67kN  78kN  78kN  92kN  92kN 107kN 107kN 121kN 121kN 160kN 160kN 200kN 200kN 240kN 240kN 300kN 300kN 400kN 400kN 550kN 550kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 30.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   8kN   8kN  13kN  13kN  19kN  19kN  24kN  24kN  29kN  29kN  36kN  36kN  42kN  42kN  49kN  49kN  57kN  57kN  69kN  69kN  80kN  80kN  95kN  95kN 110kN 110kN 131kN 131kN 152kN 152kN 189kN 189kN 223kN 223kN 310kN 310kN 400kN 400kN 550kN 550kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 35.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   9kN   9kN  14kN  14kN  18kN  18kN  22kN  22kN  27kN  27kN  32kN  32kN  39kN  39kN  45kN  45kN  52kN  52kN  60kN  60kN  71kN  71kN  82kN  82kN  95kN  95kN 109kN 109kN 130kN 130kN 150kN 150kN 185kN 185kN 220kN 220kN 300kN 300kN 380kN 380kN 500kN 500kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 40.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN  13kN  13kN  17kN  17kN  21kN  21kN  24kN  24kN  29kN  29kN  34kN  34kN  41kN  41kN  48kN  48kN  56kN  56kN  64kN  64kN  73kN  73kN  82kN  82kN  95kN  95kN 108kN 108kN 126kN 126kN 145kN 145kN 173kN 173kN 200kN 200kN 235kN 235kN 270kN 270kN 340kN 340kN 420kN 420kN 500kN 500kN 600kN 600kN 650kN 680kN 700kN 700kN  
 45.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  13kN  13kN  16kN  16kN  19kN  19kN  23kN  23kN  27kN  27kN  33kN  33kN  38kN  38kN  45kN  45kN  51kN  51kN  58kN  58kN  66kN  66kN  75kN  75kN  83kN  83kN  94kN  94kN 108kN 108kN 125kN 125kN 142kN 142kN 171kN 171kN 200kN 200kN 225kN 225kN 250kN 250kN 310kN 320kN 350kN 350kN 410kN 460kN 520kN 560kN  
 50.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   8kN   9kN  10kN  10kN  12kN  12kN  15kN  15kN  18kN  18kN  22kN  22kN  27kN  27kN  32kN  32kN  37kN  37kN  42kN  42kN  49kN  49kN  55kN  55kN  62kN  62kN  68kN  68kN  77kN  77kN  87kN  87kN  99kN  99kN 110kN 110kN 130kN 130kN 150kN 150kN 170kN 170kN 190kN 190kN 220kN 220kN 250kN 250kN 300kN 350kN 410kN 460kN  
 55.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  14kN  17kN  17kN  22kN  22kN  27kN  27kN  32kN  32kN  36kN  36kN  42kN  42kN  47kN  47kN  53kN  53kN  58kN  58kN  65kN  65kN  72kN  72kN  80kN  80kN  88kN  88kN 102kN 102kN 117kN 117kN 131kN 131kN 145kN 145kN 166kN 166kN 188kN 188kN 210kN 240kN 300kN 350kN  
 60.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  17kN  17kN  22kN  22kN  25kN  25kN  29kN  29kN  34kN  34kN  38kN  38kN  43kN  43kN  48kN  48kN  54kN  54kN  59kN  59kN  66kN  66kN  73kN  73kN  84kN  84kN  95kN  95kN 106kN 106kN 117kN 117kN 130kN 130kN 142kN 142kN 170kN 190kN 220kN 270kN  
 65.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  19kN  19kN  24kN  24kN  28kN  28kN  33kN  33kN  38kN  38kN  42kN  42kN  47kN  47kN  52kN  52kN  57kN  57kN  62kN  62kN  69kN  69kN  77kN  77kN  85kN  85kN  94kN  94kN 103kN 103kN 112kN 112kN 135kN 160kN 185kN 210kN  
 70.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  18kN  18kN  22kN  22kN  24kN  24kN  27kN  27kN  31kN  31kN  36kN  36kN  40kN  40kN  44kN  44kN  49kN  49kN  54kN  54kN  60kN  60kN  66kN  66kN  73kN  73kN  79kN  79kN  88kN  88kN  96kN  96kN 111kN 130kN 153kN 173kN  
 75.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  18kN  18kN  18kN  19kN  20kN  20kN  23kN  23kN  27kN  27kN  31kN  31kN  35kN  35kN  38kN  38kN  42kN  42kN  47kN  47kN  52kN  52kN  57kN  57kN  62kN  62kN  67kN  67kN  74kN  74kN  80kN  80kN  94kN 110kN 127kN 145kN  
 80.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  18kN  18kN  18kN  19kN  20kN  20kN  21kN  21kN  23kN  23kN  27kN  27kN  30kN  30kN  33kN  33kN  37kN  37kN  41kN  41kN  45kN  45kN  49kN  49kN  53kN  53kN  58kN  58kN  64kN  64kN  70kN  70kN  82kN  95kN 111kN 126kN  
 85.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  18kN  18kN  18kN  19kN  20kN  20kN  21kN  21kN  23kN  23kN  24kN  24kN  26kN  26kN  29kN  29kN  33kN  33kN  36kN  36kN  40kN  40kN  43kN  43kN  47kN  47kN  51kN  51kN  56kN  56kN  62kN  62kN  72kN  85kN  98kN 113kN   
 90.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  18kN  18kN  18kN  19kN  20kN  20kN  21kN  21kN  23kN  23kN  24kN  24kN  26kN  26kN  27kN  27kN  29kN  29kN  31kN  31kN  35kN  35kN  38kN  38kN  41kN  41kN  45kN  45kN  50kN  50kN  56kN  56kN  64kN  75kN  87kN 102kN  
 95.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  18kN  18kN  18kN  19kN  20kN  20kN  21kN  21kN  23kN  23kN  24kN  24kN  26kN  26kN  27kN  27kN  29kN  29kN  30kN  30kN  31kN  31kN  34kN  34kN  37kN  37kN  40kN  40kN  44kN  44kN  50kN  50kN  57kN  67kN  78kN  92kN  
100.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  18kN  18kN  18kN  19kN  20kN  20kN  21kN  21kN  23kN  23kN  24kN  24kN  26kN  26kN  27kN  27kN  29kN  29kN  30kN  30kN  31kN  31kN  32kN  32kN  33kN  33kN  35kN  35kN  39kN  39kN  45kN  45kN  51kN  62kN  72kN  85kN  
105.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  18kN  18kN  18kN  19kN  20kN  20kN  21kN  21kN  23kN  23kN  24kN  24kN  26kN  26kN  27kN  27kN  29kN  29kN  30kN  30kN  31kN  31kN  32kN  32kN  33kN  33kN  34kN  34kN  35kN  35kN  40kN  40kN  46kN  57kN  66kN  79kN
110.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  18kN  18kN  18kN  19kN  20kN  20kN  21kN  21kN  23kN  23kN  24kN  24kN  26kN  26kN  27kN  27kN  29kN  29kN  30kN  30kN  31kN  31kN  32kN  32kN  33kN  33kN  34kN  34kN  35kN  35kN  38kN  38kN  43kN  52kN  60kN  74kN
115.0km/h 0.0kN   1kN   1kN   1kN   1kN   4kN   4kN   5kN   5kN   6kN   6kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  18kN  18kN  18kN  19kN  20kN  20kN  21kN  21kN  23kN  23kN  23kN  23kN  25kN  25kN  26kN  26kN  28kN  28kN  29kN  29kN  30kN  30kN  31kN  31kN  32kN  32kN  33kN  33kN  34kN  34kN  36kN  36kN  41kN  50kN  57kN  70kN
 ) ) 


Comment ( "Brzdovy system DAKO, brzdice DAKO BS2, DAKO BP, kompresor 3DSK-100" )
Comment ( "Brzdeni I.zpusob, rezim brzdeni P" )
BrakesEngineBrakeType ( "Air_single_pipe" )
BrakesTrainBrakeType ( "Air_single_pipe" )
BrakesEngineControllers ( "Independent, Train" )
DoesBrakeCutPower ( 1 )

ORTSMainResChargingRate ( 0.06bar/s )
ORTSBrakePipeChargingRate ( 20.7bar/s ) 
AirBrakesMainMinResAirPressure ( 7.2bar )
AirBrakesMainMaxAirPressure ( 10bar )
AirBrakesMainResVolume ( 1000l )
AirBrakesAirCompressorWattage ( 35000W )
AirBrakesCompressorRestartPressure ( 8.5bar )
AirBrakesIsCompressorElectricOrMechanical ( 0 )
ORTSTrainPipeLeakRate ( 0.0042bar/s )

ORTSEngineBrakeReleaseRate ( 1.0bar/s )
ORTSEngineBrakeApplicationRate ( 1.3bar/s )
EngineBrakesControllerMinPressureReduction ( 0.3bar )
EngineBrakesControllerFullServicePressureDrop ( 1.0bar )
EngineBrakesControllerMaxApplicationRate ( 1.33bar/s )
EngineBrakesControllerMaxReleaseRate ( 1.0bar/s )
EngineBrakesControllerMaxSystemPressure ( 5bar )

TrainBrakesControllerMinPressureReduction ( 0.3bar )
TrainBrakesControllerFullServicePressureDrop ( 1.5bar )
TrainBrakesControllerMaxReleaseRate ( 0.5bar/s )
TrainBrakesControllerMaxApplicationRate ( 0.5bar/s )
TrainBrakesControllerMaxQuickReleaseRate ( 2.0bar/s )
TrainBrakesControllerEmergencyApplicationRate ( 1.86bar/s )
TrainBrakesControllerMaxSystemPressure ( 5bar )

ORTSBrakePipeTimeFactor ( 0.003 )
ORTSBrakeServiceTimeFactor ( 1.009 )
ORTSBrakeEmergencyTimeFactor ( 0.1 ) 


comment ( Monitors )


 VigilanceMonitor (
  MonitoringDeviceMonitorTimeLimit ( 27 )
  MonitoringDeviceAlarmTimeLimit ( 17 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 0 )
  MonitoringDeviceResetLevel ( 0 )
  
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceResetOnZeroSpeed ( 1 )
  MonitoringDeviceResetOnResetButton ( 1 )
  MonitoringDeviceResetOnDirectionNeutral ( 1 )
 )
 OverspeedMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0 )
  MonitoringDeviceAlarmTimeLimit ( 5 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 72.6 )
  MonitoringDeviceResetLevel ( 0 )
  Comment ( MonitoringDeviceTriggerOnHighCurrent ( 1250 ) )
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 0 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceAlarmTimeBeforeOverSpeed ( 0 )
  MonitoringDeviceDoesSuppressionReset ( 0 )
  MonitoringDeviceTriggerOnOverspeed ( 68.5 )
  MonitoringDeviceTriggerOnTrackOverspeed ( 0 )
  MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnResetButton ( 0 )
 )
		
	 
Comment	( Controllers )

        EngineControllers (
		Throttle ( 0 1 0.001 0
			NumNotches ( 69
			    Notch ( 0.0   0 Dummy )
			    
			    Notch ( 0.01  0 Dummy )
			    Notch ( 0.011 0 Dummy )
			    
			    Notch ( 0.02  0 Dummy )
			    Notch ( 0.021 0 Dummy )
			    
			    Notch ( 0.025 0 Dummy )
			    Notch ( 0.026 0 Dummy )
			    
			    Notch ( 0.03  0 Dummy )
			    Notch ( 0.031 0 Dummy )
			    
			    Notch ( 0.04  0 Dummy )
			    Notch ( 0.041 0 Dummy )
			    
			    Notch ( 0.05  0 Dummy )
			    Notch ( 0.051 0 Dummy )
			    
			    Notch ( 0.08  0 Dummy )
			    Notch ( 0.081 0 Dummy )
			    
			    Notch ( 0.1   0 Dummy )
			    Notch ( 0.101 0 Dummy )
			    
			    Notch ( 0.12  0 Dummy )
			    Notch ( 0.121 0 Dummy )
			    
			    Notch ( 0.14  0 Dummy )
			    Notch ( 0.141 0 Dummy )
			    
			    Notch ( 0.16  0 Dummy )
			    Notch ( 0.161 0 Dummy )
			    
			    Notch ( 0.19  0 Dummy )
			    Notch ( 0.191 0 Dummy )
			    
			    Notch ( 0.21  0 Dummy )
			    Notch ( 0.211 0 Dummy )
			    
			    Notch ( 0.24  0 Dummy )
			    Notch ( 0.241 0 Dummy )
			    
			    Notch ( 0.26  0 Dummy )
			    Notch ( 0.261 0 Dummy )
			    
			    Notch ( 0.29  0 Dummy )
			    Notch ( 0.291 0 Dummy )
			    
			    Notch ( 0.32  0 Dummy )
			    Notch ( 0.321 0 Dummy )
			    
			    Notch ( 0.35  0 Dummy )
			    Notch ( 0.351 0 Dummy )
			    
			    Notch ( 0.37  0 Dummy )
			    Notch ( 0.371 0 Dummy )
			    
			    Notch ( 0.40  0 Dummy )
			    Notch ( 0.401 0 Dummy )
			    
			    Notch ( 0.43  0 Dummy )
			    Notch ( 0.431 0 Dummy )
			    
			    Notch ( 0.46  0 Dummy )
			    Notch ( 0.461 0 Dummy )
			    
			    Notch ( 0.48  0 Dummy )
			    Notch ( 0.481 0 Dummy )
			    
			    Notch ( 0.51  0 Dummy )
			    Notch ( 0.511 0 Dummy )
			    
			    Notch ( 0.54  0 Dummy )
			    Notch ( 0.541 0 Dummy )
			    
			    Notch ( 0.58  0 Dummy )
			    Notch ( 0.581 0 Dummy )
			    
			    Notch ( 0.61  0 Dummy )
			    Notch ( 0.611 0 Dummy )
			    
			    Notch ( 0.64  0 Dummy )
			    Notch ( 0.641 0 Dummy )
			    
			    Notch ( 0.67  0 Dummy )
			    Notch ( 0.671 0 Dummy )
			    
			    Notch ( 0.70  0 Dummy )
			    Notch ( 0.701 0 Dummy )
 
			    Notch ( 0.73  0 Dummy )
			    Notch ( 0.731 0 Dummy )
			    
			    Notch ( 0.75  0 Dummy )
			    Notch ( 0.751 0 Dummy )
			    
			    Notch ( 0.81  0 Dummy )
			    Notch ( 0.86  0 Dummy )
			    Notch ( 0.92  0 Dummy )
			    Notch ( 1     0 Dummy )
		)
	)           

		
	comment (***Primocinna brzda typ DAKO-BP***)
		Brake_Engine ( 0 1 0.3 1
			NumNotches ( 1
				Notch ( 0 1 Dummy )                   
                )
            )
        comment (***Prubezna brzda typ DAKO-BS2***)
		Brake_Train ( 0 1 0.04 0.87
			NumNotches ( 7
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
				Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)

            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
		
	
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            BailOffButton( 0 1 0 )
        )
	
  	
comment	( CabSound and Views )

	Sound ( "..\\..\\common.snd\\sndelok\\230cabcd.sms" )
	
	CabView ( "../../common.cab/cab230_OR/230.cvf" )
	HeadOut (1.7 3.2 5.7 )
	

Comment	( Operations )


	 Name ( "CDC 230 028-3" )
	 Description (
	  "Rada 230 CD je univerzální elektrická skrínová lokomotiva, pouzívaná prevazne v nákladní doprave.\n\n"+
	  "Typ Bo'-Bo', napeti 25 kV 50Hz.\n\n"+
	  "Délka pres nárazniky: 16,44 m\n\n"+
	  "Prumer hnacích kol: 1250 mm\n\n"+
	  "Hmotnost ve sluzbe: 85 t\n\n"+
	  "Trvaly vykon trakcních motoru: 3080 kW\n\n"+
	  "Max. rychlost 110 km/h\n\n"+
	  "Ovladani a proudy v MSTS:\n\n"+
	  "Maximalni proud (nadproudova ochrana): 1250A\n\n"+
	  "Trvaly proud: 1100A\n\n"+
	  "Hodinovy proud: 1140A\n\n"+
	  "15 minutovy proud: 1300A\n\n"+
	  "5 minutovy proud: 1500A\n\n"+
	  "Proud na mezi adheze (skluz): 1262A\n\n"+
	  "Proud na mezi adheze s piskovanim (skluz): 1598A\n\n"+
	  "Kontroler: 32 stupnu (1%-75%) + 4 shuntovaci (81%-100%)\n\n"
	 )

	 EngineOperatingProcedures (
	  "Jak se rozjet\n"+
	  "1. Uz máte zvednutý pantograf. (Pokud z nejakého duvodu zvednutý není, stisknete klávesu P pro jeho zvednutí.)\n"+
	  "2. Stisknete W na prestavení reverzního kontoleru do polohy 'vpred'.\n"+
	  "3. Stisknete a drzte ; pro odbrzdení vlakové brzdy.\n"+
	  "(4. Stisknete a drzte [ pro odbrzdení lokomotivní brzdy.)\n"+
	  "5. Stisknete D pro zvýsení pozadovaného výkonu.\n"+
	  "6. Pomalu zvysujte výkon stiskem D, dokud vlak nedosáhne pozadované rychlosti.\n\n"+
	  "Jak zpomalit\n"+
	  "1. Stisknete A pro snízení pozadovaného výkonu (postupne az na 0).\n"+
	  "2. Jestlize je to nutné tak pouzijte brzdy pro postupné rychlejsí snizování rychlosti.\n\n"+
	  "Jak pouzít vlakovou brzdu\n"+
	  "1. Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosáhnete pozadovaného brzdného tlaku.\n"+
	  "2. Po dosazení pozadovaného brzd. tlaku stiskem ; presunte rukojet brzdy do polhy ZÁVER.\n\n"+
	  "Jak odbrzdit vlakovou brzdu\n"+
	  "1. Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENÍ.\n"+
	  "2. Pockejte, az klesne tlak v brzdových valcích na 0.\n"+
	  "3. Stisknete ' pro presunutí rukojeti brzdy do polohy ZÁVER.\n"+
	  "Jak pouzít lokomotvní brzdu\n"+
	  "1. Stisknete a drzte ] pro zabrzdení lokomotivní brzdy (0-100%).\n\n"+
	  "Jak odbrzdit lokomotivní brzdu\n"+
	  "1. Stisknete a drzte [ pro odbrzdení lokomotivní brzdy (0-100%).\n\n"+
	  "Jak pouzít zachrannou brzdu\n"+
	  "1. Stisknete a drzte A pro snízení výkonu az na 0.\n"+
	  "2. Stisknete BACKSPACE pro aktivaci záchrané brzdy.\n\n"+
	  "Jak zrusit záchrannou brzdu\n"+
	  "1. Pockejte na úplné zastavení vlaku.\n"+
	  "2. Stisknete Z pro odblokování ovládání lokomotivy.\n"+
	  "3. Stisknete ; a [ pro odbrzdení brzdných systému.\n"+
	  "4. Pomalu zvysujte výkon stiskem D .\n\n"+
	  "Jak zmenit smer\n"+
	  "1. Zastavte vlak.\n"+
	  "2. Presunte paku reverzniho kontroleru do polohy vzad nebo vpred dvojitým stiskem S.\n"+
	  "3. Odbrzdete brzdy stiskem ; (prípadne [ ).\n"+
	  "4. Pomalu zvysujte vykon stiskem D .\n\n"+
	  "Jak pripojit vagony/lokomotivy\n"+
	  "1. K vagonu musíte prijet pomalu, optimální rychlost je okolo 1 km/h.\n"+
	  "Tip: Pro zobrazení pohledu na spráhlo stisknete klávesu 6.\n"+
	  "2. Stisknete F9 pro otevrení okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
	  "3. Jestlize je ikona vozu cervená, je zatazena rucní brzda. Dvojtukem mysí na voze uvolníte/zatáhne rucní brzdu.\n"+
	  "4. Zavrete okno sestavení vlaku stiskem F9.\n"+
	  "5. Pockejte az odbrzdíte pripojené vozy.\n\n"+
	  "Odpojení vozu nebo lokomotivy\n"+
	  "POZOR! Melo by se provádet jen tehdy, pokud VLAK STOJÍ!\n"+
	  "1. Otevrete okno sestavy vlaku F9.\n"+
	  "2. Poklepejte 2x na ikonu vozu, ktery se má odpojit, pokud chcete, aby mel vuz zatazenou rucní brzdu.\n"+
	  "3. Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
	  "4. Pomalu se rozjedte smerem od odpojene casti vlaku.\n"+
	  "(Pozn.: V nekterých prípadech pri rychlejsím odjezdu dojde k opetovnému spojení spráhel. Pokud se toto stane tak soupravu opet rozpojte a velmi pomalu odjízdejte az do vzdálenosti jednoho prazce. Pak jiz muzete zacít zrychlovat.)\n"+
	  "5. Zavrete okno sestavení vlaku stiskem F9.\n\n"
	 ) 
)