SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( CSD_E4790002
Comment ( "Sekce vozidlo" )
Comment ( "Popis fyziky vozu pro OR" )
Comment ( "Josef Vogeltanz - 17.04.2020" )
Comment ( "Upraveno 04.06.2022" )

Comment ( "Obecne informace vozu" )
Type ( Engine )
WagonShape ( CSD_E4790002.s )
Size ( 3.186m 4.68m 17.4m )
Mass ( 84.8t )
WheelRadius ( 0.625m )
ORTSNumberAxles ( 0 )

Comment ( "Sprahla" )
Coupling (
Type ( Chain )
Spring ( Stiffness ( 6.7e6N/m 4.4e8N/m ) Break ( 850kN 850kN ) r0 ( 0cm 2.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Coupling (
Type ( Chain )
Spring ( Stiffness ( 6.7e6N/m 4.4e8N/m ) Break ( 850kN 850kN ) r0 ( 0cm 2.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Comment ( "Brzdy" )
Comment ( "Brzdovy system DAKO, zdrze, Bv.P: 50t" )
Comment ( "Rezim brzdeni P" )
BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

MaxBrakeForce ( 121kN )
MaxHandbrakeForce ( 52kN )
NumberOfHandbrakeLeverSteps ( 10 )

TripleValveRatio ( 3.0 )
MaxReleaseRate ( 0.212bar/s )
MaxApplicationRate ( 0.475bar/s )
MaxAuxilaryChargingRate ( 0.506bar/s )
EmergencyResChargingRate ( 0.506bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 4bar )
EmergencyResVolumeMultiplier ( 2.5 )
EmergencyResCapacity ( 240l )
BrakePipeVolume ( 15.2l )
ORTSBrakeInsensitivity ( 0.005bar/s )

ORTSBrakeShoeFriction (
0   0.310
8   0.238
16  0.193
24  0.168
32  0.152
40  0.140
48  0.131
56  0.123
64  0.116
72  0.109
80  0.105
88  0.101
96  0.098
104 0.096
112 0.094
120 0.093
128 0.092
136 0.092
144 0.092
152 0.092
160 0.092
)

Comment ( "Pantografy" )
ORTSPantographs (
Pantograph (
Delay ( 3s )
)
Pantograph (
Delay ( 3s )
)
)

Comment ( "Jizdni odpory a treni" )
CentreOfGravity ( 0m 2.33m  0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 3m 200mm )
ORTSUnbalancedSuperelevation ( 150mm )

ORTSAdhesion (
ORTSCurtius_Kniffler ( 8.5 52 0.149 0.7 )
ORTSSlipWarningThreshold ( 60 )
Wheelset (
Axle ( 1
ORTSInertia ( 1879 )
ORTSRadius ( 0.625m )
)
Axle ( 2
ORTSInertia ( 1879 )
ORTSRadius ( 0.625m )
)
Axle ( 3
ORTSInertia ( 1879 )
ORTSRadius ( 0.625m )
)
Axle ( 4
ORTSInertia ( 1879 )
ORTSRadius ( 0.625m )
)
)
)

ORTSBearingType ( Roller )
ORTSDavis_A ( 1056.4 )
ORTSDavis_B ( 27.9 )
ORTSDavis_C ( 6.3825 )
ORTSWagonFrontalArea ( 12.5m^2 )

ORTSLengthBogieCentre ( 8.17m )
ORTSLengthCarBody ( 15.97m )
ORTSLengthCouplerFace ( 17.21m )
ORTSNumAxles ( 4 )
ORTSNumBogies ( 2 )
ORTSWheelFlangeLength ( 0.02m )
ORTSMaximumWheelFlangeAngle ( 70deg )

Comment ( "Nastavení svetel - CSD")
Lights ( 56

Comment ( "Svetelny kuzel dalkovy" )
Light (
Type ( 1 )
Conditions ( Headlight ( 3 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFFFFC4 ) Position ( 0 3.7 7.9 ) Angle ( 15 ) Transition ( 1 ) Radius ( 70 ) )
)
)

Comment ( "Svetelny kuzel tlumeny" )
Light (
Type ( 1 )
Conditions ( Headlight ( 2 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFFFFC4 ) Position ( 0 3.7 7.9 ) Angle ( 35 ) Transition ( 1 ) Radius ( 35 ) )
)
)

Comment ( "Svetelny kuzel navestní" )
Light (
Type ( 1 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFFFC4 ) Position ( 0 0.5 8.4 ) Angle ( 90 ) Transition ( 1 ) Radius ( 3 ) )
)
)

Comment ( "Definice svetel pro predni stanoviste" )
Comment ( "Reflektor dalkovy 1" )
Light (
Type ( 0 )
Conditions ( Headlight ( 3 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFFEA99 ) Position ( 0.1 3.718 7.88 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.3 ) )
)
)

Comment ( "Reflektor dalkovy 2" )
Light (
Type ( 0 )
Conditions ( Headlight ( 3 ) Unit ( 2 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFFEA99 ) Position ( -0.1 3.718 7.88 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.3 ) )
)
)

Comment ( "Predni leve pozicni A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( 0.518 1.857 8.06 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Predni leve pozicni B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( 0.518 1.827 8.0602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Predni horni zapnute 1A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFEA99 ) Position ( 0.1 3.718 7.88 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.3 ) )
)
)

Comment ( "Predni horni zapnute 1B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFFFF9E0 ) Position ( 0.1 3.688 7.8802 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.05 ) )
)
)

Comment ( "Predni horni zapnute 2A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFEA99 ) Position ( -0.1 3.718 7.88 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.3 ) )
)
)

Comment ( "Predni horni zapnute 2B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFFFF9E0 ) Position ( -0.1 3.688 7.8802 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.05 ) )
)
)

Comment ( "Predni leve zapnute A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( 0.518 1.857 8.06 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Predni leve zapnute B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( 0.518 1.827 8.0602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Predni prave zapnute A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( -0.518 1.857 8.06 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Predni prave zapnute B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 2 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( -0.518 1.827 8.0602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Zadni prave pozicni A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( -0.518 1.857 -8.06 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni prave pozicni B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 0 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( -0.518 1.827 -8.0602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Zadni leve koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( 0.796 1.857 -8.05 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni leve koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( 0.796 1.827 -8.0502 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Zadni prave koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( -0.796 1.857 -8.05 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni prave koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( -0.796 1.827 -8.0502 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Zadni leve koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( 0.796 1.857 -8.05 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni leve koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( 0.796 1.827 -8.0502 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Zadni prave koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( -0.796 1.857 -8.05 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni prave koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 3 ) Control ( 2 ) TimeOfDay ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( -0.796 1.827 -8.0502 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Definice svetel pro zadni stanoviste" )
Comment ( "Reflektor dalkovy 1" )
Light (
Type ( 0 )
Conditions ( Headlight ( 3 ) Unit ( 5 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFFEA99 ) Position ( 0.1 3.718 -7.88 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.3 ) )
)
)

Comment ( "Reflektor dalkovy 2" )
Light (
Type ( 0 )
Conditions ( Headlight ( 3 ) Unit ( 5 ) Control ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFFEA99 ) Position ( -0.1 3.718 -7.88 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.3 ) )
)
)

Comment ( "Predni horni zapnute 1A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFEA99 ) Position ( 0.1 3.718 -7.88 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.3 ) )
)
)

Comment ( "Predni horni zapnute 1B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFFFF9E0 ) Position ( 0.1 3.688 -7.8802 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.05 ) )
)
)

Comment ( "Predni horni zapnute 2A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFEA99 ) Position ( -0.1 3.718 -7.88 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.3 ) )
)
)

Comment ( "Predni horni zapnute 2B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 2 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 2 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFFFF9E0 ) Position ( -0.1 3.688 -7.8802 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.05 ) )
)
)

Comment ( "Predni leve zapnute A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( 0.518 1.857 -8.06 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Predni leve zapnute B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( 0.518 1.827 -8.0602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Predni prave zapnute A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( -0.518 1.857 -8.06 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Predni prave zapnute B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 5 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( -0.518 1.827 -8.0602 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "Zadni leve koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( 0.796 1.857 8.05 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni leve koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( 0.796 1.827 8.0502 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Zadni prave koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( -0.796 1.857 8.05 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni prave koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 4 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( -0.796 1.827 8.0502 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Zadni leve koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( 0.796 1.857 8.05 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni leve koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( 0.796 1.827 8.0502 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Zadni prave koncove A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( -0.796 1.857 8.05 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "Zadni prave koncove B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 1 ) Unit ( 4 ) Control ( 2 ) TimeOfDay ( 1 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( -0.796 1.827 8.0502 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Definice svetel pro loko ovladanou PC" )
Comment ( "PC predni leve A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( 0.518 1.857 8.06 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "PC predni leve B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( 0.518 1.827 8.0602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "PC predni prave A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFCC8D27 ) Position ( -0.518 1.857 8.06 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "PC predni prave B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFFAEAAF ) Position ( -0.518 1.827 8.0602 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.15 ) )
)
)

Comment ( "PC predni horni 1A" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFEA99 ) Position ( 0.1 3.718 7.88 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.3 ) )
)
)

Comment ( "PC predni horni 1B" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFFFF9E0 ) Position ( 0.1 3.688 7.8802 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.05 ) )
)
)

Comment ( "PC predni horni 2A" )
Light (
Type ( 0 )
Conditions ( Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFEA99 ) Position ( -0.1 3.718 7.88 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.3 ) )
)
)

Comment ( "PC predni horni 2B" )
Light (
Type ( 0 )
Conditions ( Unit ( 2 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( BFFFF9E0 ) Position ( -0.1 3.688 7.8802 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.05 ) )
)
)

Comment ( "PC zadni leve koncove A" )
Light (
Type ( 0 )
Conditions ( Unit ( 3 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( 0.796 1.857 -8.05 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "PC zadni leve koncove B" )
Light (
Type ( 0 )
Conditions ( Unit ( 3 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( 0.796 1.827 -8.0502 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "PC zadni prave koncove A" )
Light (
Type ( 0 )
Conditions ( Unit ( 3 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( FFD10209 ) Position ( -0.796 1.857 -8.05 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.35 ) )
)
)

Comment ( "PC zadni prave koncove B" )
Light (
Type ( 0 )
Conditions ( Unit ( 3 ) Control ( 1 ) Service ( 2 ) TimeOfDay ( 0 ) )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State ( Duration ( 0 ) LightColour ( 80FFE5C9 ) Position ( -0.796 1.827 -8.0502 ) Azimuth ( 180 180 180 ) Transition ( 0 ) Elevation ( 0 0 0 ) Radius ( 0.12 ) )
)
)

Comment ( "Zablesky na smykadle" )
Light (
Type ( 0 )
Conditions ( Headlight ( 0 ) Unit ( 2 ) Service ( 2 ) )
FadeIn ( 0 )
FadeOut ( 0 )
Cycle ( 0 )
States ( 16
State ( Duration ( 0.03 ) LightColour ( ff0000ff ) Position ( 0 5.41 -4.18 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 3 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.04 ) LightColour ( ff87cefa ) Position ( -0.05 5.41 -4.18 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 7.6 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.1 ) LightColour ( ff87cefa ) Position ( 0.025 5.41 -4.18 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 8.3 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.04 ) LightColour ( ff87cefa ) Position ( 0 5.41 -4.18 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 0.05 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.05 ) LightColour ( ff0000ff ) Position ( -0.01 5.41 -4.18 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 9 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.07 ) LightColour ( ff0000ff ) Position ( -0.05 5.41 -4.18 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 12 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.05 ) LightColour ( ff87cefa ) Position ( 0.01 5.41 -4.18 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 0.1 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
State ( Duration ( 0.03 ) LightColour ( ff0000ff ) Position ( -0.01 5.41 -4.18 ) Azimuth ( 0 -180 180 ) Transition ( 0 ) Radius ( 0.6 ) )
State ( Duration ( 13 ) LightColour ( 00000000 ) Position ( 0 3 0 ) Azimuth ( 0 0 0 ) Transition ( 0 ) Radius ( 0 ) )
)
)
)

Comment ( "Ostatni informace" )
Sound ( 130eng.sms )
)

Engine ( CSD_E4790002
Comment ( "Sekce pohon" )
Comment ( "Obecne informace pohonu" )

Wagon ( CSD_E4790002 )
Name ( "CSD E479.0002" )

Comment ( "Pohon" )
Type ( Electric )
MaxVelocity ( 100km/h )
ORTSSpeedOfMaxContinuousForce ( 49km/h )
WheelRadius ( 0.625m )
Sanding ( 40km/h )
MaxForce ( 228kN )
MaxContinuousForce ( 147kN )
AntiSlip ( 0 )
MaxPower ( 2340kW )
MaxCurrent ( 1100A )
ORTSDriveWheelWeight ( 84.8t )
ORTSNumberDriveAxles ( 4 )

ORTSCircuitBreaker ( Manual )
ORTSCircuitBreakerClosingDelay ( 2s )
ORTSPowerOnDelay ( 5s )

ORTSContinuousForceTimeFactor ( 3600 )
ORTSTractionCharacteristics ( 20 47
throttle ( 0  0.001  0.004 0.02   0.04    0.07    0.09    0.11    0.13    0.15    0.17    0.19    0.21    0.23    0.25    0.27    0.29    0.30    0.32    0.34    0.36    0.37    0.38    0.39    0.40    0.41    0.43    0.47    0.50    0.53    0.57    0.59    0.60    0.62    0.63    0.65    0.66    0.69    0.71    0.72    0.76    0.82    0.86    0.92    0.96    1.00 )
table (
0km/h   0.0kN 0.0kN 39.0kN 81.0kN 126.0kN 160.0kN 190.0kN 207.0kN 228.0kN 244.0kN 270.0kN 270.0kN 270.0kN 270.0kN 270.0kN 239.0kN 237.0kN 234.0kN 232.0kN 230.0kN 229.0kN 227.0kN 226.0kN 224.0kN 223.0kN 222.0kN 221.0kN 234.5kN 248.0kN 227.0kN 222.0kN 217.0kN 214.0kN 210.0kN 208.0kN 205.0kN 203.0kN 201.0kN 200.0kN 198.0kN 197.0kN 195.0kN 193.0kN 190.0kN 188.0kN 185.0kN
5km/h   0.0kN 0.0kN 33.0kN 64.0kN 95.0kN  122.0kN 144.0kN 156.0kN 170.0kN 182.0kN 198.0kN 220.0kN 248.0kN 245.0kN 242.0kN 239.0kN 237.0kN 234.0kN 232.0kN 230.0kN 229.0kN 227.0kN 226.0kN 224.0kN 223.0kN 222.0kN 221.0kN 234.5kN 248.0kN 227.0kN 222.0kN 217.0kN 214.0kN 210.0kN 208.0kN 205.0kN 203.0kN 201.0kN 200.0kN 198.0kN 197.0kN 195.0kN 193.0kN 190.0kN 188.0kN 185.0kN
10km/h  0.0kN 0.0kN 28.0kN 51.0kN 73.0kN  91.0kN  105.0kN 114.0kN 122.0kN 131.0kN 143.0kN 157.0kN 174.0kN 186.0kN 202.0kN 220.0kN 237.0kN 234.0kN 232.0kN 230.0kN 229.0kN 227.0kN 226.0kN 224.0kN 223.0kN 222.0kN 221.0kN 216.0kN 211.0kN 227.0kN 222.0kN 217.0kN 214.0kN 210.0kN 208.0kN 205.0kN 203.0kN 201.0kN 200.0kN 198.0kN 197.0kN 195.0kN 193.0kN 190.0kN 188.0kN 185.0kN
15km/h  0.0kN 0.0kN 28.0kN 42.0kN 56.0kN  66.0kN  77.0kN  82.0kN  88.0kN  94.0kN  102.0kN 110.0kN 120.0kN 126.0kN 138.0kN 148.0kN 160.0kN 172.0kN 192.0kN 210.0kN 229.0kN 227.0kN 226.0kN 224.0kN 223.0kN 222.0kN 221.0kN 199.5kN 178.0kN 227.0kN 222.0kN 217.0kN 214.0kN 210.0kN 208.0kN 205.0kN 203.0kN 201.0kN 200.0kN 198.0kN 197.0kN 195.0kN 193.0kN 190.0kN 188.0kN 185.0kN
20km/h  0.0kN 0.0kN 28.0kN 34.0kN 44.0kN  49.0kN  55.0kN  59.0kN  62.0kN  66.0kN  72.0kN  76.0kN  81.0kN  86.0kN  72.0kN  97.0kN  103.0kN 111.0kN 120.0kN 128.0kN 140.0kN 153.0kN 166.0kN 182.0kN 202.0kN 222.0kN 221.0kN 183.0kN 145.0kN 198.0kN 222.0kN 217.0kN 214.0kN 210.0kN 208.0kN 205.0kN 203.0kN 201.0kN 200.0kN 198.0kN 197.0kN 195.0kN 193.0kN 190.0kN 188.0kN 185.0kN
25km/h  0.0kN 0.0kN 28.0kN 29.0kN 35.0kN  37.0kN  41.0kN  43.0kN  45.0kN  47.0kN  51.0kN  52.0kN  58.0kN  60.0kN  62.0kN  65.0kN  68.0kN  72.0kN  78.0kN  81.0kN  86.0kN  93.0kN  102.0kN 108.0kN 116.0kN 124.0kN 132.0kN 127.0kN 122.0kN 163.0kN 184.0kN 211.0kN 214.0kN 210.0kN 208.0kN 205.0kN 203.0kN 201.0kN 200.0kN 198.0kN 197.0kN 195.0kN 193.0kN 190.0kN 188.0kN 185.0kN
30km/h  0.0kN 0.0kN 27.0kN 28.0kN 27.0kN  29.0kN  30.5kN  32.0kN  34.0kN  35.0kN  37.0kN  40.0kN  42.0kN  43.0kN  45.0kN  46.0kN  48.0kN  50.0kN  53.0kN  55.0kN  57.0kN  61.0kN  64.0kN  67.0kN  70.5kN  74.0kN  76.0kN  90.5kN  105.0kN 133.0kN 150.0kN 169.0kN 190.0kN 210.0kN 208.0kN 205.0kN 203.0kN 201.0kN 200.0kN 198.0kN 197.0kN 195.0kN 193.0kN 190.0kN 188.0kN 185.0kN
35km/h  0.0kN 0.0kN 26.0kN 27.0kN 27.0kN  27.0kN  30.5kN  32.0kN  27.0kN  27.0kN  29.0kN  30.0kN  32.0kN  32.0kN  33.0kN  34.0kN  35.0kN  37.0kN  39.0kN  40.0kN  41.0kN  43.0kN  45.0kN  46.0kN  48.0kN  50.0kN  52.0kN  70.0kN  88.0kN  109.0kN 122.0kN 135.0kN 149.0kN 170.0kN 190.0kN 205.0kN 203.0kN 201.0kN 200.0kN 198.0kN 197.0kN 195.0kN 193.0kN 190.0kN 188.0kN 185.0kN
40km/h  0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  27.0kN  29.0kN  30.0kN  32.0kN  32.0kN  33.0kN  34.0kN  26.0kN  27.0kN  29.0kN  30.0kN  30.0kN  31.0kN  32.0kN  34.0kN  35.0kN  36.0kN  36.0kN  54.5kN  73.0kN  89.0kN  99.0kN  109.0kN 117.0kN 132.0kN 146.0kN 160.0kN 182.0kN 201.0kN 200.0kN 198.0kN 197.0kN 195.0kN 193.0kN 190.0kN 188.0kN 185.0kN
45km/h  0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  30.0kN  30.0kN  30.0kN  30.0kN  26.0kN  26.0kN  26.0kN  29.0kN  29.0kN  29.0kN  29.0kN  29.0kN  29.0kN  29.0kN  29.0kN  45.0kN  61.0kN  73.0kN  81.0kN  84.0kN  94.0kN  105.0kN 112.0kN 122.0kN 135.0kN 147.0kN 166.0kN 186.0kN 197.0kN 195.0kN 193.0kN 190.0kN 188.0kN 185.0kN
50km/h  0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  39.0kN  52.0kN  62.0kN  67.0kN  72.0kN  77.0kN  83.0kN  88.0kN  95.0kN  104.0kN 111.0kN 122.0kN 132.0kN 144.0kN 172.0kN 193.0kN 190.0kN 188.0kN 185.0kN
55km/h  0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  32.0kN  38.0kN  44.0kN  47.0kN  51.0kN  54.0kN  55.0kN  59.0kN  62.0kN  66.0kN  69.0kN  73.0kN  77.0kN  81.0kN  100.0kN 127.0kN 153.0kN 188.0kN 185.0kN
65km/h  0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  29.5kN  33.0kN  38.0kN  40.0kN  43.0kN  45.0kN  46.0kN  49.0kN  31.0kN  54.0kN  57.0kN  60.0kN  62.0kN  65.0kN  80.0kN  104.0kN 124.0kN 188.0kN 185.0kN
70km/h  0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  27.5kN  29.0kN  32.0kN  34.0kN  36.0kN  38.0kN  39.0kN  41.0kN  43.0kN  45.0kN  46.0kN  48.0kN  50.0kN  53.0kN  66.0kN  86.0kN  104.0kN 126.0kN 153.0kN
75km/h  0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  25.5kN  25.0kN  28.0kN  30.0kN  31.0kN  32.0kN  33.0kN  35.0kN  36.0kN  37.0kN  39.0kN  40.0kN  42.0kN  43.0kN  55.0kN  73.0kN  88.0kN  107.0kN 129.0kN
80km/h  0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  25.5kN  25.0kN  24.0kN  26.0kN  27.0kN  28.0kN  29.0kN  29.0kN  31.0kN  31.0kN  32.0kN  34.0kN  35.0kN  36.0kN  46.0kN  62.0kN  75.0kN  91.0kN  109.0kN
85km/h  0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  25.5kN  25.0kN  24.0kN  26.0kN  27.0kN  28.0kN  29.0kN  25.0kN  27.0kN  27.0kN  28.0kN  29.0kN  29.0kN  30.0kN  41.0kN  53.0kN  65.0kN  78.0kN  93.0kN
90km/h  0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  25.5kN  25.0kN  24.0kN  26.0kN  27.0kN  28.0kN  29.0kN  25.0kN  27.0kN  27.0kN  28.0kN  29.0kN  25.0kN  26.0kN  34.0kN  45.0kN  56.0kN  66.0kN  79.0kN
95km/h  0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  25.5kN  25.0kN  24.0kN  26.0kN  27.0kN  28.0kN  29.0kN  25.0kN  27.0kN  27.0kN  28.0kN  29.0kN  25.0kN  23.0kN  30.0kN  40.0kN  48.0kN  57.0kN  68.0kN
100km/h 0.0kN 0.0kN 26.0kN 26.0kN 26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  26.0kN  25.5kN  25.0kN  24.0kN  26.0kN  27.0kN  28.0kN  29.0kN  25.0kN  27.0kN  27.0kN  28.0kN  29.0kN  25.0kN  21.0kN  26.0kN  34.0kN  41.0kN  49.0kN  57.0kN
)
)

Comment ( "Brzdy" )
Comment ( "Brzdovy system DAKO-GP, brzdic DAKO-BS2 a DAKO-BP, kompresor 2x 3DSK100 " )
Comment ( "Brzdeni I.zpusob, Rezim brzdeni P, Bv.P:50t")

ORTSMainResChargingRate ( 0.06bar/s )
ORTSBrakePipeChargingRate ( 20.7bar/s )
AirBrakesMainMaxAirPressure ( 10bar )
AirBrakesMainResVolume ( 1.1m^3 )
AirBrakesCompressorRestartPressure ( 8.5bar )
TrainPipeLeakRate ( 0.0016bar/s )

ORTSEngineBrakeReleaseRate ( 1.0bar/s )
ORTSEngineBrakeApplicationRate ( 1.33bar/s )
EngineBrakesControllerMinPressureReduction ( 0.3bar )
EngineBrakesControllerFullServicePressureDrop ( 1.0bar )
EngineBrakesControllerMaxApplicationRate ( 1.33bar/s )
EngineBrakesControllerMaxReleaseRate ( 1.0bar/s )
EngineBrakesControllerMaxSystemPressure ( 5bar )

ORTSTrainBrakesControllerMaxOverchargePressure ( 5.4bar )
ORTSTrainBrakesControllerOverchargeEliminationRate ( 0.0023bar/s ) 
TrainBrakesControllerMinPressureReduction ( 0.3bar )
TrainBrakesControllerFullServicePressureDrop ( 1.5bar )
TrainBrakesControllerMaxApplicationRate ( 0.67bar/s )
TrainBrakesControllerMaxReleaseRate ( 0.67bar/s )
TrainBrakesControllerMaxQuickReleaseRate ( 2.0bar/s )
TrainBrakesControllerEmergencyApplicationRate ( 1.86bar/s )
TrainBrakesControllerMaxSystemPressure ( 5bar )

ORTSBrakePipeTimeFactor ( 0.003 )
ORTSBrakeServiceTimeFactor ( 1.009 )
ORTSBrakeEmergencyTimeFactor ( 0.1 )

BrakesTrainBrakeType ( "Air_single_pipe" )
BrakesEngineControllers ( "Independent, Train" )

Comment ( "Ovladani jizdy" )
ORTSBattery (
Mode ( Switch )
Delay ( 2s )
)

ORTSMasterKey (
Mode ( Manual )
DelayOff ( 2s )
)

ORTSElectricTrainSupply (
Mode ( Switch )
)

Comment ( "Vlakovy zabezpecovac - pouze KBS" )
VigilanceMonitor (
MonitoringDeviceMonitorTimeLimit ( 16 )
MonitoringDeviceAlarmTimeLimit ( 6 )
MonitoringDevicePenaltyTimeLimit ( 0 )
MonitoringDeviceCriticalLevel ( 0 )
MonitoringDeviceResetLevel ( 1.3 )
MonitoringDeviceAppliesFullBrake ( 0 )
MonitoringDeviceAppliesEmergencyBrake ( 1 )
MonitoringDeviceAppliesCutsPower ( 1 )
MonitoringDeviceAppliesShutsDownEngine ( 0 )
MonitoringDeviceResetOnZeroSpeed ( 1 )
MonitoringDeviceResetOnResetButton ( 1 )
)

Comment ( "Rizeni" )

EngineControllers (
Throttle ( 0 1 0.005 0
NumNotches ( 46
Notch ( 0 0 Dummy )       
Notch ( 0.001 0 Dummy )  
Notch ( 0.004 0 Dummy ) 
Notch ( 0.02 0 Dummy )  
Notch ( 0.04 0 Dummy ) 
Notch ( 0.07 0 Dummy )
Notch ( 0.09 0 Dummy )  
Notch ( 0.11 0 Dummy )  
Notch ( 0.13 0 Dummy )  
Notch ( 0.15 0 Dummy ) 
Notch ( 0.17 0 Dummy ) 
Notch ( 0.19 0 Dummy ) 
Notch ( 0.21 0 Dummy )  
Notch ( 0.23 0 Dummy )  
Notch ( 0.25 0 Dummy )  
Notch ( 0.27 0 Dummy )  
Notch ( 0.29 0 Dummy )  
Notch ( 0.30 0 Dummy )  
Notch ( 0.32 0 Dummy )  
Notch ( 0.34 0 Dummy )  
Notch ( 0.36 0 Dummy )  
Notch ( 0.37 0 Dummy )  
Notch ( 0.38 0 Dummy )  
Notch ( 0.39 0 Dummy )  
Notch ( 0.40 0 Dummy )  
Notch ( 0.41 0 Dummy )  
Notch ( 0.43 0 Dummy )  
Notch ( 0.47 0 Dummy ) 
Notch ( 0.50 0 Dummy ) 
Notch ( 0.53 0 Dummy )  
Notch ( 0.57 0 Dummy )  
Notch ( 0.59 0 Dummy ) 
Notch ( 0.60 0 Dummy )  
Notch ( 0.62 0 Dummy )  
Notch ( 0.63 0 Dummy )  
Notch ( 0.65 0 Dummy )  
Notch ( 0.66 0 Dummy )  
Notch ( 0.69 0 Dummy )  
Notch ( 0.71 0 Dummy )  
Notch ( 0.72 0 Dummy )  
Notch ( 0.76 0 Dummy )  
Notch ( 0.82 0 Dummy )  
Notch ( 0.86 0 Dummy )  
Notch ( 0.92 0 Dummy )  
Notch ( 0.96 0 Dummy ) 
Notch ( 1.00 0 Dummy )  
)
)

Comment ( "Primocinna brzda typ DAKO-BP" )
Brake_Engine ( 0 1 0.125 0.0
NumNotches ( 1
Notch (  0 1 Dummy ) 
)
)

Comment ( "Prubezna brzda typ DAKO-BS2" )
Brake_Train ( 0 1 0.04 0.21
NumNotches ( 7
Notch ( 0 0 TrainBrakesControllerOverchargeStart )
Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
Notch ( 0.85 0 TrainBrakesControllerNeutralhandleOffStart )
Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
)
)

Brake_Hand ( 0 1 0.025 0
NumNotches ( 0 )
)

DirControl ( -1 0 1 1 )
Sanding ( 0 1 0 )
Horn ( 0 1 0 )
Wipers ( 0 1 0 )
PantographToggle1 ( 0 1 0 )
EmergencyStopToggle ( 0 1 1 )
Vigilance ( 0 1 0 )
Headlights ( 0 0.25 1 0 )
)

Comment ( "Ostatni informace" )
Sound ( 130cab.sms )
CabView ( 130.cvf )
HeadOut ( 1.7 3.2 6.5 )

Comment ( "Poznamky" )
Description (
"Pokyny pro obecne nastaveni OR:\n"+
"-> Karta Obecne: Rychlost plneni brzdoveho potrubi 1000 PSI/s (nutne aby OR akceptoval hodnoty engu!)\n"+
"-> Karta Simulace: Pokrocily model adheze\n"+
"-> Karta Experimentalni: Faktor korekce adheze 100%\n"+
"-> Karta Experimentalni: Nahodna zmena faktoru adheze 10%\n\n"+ 
"Rada E479.0 CSD je univerzalni elektricka skrinova lokomotiva, pouzivana v nakladni i osobni doprave.\n"+
"Vyrobeno ve SKODA Plzen v roce 1977 jako typ 79E1 v poctu 54 kusu\n"+
"Typ Bo'-Bo', napeti 3 kV ss.\n"+
"Delka pres narazniky: 17,21 m\n"+
"Prumer hnacich kol: 1250 mm\n"+
"Hmotnost ve sluzbe: 85 t\n"+
"Trvaly vykon trakcnich motoru: 2040 kW\n"+
"Max. tazna sila: 228 kN\n"+
"Trvala tazna sila: 147 kN\n"+
"Max. rychlost 100 km/h\n"+
"43% vykonu reprezentuje seriovy hospodarsky stupen\n"+
"76% vykonu reprezentuje seriovo-paralelni hospodarsky stupen\n"+
"82-100% vykonu reprezentuje 5 shuntovacich stupnu."
)

EngineOperatingProcedures (
"Viz. manual Open Rails"+
"TIP: V prubehu jizdy pomoc na klavese F1-Postupy.\n\n"+
"Rozjezd: Zapnutí baterie (INSERT)\n"+
"Rozjezd: Zapnutí rizení (ENTER)\n"+
"Rozjezd: Zapnutí Hlavniho vypinace (O)\n"+
"Rozjezd: Pantograf nahoru (P)\n"+
"Zapnuti topeni vlaku (ALT+B)\n"+
"Stupne kontroleru (informativne):\n"+
"1.-24.	Rozjezdove stupne seriove (0-41%)\n"+
"25. Hospodarny seriovy stupen (odporniky vyrazeny)(43%)\n"+
"28.-38. Rozjezdove serioparalelni stupne (vzdy dva motory v serii)(53-72%)\n"+
"39. Hospodarny serioparalelni stupen (odporniky vyrazeny)(76%)\n"+
"I.-V. Shuntovaci stupne pro serioparalelni zapojeni motoru.(82-100%)\n"+
"Odporniky jsou fechralove, pri jizde\n"+
"lze na nich setrvat libovolnou dobu."
)
)
